Internet X.509 Public Key Infrastructure -- Certificate Management Protocol (CMP)
RFC 9810
Hendrik Brockhaus
Siemens
Werner-von-Siemens-Strasse 1
Munich
80333
Germany
hendrik.brockhaus@siemens.com
https://www.siemens.com
David von Oheimb
Siemens
Werner-von-Siemens-Strasse 1
Munich
80333
Germany
david.von.oheimb@siemens.com
https://www.siemens.com
Mike Ounsworth
Entrust
1187 Park Place
Minneapolis
MN
55379
United States of America
mike.ounsworth@entrust.com
https://www.entrust.com
John Gray
Entrust
1187 Park Place
Minneapolis
MN
55379
United States of America
john.gray@entrust.com
https://www.entrust.com
July 2025
SEC
lamps
CMP
Certificate Management
PKI
This document describes the Internet X.509 Public Key Infrastructure (PKI) Certificate Management Protocol (CMP). Protocol messages are defined for X.509v3 certificate creation and management. CMP provides interactions between client systems and PKI components such as a Registration Authority (RA) and a Certification Authority (CA).
This document adds support for management of certificates containing a Key Encapsulation Mechanism (KEM) public key and uses EnvelopedData instead of EncryptedValue. This document also includes the updates specified in Section 2 and Appendix A.2 of RFC 9480.
This document obsoletes RFC 4210, and together with RFC 9811, it also obsoletes RFC 9480. Appendix F of this document updates Section 9 of RFC 5912.
Introduction
This document describes the Internet X.509 PKI CMP. Protocol messages are defined for certificate creation and management. The term "certificate" in this document refers to an X.509v3 certificate as defined in [RFC5280].
Changes Made by RFC 4210
[RFC4210] differs from [RFC2510] in the following areas:
- The PKI management message profile section is split to two appendices: the required profile and the optional profile. Some of the formerly mandatory functionality is moved to the optional profile.
- The message confirmation mechanism has changed substantially.
- A new polling mechanism is introduced, deprecating the old polling method at the CMP transport level.
- The CMP transport protocol issues are handled in a separate document [RFC6712], thus the "Transports" section is removed.
- A new implicit confirmation method is introduced to reduce the number of protocol messages exchanged in a transaction.
- The new specification contains some less prominent protocol enhancements and improved explanatory text on several issues.
Updates Made by RFC 9480
CMP Updates [RFC9480] and CMP Algorithms [RFC9481] updated [RFC4210], supporting the PKI management operations specified in the Lightweight CMP Profile [RFC9483], in the following areas:
- Added new extended key usages (EKUs) for various CMP server types, e.g., RA and CA, to express the authorization of the certificate holder that acts as the indicated type of PKI management entity.
- Extended the description of multiple protection to cover additional use cases, e.g., batch processing of messages.
- Used the Cryptographic Message Syntax (CMS) [RFC5652] type EnvelopedData as the preferred choice instead of EncryptedValue to better support crypto agility in CMP.
For reasons of completeness and consistency, the type EncryptedValue has been exchanged in all occurrences. This includes the protection of centrally generated private keys, encryption of certificates, Proof-of-Possession (POP) methods, and protection of revocation passphrases. To properly differentiate the support of EnvelopedData instead of EncryptedValue, CMP version 3 is introduced in case a transaction is supposed to use EnvelopedData.
Note: According to point 9 in Section 2.1 of [RFC4211], the use of the EncryptedValue structure has been deprecated in favor of the EnvelopedData structure. [RFC4211] offers the EncryptedKey structure a choice of EncryptedValue and EnvelopedData for migration to EnvelopedData.
- Offered an optional hashAlg field in CertStatus supporting cases when a certificate needs to be confirmed, but the certificate was signed using a signature algorithm that does not indicate a specific hash algorithm to use for computing the certHash. This is also in preparation for upcoming post-quantum algorithms.
- Added new general message types to request CA certificates, a root CA update, a certificate request template, or Certificate Revocation List (CRL) updates.
- Extended the use of polling to p10cr, certConf, rr, genm, and error messages.
- Deleted the mandatory algorithm profile in Appendix C.2 and instead referred to Section 7 of [RFC9481].
- Added Sections 8.6, 8.7, 8.9, and 8.10 to the security considerations.
Changes Made by This Document
This document obsoletes [RFC4210] and [RFC9480].
Backward compatibility with CMP version 2 is maintained wherever possible. Updates to CMP version 2 improve crypto agility, extend the polling mechanism, add new general message types, and add EKUs to identify special CMP server authorizations. CMP version 3 is introduced for changes to the ASN.1 syntax, which support EnvelopedData, certConf with hashAlg, POPOPrivKey with agreeMAC, and RootCaKeyUpdateContent in ckuann messages.
The updates made in this document include the changes specified by Section 2 and Appendix A.2 of [RFC9480] as described in Section 1.2. Additionally, this document updates the content of [RFC4210] in the following areas:
- Added Section 3.1.1.4 introducing the Key Generation Authority (KGA).
- Extended Section 3.1.2 regarding use of Certificate Transparency (CT) logs.
- Updated Section 4.4 introducing RootCaKeyUpdateContent as an alternative to using a repository to acquire new root CA certificates.
- Added Section 5.1.1.3 containing a description of origPKIMessage content, moved here from Section 5.1.3.4.
- Added support for KEM keys for POP to Sections 4.3 and 5.2.8, for message protection to Sections 5.1.1 and 5.1.3.4 and Appendix E, and for usage with CMS EnvelopedData to Section 5.2.2.
- Deprecated CAKeyUpdAnnContent in favor of RootCaKeyUpdateContent.
- Incorporated the request message behavioral clarifications from Appendix C of [RFC4210] to Section 5. The definition of altCertTemplate was incorporated into Section 5.2.1, and the clarification on POPOSigningKey and on POPOPrivKey was incorporated into Section 5.2.8.
- Added support for CMS EnvelopedData to different POP methods for transferring encrypted private keys, certificates, and challenges to Section 5.2.8.
- Added Sections 8.1, 8.5, 8.8, and 8.11 to the security considerations.
Terminology and Abbreviations
The key words "MUST", "MUST NOT", "REQUIRED", "SHALL", "SHALL NOT", "SHOULD", "SHOULD NOT", "RECOMMENDED", "NOT RECOMMENDED", "MAY", and "OPTIONAL" in this document are to be interpreted as described in BCP 14 [RFC2119] [RFC8174] when, and only when, they appear in all capitals, as shown here.
This document relies on the terminology defined in [RFC5280]. The most important abbreviations are listed below:
CA:
Certification Authority
CMP:
Certificate Management Protocol
CMS:
Cryptographic Message Syntax
CRL:
Certificate Revocation List
CRMF:
Certificate Request Message Format
KEM:
Key Encapsulation Mechanism
KGA:
Key Generation Authority
LRA:
Local Registration Authority
MAC:
Message Authentication Code
PKI:
Public Key Infrastructure
POP:
Proof-of-Possession
RA:
Registration Authority
TEE:
Trusted Execution Environment
PKI Management Overview
The PKI must be structured to be consistent with the types of individuals who must administer it. Providing such administrators with unbounded choices not only complicates the software required but also increases the chances that a subtle mistake by an administrator or software developer will result in broader compromise. Similarly, restricting administrators with cumbersome mechanisms will cause them not to use the PKI.
Management protocols are REQUIRED to support online interactions between PKI components. For example, a management protocol might be used between a CA and a client system with which a key pair is associated or between two CAs that issue cross-certificates for each other.
PKI Management Model
Before specifying particular message formats and procedures, we first define the entities involved in PKI management and their interactions (in terms of the PKI management functions required). We then group these functions in order to accommodate different identifiable types of end entities.
Definitions of PKI Entities
The entities involved in PKI management include the end entity (i.e., the entity to whom the certificate is issued) and the CA (i.e., the entity that issues the certificate). An RA might also be involved in PKI management.
Subjects and End Entities
The term "subject" is used here to refer to the entity to whom the certificate is issued, typically named in the subject or subjectAltName field of a certificate. When we wish to distinguish the tools and/or software used by the subject (e.g., a local certificate management module), we will use the term "subject equipment". In general, the term "end entity", rather than "subject", is preferred in order to avoid confusion with the field name. It is important to note that the end entities here will include not only human users of applications but also applications themselves (e.g., for Internet Key Exchange Protocol (IKE) / IPsec) or devices (e.g., routers or industrial control systems). This factor influences the protocols that the PKI management operations use; for example, application software is far more likely to know exactly which certificate extensions are required than are human users. PKI management entities are also end entities in the sense that they are sometimes named in the subject or subjectAltName field of a certificate or cross-certificate. Where appropriate, the term "end entity" will be used to refer to end entities who are not PKI management entities.
All end entities require secure local access to some information -- at a minimum, their own name and private key, the name of a CA that is directly trusted by this entity, and that CA's public key (or a fingerprint of the public key where a self-certified version is available elsewhere). Implementations MAY use secure local storage for more than this minimum (e.g., the end entity's own certificates or application-specific information). The form of storage will also vary -- from files to tamper-resistant cryptographic tokens. The information stored in such local, trusted storage is referred to here as the end entity's TEE, also known as Personal Security Environment (PSE).
Though TEE formats are beyond the scope of this document (they are very dependent on equipment, et cetera), a generic interchange format for TEEs is defined here: a certification response message (see Section 5.3.4) MAY be used.
Certification Authority
The CA may or may not actually be a real "third party" from the end entity's point of view. Quite often, the CA will actually belong to the same organization as the end entities it supports.
Again, we use the term "CA" to refer to the entity named in the issuer field of a certificate. When it is necessary to distinguish the software or hardware tools used by the CA, we use the term "CA equipment".
The CA equipment will often include both an "offline" component and an "online" component, with the CA private key only available to the "offline" component. This is, however, a matter for implementers (though it is also relevant as a policy issue).
We use the term "root CA" to indicate a CA that is directly trusted by an end entity; that is, securely acquiring the value of a root CA public key requires some out-of-band step(s). This term is not meant to imply that a root CA is necessarily at the top of any hierarchy, simply that the CA in question is trusted directly. The "root CA" may provide its trust anchor information with or without using a certificate. In some circumstances, such a certificate may be self-signed, but in other circumstances, it may be cross-signed, signed by a peer, signed by a superior CA, or unsigned.
Note that other documents like [X509.2019] and [RFC5280] use the term "trusted CA" or "trust anchor" instead of "root CA". This document continues using "root CA" based on the above definition because it is also present in the ASN.1 syntax that cannot be changed easily.
A "subordinate CA" is one that is not a root CA for the end entity in question. Often, a subordinate CA will not be a root CA for any entity, but this is not mandatory.
Registration Authority
In addition to end entities and CAs, many environments call for the existence of an RA separate from the CA. The functions that the RA may carry out will vary from case to case but MAY include identity checking, token distribution, checking certificate requests and authentication of their origin, revocation reporting, name assignment, archival of key pairs, et cetera.
This document views the RA as an OPTIONAL component: When it is not present, the CA is assumed to be able to carry out the RA's functions so that the PKI management protocols are the same from the end entity's point of view.
Again, we distinguish, where necessary, between the RA and the tools used (the "RA equipment").
Note that an RA is itself an end entity. We further assume that all RAs are in fact certified end entities and that RAs have private keys that are usable for signing. How a particular CA equipment identifies some end entities as RAs is an implementation issue (i.e., this document specifies no special RA certification operation). We do not mandate that the RA is certified by the CA with which it is interacting at the moment (so one RA may work with more than one CA whilst only being certified once).
In some circumstances, end entities will communicate directly with a CA even where an RA is present. For example, for initial registration and/or certification, the end entity may use its RA but communicate directly with the CA in order to refresh its certificate.
Key Generation Authority
A KGA is a PKI management entity generating key pairs on behalf of an end entity. As the KGA generates the key pair, it knows the public and the private part.
This document views the KGA as an OPTIONAL component. When it is not present and central key generation is needed, the CA is assumed to be able to carry out the KGA's functions so that the PKI management protocol messages are the same from the end entity's point of view. If certain tasks of a CA are delegated to other components, this delegation needs authorization, which can be indicated by EKUs (see Section 4.5).
Note: When doing central generation of key pairs, implementers should consider the implications of server-side retention on the overall security of the system; in some cases, retention is good, for example, for escrow reasons, but in other cases, the server should clear its copy after delivery to the end entity.
Note: If the CA delegates key generation to a KGA, the KGA can be collocated with the RA.
PKI Management Requirements
The protocols given here meet the following requirements on PKI management
1. PKI management must conform to the ISO/IEC 9594-8/ITU-T X.509 standards, in particular [X509.2019].
2. It must be possible to regularly update any key pair without affecting any other key pair.
3. The use of confidentiality in PKI management protocols must be kept to a minimum in order to ease acceptance in environments where strong confidentiality might cause regulatory problems.
4. PKI management protocols must allow the use of different industry-standard cryptographic algorithms (see CMP Algorithms [RFC9481]). This means that any given CA, RA, or end entity may, in principle, use whichever algorithms suit it for its own key pair(s).
5. PKI management protocols must not preclude the generation of key pairs by the end entity concerned, by a KGA, or by a CA. Key generation may also occur elsewhere, but for the purposes of PKI management, we can regard key generation as occurring wherever the key is first present at an end entity, KGA, or CA.
6. PKI management protocols must support the publication of certificates by the end entity concerned, by an RA, or by a CA. Different implementations and different environments may choose any of the above approaches.
7. PKI management protocols must support the production of Certificate Revocation Lists (CRLs) by allowing certified end entities to make requests for the revocation of certificates. This must be done in such a way that the denial-of-service attacks, which are possible, are not made simpler.
8. PKI management protocols must be usable over a variety of "transport" mechanisms, specifically including email, Hypertext Transfer Protocol (HTTP), Message Queuing Telemetry Transport (MQTT), Constrained Application Protocol (CoAP), and various offline and non-networked file transfer methods.
9. Final authority for certification creation rests with the CA. No RA or end entity equipment can assume that any certificate issued by a CA will contain what was requested; a CA may alter certificate field values or may add, delete, or alter extensions according to its operating policy. In other words, all PKI entities (end entities, RAs, KGAs, and CAs) must be capable of handling responses to requests for certificates in which the actual certificate issued is different from that requested (for example, a CA may shorten the validity period requested). Note that policy may dictate that the CA must not publish or otherwise distribute the certificate until the requesting entity has reviewed and accepted the newly created certificate or the POP is completed. In case of publication of the certificate (when using indirect POP, see Section 8.11) or a precertificate in a CT log [RFC9162], the certificate must be revoked if it was not accepted by the end entity or the POP could not be completed.
10. A graceful, scheduled changeover from one non-compromised CA key pair to the next (CA key update) must be supported (note that if the CA key is compromised, re-initialization must be performed for all entities in the domain of that CA). An end entity whose TEE contains the new CA public key (following a CA key update) may also need to be able to verify certificates verifiable using the old public key. End entities who directly trust the old CA key pair may also need to be able to verify certificates signed using the new CA private key (required for situations where the old CA public key is "hardwired" into the end entity's cryptographic equipment).
11. The functions of an RA may, in some implementations or environments, be carried out by the CA itself. The protocols must be designed so that end entities will use the same protocol regardless of whether the communication is with an RA or CA. Naturally, the end entity must use the correct RA or CA public key to verify the protection of the communication.
12. Where an end entity requests a certificate containing a given public key value, the end entity must be ready to demonstrate possession of the corresponding private key value. This may be accomplished in various ways, depending on the type of certification request. See Section 4.3 for details of the in-band methods defined for the PKIX-CMP (i.e., CMP) messages.
PKI Management Operations
The following diagram shows the relationship between the entities defined above in terms of the PKI management operations. The letters in the diagram indicate "protocols" in the sense that a defined set of PKI management messages can be sent along each of the lettered lines.
PKI Entities

cert.

publish

j

End

Entity

C

g

"out-of-band"

e

loading

r

initial

t

a

b

registration/

certification
                    /

key

pair

recovery

key

pair

update

C

certificate

update

R

PKI

"USERS"

revocation

request

L

PKI

MANAGEMENT

ENTITIES

a

b

a

b

R

e

g

d

p

RA

o

cert.

s

publish

c

i

t

o

g

i

r

CA

y

h

"out-of-band"

cert.

publish

publication

CRL

publish

cross-certification

e

f

cross-certificate

update

CA-2

  +---+     cert. publish        +------------+      j
  |   |  <---------------------  | End Entity | <-------
  | C |             g            +------------+      "out-of-band"
  | e |                            | ^                loading
  | r |                            | |      initial
  | t |                          a | | b     registration/
  |   |                            | |       certification
  | / |                            | |      key pair recovery
  |   |                            | |      key pair update
  | C |                            | |      certificate update
  | R |  PKI "USERS"               V |      revocation request
  | L | -------------------+-+-----+-+------+-+-------------------
  |   |  PKI MANAGEMENT    | ^              | ^
  |   |    ENTITIES      a | | b          a | | b
  | R |                    V |              | |
  | e |             g   +------+    d       | |
  | p |   <------------ | RA   | <-----+    | |
  | o |      cert.      |      | ----+ |    | |
  | s |       publish   +------+   c | |    | |
  | i |                              | |    | |
  | t |                              V |    V |
  | o |          g                 +------------+   i
  | r |   <------------------------|     CA     |------->
  | y |          h                 +------------+  "out-of-band"
  |   |      cert. publish              | ^         publication
  |   |      CRL publish                | |
  +---+                                 | |    cross-certification
                                      e | | f  cross-certificate
                                        | |       update
                                        | |
                                        V |
                                      +------+
                                      | CA-2 |
                                      +------+

At a high level, the set of operations for which management messages are defined can be grouped as follows.
1. CA establishment: When establishing a new CA, certain steps are required (e.g., production of initial CRLs and export of CA public key).
2. End entity initialization: This includes importing a root CA public key and requesting information about the options supported by a PKI management entity.
3. Certification: Various operations result in the creation of new certificates:
  a. initial registration/certification: This is the process whereby an end entity first makes itself known to a CA or RA, prior to the CA issuing a certificate or certificates for that end entity. The end result of this process (when it is successful) is that a CA issues a certificate for an end entity's public key and returns that certificate to the end entity and/or posts that certificate in a repository. This process may, and typically will, involve multiple "steps", possibly including an initialization of the end entity's equipment. For example, the end entity's equipment must be securely initialized with the public key of a CA, e.g., using zero-touch methods like Bootstrapping Remote Secure Key Infrastructure (BRSKI) [RFC8995] or Secure Zero Touch Provisioning (SZTP) [RFC8572], to be used in validating certificate paths. Furthermore, an end entity typically needs to be initialized with its own key pair(s).
  b. key pair update: Every key pair needs to be updated regularly (i.e., replaced with a new key pair), and a new certificate needs to be issued.
  c. certificate update: As certificates expire, they may be "refreshed" if nothing relevant in the environment has changed.
  d. CA key pair update: As with end entities, CA key pairs need to be updated regularly; however, different mechanisms are required.
  e. cross-certification request: One CA requests issuance of a cross-certificate from another CA. For the purposes of this standard, the following terms are defined. A "cross-certificate" is a certificate in which the subject CA and the issuer CA are distinct and SubjectPublicKeyInfo contains a verification key (i.e., the certificate has been issued for the subject CA's signing key pair). When it is necessary to distinguish more finely, the following terms may be used: A cross-certificate is called an "inter-domain cross-certificate" if the subject and issuer CAs belong to different administrative domains; it is called an "intra-domain cross-certificate" otherwise.
    1. The above definition of "cross-certificate" aligns with the defined term "CA-certificate" in X.509. Note that this term is not to be confused with the X.500 "cACertificate" attribute type, which is unrelated.
    2. In many environments, the term "cross-certificate", unless further qualified, will be understood to be synonymous with "inter-domain cross-certificate" as defined above.
    3. Issuance of cross-certificates may be, but is not necessarily, mutual; that is, two CAs may issue cross-certificates for each other.
  f. cross-certificate update: Similar to a normal certificate update but involving a cross-certificate.
4. Certificate/CRL discovery operations: Some PKI management operations result in the publication of certificates or CRLs:
  a. certificate publication: Having gone to the trouble of producing a certificate, some means for publishing may be needed. The "means" defined in PKIX MAY involve the messages specified in Sections 5.3.13 to 5.3.16 or MAY involve other methods (for example, Lightweight Directory Access Protocol (LDAP)) as described in [RFC4511] or [RFC2585] (the "Operational Protocols" documents of the PKIX series of specifications).
  b. CRL publication: As for certificate publication.
5. Recovery operations: Some PKI management operations are used when an end entity has "lost" its TEE:
  a. key pair recovery: As an option, user client key materials (e.g., a user's private key used for decryption purposes) MAY be backed up by a CA, an RA, or a key backup system associated with a CA or RA. If an entity needs to recover these backed up key materials (e.g., as a result of a forgotten password or a lost key chain file), a protocol exchange may be needed to support such recovery.
6. Revocation operations: Some PKI management operations result in the creation of new CRL entries and/or new CRLs:
  a. revocation request: An authorized person advises a CA of an abnormal situation requiring certificate revocation.
7. TEE operations: Whilst the definition of TEE operations (e.g., moving a TEE, changing a PIN, etc.) are beyond the scope of this specification, we do define a PKIMessage (CertRepMessage) that can form the basis of such operations.
Note that online protocols are not the only way of implementing the above operations. For all operations, there are offline methods of achieving the same result, and this specification does not mandate use of online protocols. For example, when hardware tokens are used, many of the operations MAY be achieved as part of the physical token delivery.
Later sections define a set of standard messages supporting the above operations. Transfer protocols for conveying these exchanges in various environments (e.g., offline: file-based; online: email, HTTP [RFC9811], MQTT, and CoAP [RFC9482]) are beyond the scope of this document and must be specified separately. Appropriate transfer protocols MUST be capable of delivering the CMP messages reliably.
CMP provides inbuilt integrity protection and authentication. The information communicated unencrypted in CMP messages does not contain sensitive information endangering the security of the PKI when intercepted. However, it might be possible for an eavesdropper to utilize the available information to gather confidential technical or business-critical information. Therefore, users should consider protection of confidentiality on lower levels of the protocol stack, e.g., by using TLS [RFC8446], DTLS [RFC9147], or IPsec [RFC7296][RFC4303].
Assumptions and Restrictions
End Entity Initialization
The first step for an end entity in dealing with PKI management entities is to request information about the PKI functions supported and to securely acquire a copy of the relevant root CA public key(s).
Initial Registration/Certification
There are many schemes that can be used to achieve initial registration and certification of end entities. No one method is suitable for all situations due to the range of policies that a CA may implement and the variation in the types of end entity that can occur.
However, we can classify the initial registration/certification schemes that are supported by this specification. Note that the word "initial", above, is crucial: We are dealing with the situation where the end entity in question has had no previous contact with the PKI, except having received the root CA certificate of that PKI by some zero-touch method like BRSKI [RFC8995] [RFC9733] or SZTP [RFC8572]. In case the end entity already possesses certified keys, then some simplifications/alternatives are possible.
Having classified the schemes that are supported by this specification, we can then specify some as mandatory and some as optional. The goal is that the mandatory schemes cover a sufficient number of the cases that will arise in real use, whilst the optional schemes are available for special cases that arise less frequently. In this way, we achieve a balance between flexibility and ease of implementation.
Further classification of mandatory and optional schemes addressing different environments is available, e.g., in Appendices C and D of this specification on managing human user certificates as well as in the Lightweight CMP Profile [RFC9483] on fully automating certificate management in a machine-to-machine and Internet of Things (IoT) environment. Industry standards such as [ETSI-3GPP.33.310] for mobile networks and [UNISIG.Subset-137] for railroad automation have adopted CMP and defined a series of mandatory schemes for their use cases.
We will now describe the classification of initial registration/certification schemes.
Criteria Used
Initiation of Registration/Certification
In terms of the PKI messages that are produced, we can regard the initiation of the initial registration/certification exchanges as occurring wherever the first PKI message relating to the end entity is produced. Note that the real-world initiation of the registration/certification procedure may occur elsewhere (e.g., a personnel department may telephone an RA operator or use zero-touch methods like BRSKI [RFC8995] or SZTP [RFC8572]).
The possible locations are at the end entity, an RA, or a CA.
End Entity Message Origin Authentication
The online messages produced by the end entity that requires a certificate may be authenticated or not. The requirement here is to authenticate the origin of any messages from the end entity to the PKI (CA/RA).
In this specification, such authentication is achieved by two different means:
- symmetric: The PKI (CA/RA) issuing the end entity with a secret value (initial authentication key) and reference value (used to identify the secret value) via some out-of-band means. The initial authentication key can then be used to protect relevant PKI messages.
- asymmetric: Using a private key and certificate issued by another PKI trusted for initial authentication, e.g., an Initial Device Identifier (IDevID) IEEE 802.1AR. The trust establishment in this external PKI is out of scope of this document.
Thus, we can classify the initial registration/certification scheme according to whether or not the online 'end entity -> PKI management entity' messages are authenticated or not.
1. We do not discuss the authentication of the 'PKI management entity -> end entity' messages here, as this is always REQUIRED. In any case, it can be achieved simply once the root-CA public key has been installed at the end entity's equipment or it can be based on the initial authentication key.
2. An initial registration/certification procedure can be secure where the messages from the end entity are authenticated via some out-of-band means (e.g., a subsequent visit).
Location of Key Generation
In this specification, "key generation" is regarded as occurring wherever either the public or private component of a key pair first occurs in a PKIMessage. Note that this does not preclude a centralized key generation service by a KGA; the actual key pair MAY have been generated elsewhere and transported to the end entity, RA, or CA using a (proprietary or standardized) key generation request/response protocol (outside the scope of this specification).
Thus, there are three possibilities for the location of "key generation": the end entity, a KGA, or a CA.
Confirmation of Successful Certification
Following the creation of a certificate for an end entity, additional assurance can be gained by having the end entity explicitly confirm successful receipt of the message containing (or indicating the creation of) the certificate. Naturally, this confirmation message must be protected (based on the initial symmetric or asymmetric authentication key or other means).
This gives two further possibilities: confirmed or not.
Initial Registration/Certification Schemes
The criteria above allow for a large number of initial registration/certification schemes. Examples of possible initial registration/certification schemes can be found in the following subsections. An entity may support other schemes specified in profiles of PKIX-CMP, such as Appendices C and D or [RFC9483].
Centralized Scheme
In terms of the classification above, this scheme is, in some ways, the simplest possible, where:
- initiation occurs at the certifying CA;
- no online message authentication is required;
- "key generation" occurs at the certifying CA (see Section 4.2.1.3); and
- no confirmation message is required.
In terms of message flow, this scheme means that the only message required is sent from the CA to the end entity. The message must contain the entire TEE for the end entity. Some out-of-band means must be provided to allow the end entity to authenticate the message received and to decrypt any encrypted values.
Basic Authenticated Scheme
In terms of the classification above, this scheme is where:
- initiation occurs at the end entity;
- message authentication is required;
- "key generation" occurs at the end entity (see Section 4.2.1.3); and
- a confirmation message is recommended.
Note: An Initial Authentication Key (IAK) can be either a symmetric key or an asymmetric private key with a certificate issued by another PKI trusted for this purpose. The establishment of such trust is out of scope of this document.
In terms of message flow, the basic authenticated scheme is as follows:

In

terms

of

message

flow,

the

basic

authenticated

scheme

is

as

follows:

End

Entity

RA/CA

out-of-band

distribution

of

Initial

Authentication

Key

(IAK)

and

reference

value

(RA/CA
                    ->

end

entity)

Key

generation

Creation

of

certification

request

Protect

request

with

IAK

certification

request

verify

request

process

request

create

response

certification

response

handle

response

create

confirmation

cert

conf

message

verify

confirmation

create

response

conf

ack

(optional)

handle

response

  End Entity                                              RA/CA
  ==========                                      =============
       out-of-band distribution of Initial Authentication
       Key (IAK) and reference value (RA/CA -> end entity)
  Key generation
  Creation of certification request
  Protect request with IAK
                -----> certification request ----->
                                                 verify request
                                                 process request
                                                 create response
                <----- certification response <-----
  handle response
  create confirmation
                -----> cert conf message      ----->
                                                 verify confirmation
                                                 create response
                <----- conf ack (optional)    <-----
  handle response

Note: Where verification of the cert confirmation message fails, the RA/CA MUST revoke the newly issued certificate if it has been published or otherwise made available.
POP of Private Key
POP is where a PKI management entity (CA/RA) verifies if an end entity has access to the private key corresponding to a given public key. The question of whether, and in what circumstances, POPs add value to a PKI is a debate as old as PKI itself! See Section 8.1 for a further discussion on the necessity of POP in PKI.
The PKI management operations specified here make it possible for an end entity to prove to a CA/RA that it has possession of (i.e., is able to use) the private key corresponding to the public key for which a certificate is requested (see Section 5.2.8 for different POP methods). A given CA/RA is free to choose how to enforce POP (e.g., out-of-band procedural means versus PKIX-CMP in-band messages) in its certification exchanges (i.e., this may be a policy issue). However, it is REQUIRED that CAs/RAs MUST enforce POP by some means because there are currently many non-PKIX operational protocols in use (various electronic mail protocols are one example) that do not explicitly check the binding between the end entity and the private key. Until operational protocols that do verify the binding (for signature, encryption, key agreement, and KEM key pairs) exist, and are ubiquitous, this binding can only be assumed to have been verified by the CA/RA. Therefore, if the binding is not verified by the CA/RA, certificates in the Internet PKI end up being somewhat less meaningful.
POP is accomplished in different ways depending upon the type of key for which a certificate is requested. If a key can be used for multiple purposes (e.g., an RSA key), then any appropriate method MAY be used (e.g., a key that may be used for signing, as well as other purposes, MUST NOT be sent to the CA/RA in order to prove possession unless archival of the private key is explicitly desired).
This specification explicitly allows for cases where an end entity supplies the relevant proof to an RA and the RA subsequently attests to the CA that the required proof has been received (and validated!). For example, an end entity wishing to have a signing key certified could send the appropriate signature to the RA, which then simply notifies the relevant CA that the end entity has supplied the required proof. Of course, such a situation may be disallowed by some policies (e.g., CAs may be the only entities permitted to verify POP during certification).
Signature Keys
For signature keys, the end entity can sign a value to prove possession of the private key; see Section 5.2.8.2.
Encryption Keys
For encryption keys, the end entity can provide the private key to the CA/RA (e.g., for archiving), see Section 5.2.8.3.1, or can be required to decrypt a value in order to prove possession of the private key. Decrypting a value can be achieved either directly (see Section 5.2.8.3.3) or indirectly (see Section 5.2.8.3.2).
The direct method is for the RA/CA to issue a random challenge to which an immediate response by the end entity is required.
The indirect method is to issue a certificate that is encrypted for the end entity (and have the end entity demonstrate its ability to decrypt this certificate in the confirmation message). This allows a CA to issue a certificate in a form that can only be used by the intended end entity.
This specification encourages use of the indirect method because it requires no extra messages to be sent (i.e., the proof can be demonstrated using the {request, response, confirmation} triple of messages).
Key Agreement Keys
For key agreement keys, the end entity and the PKI management entity (i.e., CA or RA) must establish a shared secret key in order to prove that the end entity has possession of the private key.
Note that this need not impose any restrictions on the keys that can be certified by a given CA. In particular, for Diffie-Hellman (DH) keys, the end entity may freely choose its algorithm parameters provided that the CA can generate a short-term (or one-time) key pair with the appropriate parameters when necessary.
KEM Keys
For KEM keys, the end entity can provide the private key to the CA/RA (e.g., for archiving), see Section 5.2.8.3.1, or can be required to decrypt a value in order to prove possession of the private key. Decrypting a value can be achieved either directly (see Section 5.2.8.3.3) or indirectly (see Section 5.2.8.3.2).
Note: A definition of KEMs can be found in Section 1 of [RFC9629].
The direct method is for the RA/CA to issue a random challenge to which an immediate response by the end entity is required.
The indirect method is to issue a certificate that is encrypted for the end entity using a shared secret key derived from a key encapsulated using the public key (and have the end entity demonstrate its ability to use its private key for decapsulation of the KEM ciphertext, derive the shared secret key, decrypt this certificate, and provide a hash of the certificate in the confirmation message). This allows a CA to issue a certificate in a form that can only be used by the intended end entity.
This specification encourages use of the indirect method because it requires no extra messages to be sent (i.e., the proof can be demonstrated using the {request, response, confirmation} triple of messages).
A certification request message for a KEM certificate SHALL use POPOPrivKey by using the keyEncipherment choice of ProofOfPossession (see Section 5.2.8) in the popo field of CertReqMsg as long as no KEM-specific choice is available.
Root CA Key Update
This discussion only applies to CAs that are directly trusted by some end entities. Recognizing whether a self-signed or non-self-signed CA is supposed to be directly trusted for some end entities is a matter of CA policy and end entity configuration. Thus, this is beyond the scope of this document.
The basis of the procedure described here is that the CA protects its new public key using its previous private key and vice versa. Thus, when a CA updates its key pair, it may generate two link certificates: "old with new" and "new with old".
Note: The usage of link certificates has been shown to be very specific for each use case, and no assumptions are done on this aspect. RootCaKeyUpdateContent is updated to specify these link certificates as optional.
Note: When an LDAP directory is used to publish root CA updates, the old and new root CA certificates together with the two link certificates are stored as cACertificate attribute values.
When a CA changes its key pair, those entities who have acquired the old CA public key via "out-of-band" means are most affected. These end entities need to acquire the new CA public key in a trusted way. This may be achieved "out-of-band" by using a repository or by using online messages also containing the link certificates "new with old". Once the end entity acquired and properly verified the new CA public key, it must load the new trust anchor information into its trusted store.
The data structure used to protect the new and old CA public keys is typically a standard X.509v3 certificate (which may also contain extensions). There are no new data structures required.
Note: Sometimes self-signed root CA certificates do not make use of X.509v3 extensions and may be X.509v1 certificates. Therefore, a root CA key update must be able to work for version 1 certificates. The use of the X.509v3 KeyIdentifier extension is recommended for easier path building.
Note: While the scheme could be generalized to cover cases where the CA updates its key pair more than once during the validity period of one of its end entities' certificates, this generalization seems of dubious value. Not having this generalization simply means that the validity periods of certificates issued with the old CA key pair cannot exceed the end of the "old with new" certificate validity period.
Note: This scheme offers a mechanism to ensures that end entities will acquire the new CA public key, at the latest by the expiry of the last certificate they owned that was signed with the old CA private key. Certificate and/or key update operations occurring at other times do not necessarily require this (depending on the end entity's equipment).
Note: In practice, a new root CA may have a slightly different subject Distinguished Name (DN), e.g., indicating a generation identifier like the year of issuance or a version number, for instance, in an Organizational Unit (OU) element. How to bridge trust to the new root CA certificate in a CA DN change or a cross-certificate scenario is out of scope for this document.
CA Operator Actions
To change the key of the CA, the CA operator does the following:
1. Generate a new key pair.
2. Create a certificate containing the new CA public key signed with the new private key or by the private key of some other CA (the "new with new" certificate).
3. Optionally: Create a link certificate containing the new CA public key signed with the old private key (the "new with old" certificate).
4. Optionally: Create a link certificate containing the old CA public key signed with the new private key (the "old with new" certificate).
5. Publish these new certificates so that end entities may acquire it, e.g., using a repository or RootCaKeyUpdateContent.
The old CA private key is then no longer required when the validity of the "old with old" certificate ended. However, the old CA public key will remain in use for validating the "new with old" link certificate until the new CA public key is loaded into the trusted store. The old CA public key is no longer required (other than for non-repudiation) when all end entities of this CA have securely acquired and stored the new CA public key.
The "new with new" certificate must have a validity period with a notBefore time that is before the notAfter time of the "old with old" certificate and a notAfter time that is after the notBefore time of the next update of this certificate.
The "new with old" certificate must have a validity period with the same notBefore time as the "new with new" certificate and a notAfter time by which all end entities of this CA will securely possess the new CA public key (at the latest, at the notAfter time of the "old with old" certificate).
The "old with new" certificate must have a validity period with the same notBefore and notAfter time as the "old with old" certificate.
Note: Further operational considerations on transition from one root CA self-signed certificate to the next is available in Section 5 of [RFC8649].
Verifying Certificates
Normally when verifying a signature, the verifier verifies (among other things) the certificate containing the public key of the signer. However, once a CA is allowed to update its key, there are a range of new possibilities. These are shown in the table below.
| Verifier's TEE contains NEW public key | Verifier's TEE contains OLD public key
Signer's certificate is protected using NEW key pair | Case 1: The verifier can directly verify the certificate. | Case 2: The verifier is missing the NEW public key.
Signer's certificate is protected using OLD key pair | Case 3: The verifier is missing the OLD public key. | Case 4: The verifier can directly verify the certificate.
Verification in Cases 1 and 4
In these cases, the verifier has a local copy of the CA public key that can be used to verify the certificate directly. This is the same as the situation where no key change has occurred.
Verification in Case 2
In case 2, the verifier must get access to the new public key of the CA. Case 2 will arise when the CA operator has issued the verifier's certificate, then changed the CA's key, and then issued the signer's certificate; so it is quite a typical case.
The verifier does the following:
1. Get the "new with new" and "new with old" certificates. The location of where to retrieve these certificates may be available in the authority information access extension of the "old with old" certificate (see the access method for caIssuers in Section 4.2.2.1 of [RFC5280]), or it may be locally configured.
  a. If a repository is available, look up the certificates in the caCertificate attribute.
  b. If an HTTP or FTP server is available, pick the certificates from the "certs-only" CMS message.
  c. If a CMP server is available, request the certificates using the root CA update the general message (see Section 5.3.19.15).
  d. Otherwise, get the certificates "out-of-band" using any trustworthy mechanism.
2. If the certificates are received, check that the validity periods and the subject and issuer fields match. Verify the signatures using the old root CA key (which the verifier has locally).
3. If all checks are successful, securely store the new trust anchor information and validate the signer's certificate.
Verification in Case 3
In case 3, the verifier must get access to the old public key of the CA. Case 3 will arise when the CA operator has issued the signer's certificate, then changed the key, and then issued the verifier's certificate.
The verifier does the following:
1. Get the "old with new" certificate. The location of where to retrieve these certificates may be available in the authority information access extension of the "new with new" certificate (see caIssuers access method in Section 4.2.2.1 of [RFC5280]), or it may be locally configured.
  a. If a repository is available, look up the certificate in the caCertificate attribute.
  b. If an HTTP or FTP server is available, pick the certificate from the "certs-only" CMS message.
  c. If a CMP server and an untrusted copy of the old root CA certificate are available (e.g., the signer provided it in-band in the CMP extraCerts filed), request the certificate using the root CA update the general message (see Section 5.3.19.15).
  d. Otherwise, get the certificate "out-of-band" using any trustworthy mechanism.
2. If the certificate is received, check that the validity periods and the subject and issuer fields match. Verify the signatures using the new root CA key (which the verifier has locally).
3. If all checks were successful, securely store the old trust anchor information and validate the signer's certificate.
Revocation - Change of the CA Key
As we saw above, the verification of a certificate becomes more complex once the CA is allowed to change its key. This is also true for revocation checks, as the CA may have signed the CRL using a newer private key than the one within the user's TEE.
The analysis of the alternatives is the same as for certificate verification.
EKU for PKI Entities
The EKU extension indicates the purposes for which the certified key pair may be used. Therefore, it restricts the use of a certificate to specific applications.
A CA may want to delegate parts of its duties to other PKI management entities. This section provides a mechanism to both prove this delegation and enable automated means for checking the authorization of this delegation. Such delegation may also be expressed by other means, e.g., explicit configuration.
To offer automatic validation for the delegation of a role by a CA to another entity, the certificates used for CMP message protection or signed data for central key generation MUST be issued by the delegating CA and MUST contain the respective EKUs. This proves that the delegating CA authorized this entity to act in the given role, as described below.
The OIDs to be used for these EKUs are:

  id-kp-cmcCA OBJECT IDENTIFIER ::= {
     iso(1) identified-organization(3) dod(6) internet(1)
     security(5) mechanisms(5) pkix(7) kp(3) 27 }

  id-kp-cmcRA OBJECT IDENTIFIER ::= {
     iso(1) identified-organization(3) dod(6) internet(1)
     security(5) mechanisms(5) pkix(7) kp(3) 28 }

  id-kp-cmKGA OBJECT IDENTIFIER ::= {
     iso(1) identified-organization(3) dod(6) internet(1)
     security(5) mechanisms(5) pkix(7) kp(3) 32 }

Note: Section 2.10 of [RFC6402] specifies OIDs for a Certificate Management over CMS (CMC) CA and a CMC RA. As the functionality of a CA and RA is not specific to any protocol used for managing certificates (such as CMC or CMP), these EKUs are reused by CMP.
The meaning of the id-kp-cmKGA EKU is as follows:
CMP KGA:
CMP KGAs are CAs or are identified by the id-kp-cmKGA EKU. The CMP KGA knows the private key it generated on behalf of the end entity. This is a very sensitive service and needs specific authorization, which by default is with the CA certificate itself. The CA may delegate its authorization by placing the id-kp-cmKGA EKU in the certificate used to authenticate the origin of the generated private key. The authorization may also be determined through local configuration of the end entity.
Data Structures
This section contains descriptions of the data structures required for PKI management messages. Section 6 describes constraints on their values and the sequence of events for each of the various PKI management operations.
Overall PKI Message
All of the messages used in this specification for the purposes of PKI management use the following structure:

  PKIMessage ::= SEQUENCE {
     header           PKIHeader,
     body             PKIBody,
     protection   [0] PKIProtection OPTIONAL,
     extraCerts   [1] SEQUENCE SIZE (1..MAX) OF CMPCertificate
                       OPTIONAL
  }

  PKIMessages ::= SEQUENCE SIZE (1..MAX) OF PKIMessage

The PKIHeader contains information that is common to many PKI messages.
The PKIBody contains message-specific information.
The PKIProtection, when used, contains bits that protect the PKI message.
The extraCerts field can contain certificates that may be useful to the recipient. For example, this can be used by a CA or RA to present an end entity with certificates that it needs to verify its own new certificate (for example, if the CA that issued the end entity's certificate is not a root CA for the end entity). Note that this field does not necessarily contain a certification path; the recipient may have to sort, select from, or otherwise process the extra certificates in order to use them.
PKI Message Header
All PKI messages require some header information for addressing and transaction identification. Some of this information will also be present in a transport-specific envelope. However, if the PKI message is protected, then this information is also protected (i.e., we make no assumption about secure transport).
The following data structure is used to contain this information:

  PKIHeader ::= SEQUENCE {
     pvno                INTEGER     { cmp1999(1), cmp2000(2),
                                       cmp2021(3) },
     sender              GeneralName,
     recipient           GeneralName,
     messageTime     [0] GeneralizedTime         OPTIONAL,
     protectionAlg   [1] AlgorithmIdentifier{ALGORITHM, {...}}
                         OPTIONAL,
     senderKID       [2] KeyIdentifier           OPTIONAL,
     recipKID        [3] KeyIdentifier           OPTIONAL,
     transactionID   [4] OCTET STRING            OPTIONAL,
     senderNonce     [5] OCTET STRING            OPTIONAL,
     recipNonce      [6] OCTET STRING            OPTIONAL,
     freeText        [7] PKIFreeText             OPTIONAL,
     generalInfo     [8] SEQUENCE SIZE (1..MAX) OF
                         InfoTypeAndValue     OPTIONAL
  }

  PKIFreeText ::= SEQUENCE SIZE (1..MAX) OF UTF8String

The usage of the protocol version number (pvno) is described in Section 7.
The sender field contains the name of the sender of the PKIMessage. This name (in conjunction with senderKID, if supplied) should be sufficient to indicate the key to use to verify the protection on the message. If nothing about the sender is known to the sending entity (e.g., in the initial request message, where the end entity may not know its own DN, email name, IP address, etc.), then the "sender" field MUST contain a "NULL-DN" value in the directoryName choice. A "NULL-DN" is a SEQUENCE OF relative DNs of zero length and is encoded as 0x3000. In such a case, the senderKID field MUST hold an identifier (i.e., a reference number) that indicates to the receiver the appropriate shared secret information to use to verify the message.
The recipient field contains the name of the recipient of the PKIMessage. This name (in conjunction with recipKID, if supplied) should be usable to verify the protection on the message.
The protectionAlg field specifies the algorithm used to protect the message. If no protection bits are supplied (note that PKIProtection is OPTIONAL), then this field MUST be omitted; if protection bits are supplied, then this field MUST be supplied.
senderKID and recipKID are usable to indicate which keys have been used to protect the message (recipKID will normally only be required where protection of the message uses DH or Elliptic Curve Diffie-Hellman (ECDH) keys). These fields MUST be used if required to uniquely identify a key (e.g., if more than one key is associated with a given sender name). The senderKID SHOULD be used in any case.
Note: The recommendation of using senderKID has changed since [RFC4210], where it was recommended to be omitted if not needed to identify the protection key.
The transactionID field within the message header is to be used to allow the recipient of a message to correlate this with an ongoing transaction. This is needed for all transactions that consist of more than just a single request/response pair. For transactions that consist of a single request/response pair, the rules are as follows. A client MUST populate the transactionID field if the message contains an infoValue of type KemCiphertextInfo (see Section 5.1.3.4). In all other cases, the client MAY populate the transactionID field of the request. If a server receives such a request that has the transactionID field set, then it MUST set the transactionID field of the response to the same value. If a server receives such request with a missing transactionID field, then it MUST populate the transactionID field if the message contains a KemCiphertextInfo field. In all other cases, the server MAY set the transactionID field of the response.
For transactions that consist of more than just a single request/response pair, the rules are as follows. If the message contains an infoValue of type KemCiphertextInfo, the client MUST generate a transactionID; otherwise, the client SHOULD generate a transactionID for the first request. If a server receives such a request that has the transactionID field set, then it MUST set the transactionID field of the response to the same value. If a server receives such request with a missing transactionID field, then it MUST populate the transactionID field of the response with a server-generated ID. Subsequent requests and responses MUST all set the transactionID field to the thus established value. In all cases where a transactionID is being used, a given client MUST NOT have more than one transaction with the same transactionID in progress at any time (to a given server). Servers are free to require uniqueness of the transactionID or not, as long as they are able to correctly associate messages with the corresponding transaction. Typically, this means that a server will require the {client, transactionID} tuple to be unique, or even the transactionID alone to be unique, if it cannot distinguish clients based on any transport-level information. A server receiving the first message of a transaction (which requires more than a single request/response pair) that contains a transactionID that does not allow it to meet the above constraints (typically because the transactionID is already in use) MUST send back an ErrorMsgContent with a PKIFailureInfo of transactionIdInUse. It is RECOMMENDED that the clients fill the transactionID field with 128 bits of (pseudo-)random data for the start of a transaction to reduce the probability of having the transactionID in use at the server.
The senderNonce and recipNonce fields protect the PKIMessage against replay attacks. The senderNonce will typically be 128 bits of (pseudo-)random data generated by the sender, whereas the recipNonce is copied from the senderNonce field of the previous message in the transaction.
The messageTime field contains the time at which the sender created the message. This may be useful to allow end entities to correct/check their local time for consistency with the time on a central system.
The freeText field may be used to send a human-readable message to the recipient (in any number of languages). Each UTF8String MAY include a language tag [RFC5646] to indicate the language of the contained text. The first language used in this sequence indicates the desired language for replies.
The generalInfo field may be used to send machine-processable additional data to the recipient. The following generalInfo extensions are defined and MAY be supported.
ImplicitConfirm
This is used by the end entity to inform the CA or RA that it does not wish to send a certificate confirmation for issued certificates.

  id-it-implicitConfirm OBJECT IDENTIFIER ::= {id-it 13}
  ImplicitConfirmValue ::= NULL

If the CA grants the request to the end entity, it MUST put the same extension in the PKIHeader of the response. If the end entity does not find the extension in the response, it MUST send the certificate confirmation.
ConfirmWaitTime
This is used by the CA or RA to inform the end entity how long it intends to wait for the certificate confirmation before revoking the certificate and deleting the transaction.

  id-it-confirmWaitTime OBJECT IDENTIFIER ::= {id-it 14}
  ConfirmWaitTimeValue ::= GeneralizedTime

OrigPKIMessage
An RA MAY include the original PKIMessage from the end entity in the generalInfo field of the PKIHeader of a PKIMessage. This is used by the RA to inform the CA of the original PKIMessage that it received from the end entity and modified in some way (e.g., added or modified particular field values or added new extensions) before forwarding the new PKIMessage. This accommodates, for example, cases in which the CA wishes to check the message origin, the POP, or other information on the original end entity message.
Note: If the changes made by the RA to the original PKIMessage break the POP of a certificate request, the RA can set the popo field of the new PKIMessage to raVerified (see Section 5.2.8.4).
Unless the OrigPKIMessage infoValue is in the header of a nested message, it MUST contain exactly one PKIMessage. The contents of OrigPKIMessage infoValue in the header of a nested message MAY contain multiple PKIMessage structures, which MUST be in the same order as the PKIMessage structures in PKIBody.

  id-it-origPKIMessage OBJECT IDENTIFIER ::= {id-it 15}
  OrigPKIMessageValue ::= PKIMessages

CertProfile
This is used by the end entity to indicate specific certificate profiles, e.g., when requesting a new certificate or a certificate request template (see Section 5.3.19.16).

  id-it-certProfile OBJECT IDENTIFIER ::= {id-it 21}
  CertProfileValue ::= SEQUENCE SIZE (1..MAX) OF UTF8String

When used in a p10cr message, the CertProfileValue sequence MUST NOT contain multiple certificate profile names. When used in an ir/cr/kur/genm message, the CertProfileValue sequence MUST NOT contain more certificate profile names than the number of CertReqMsg or GenMsgContent InfoTypeAndValue elements contained in the message body.
The certificate profile names in the CertProfileValue sequence relate to the CertReqMsg or GenMsgContent InfoTypeAndValue elements in the given order. An empty string means no certificate profile name is associated with the respective CertReqMsg or GenMsgContent InfoTypeAndValue element. If the CertProfileValue sequence contains less certificate profile entries than CertReqMsg or GenMsgContent InfoTypeAndValue elements, the remaining CertReqMsg or GenMsgContent InfoTypeAndValue elements have no profile name associated with them.
KemCiphertextInfo
A PKI entity MAY provide the KEM ciphertext for MAC-based message protection using KEM (see Section 5.1.3.4) in the generalInfo field of a request message to a PKI management entity if it knows that the PKI management entity uses a KEM key pair and has its public key.

  id-it-KemCiphertextInfo OBJECT IDENTIFIER ::= { id-it 24 }
  KemCiphertextInfoValue ::= KemCiphertextInfo

For more details of KEM-based message protection, see Section 5.1.3.4. See Section 5.3.19.18 for the definition of {id-it 24}.
PKI Message Body

  PKIBody ::= CHOICE {
     ir       [0]  CertReqMessages,        --Initialization Req
     ip       [1]  CertRepMessage,         --Initialization Resp
     cr       [2]  CertReqMessages,        --Certification Req
     cp       [3]  CertRepMessage,         --Certification Resp
     p10cr    [4]  CertificationRequest,   --PKCS #10 Cert.  Req.
     popdecc  [5]  POPODecKeyChallContent, --pop Challenge
     popdecr  [6]  POPODecKeyRespContent,  --pop Response
     kur      [7]  CertReqMessages,        --Key Update Request
     kup      [8]  CertRepMessage,         --Key Update Response
     krr      [9]  CertReqMessages,        --Key Recovery Req
     krp      [10] KeyRecRepContent,       --Key Recovery Resp
     rr       [11] RevReqContent,          --Revocation Request
     rp       [12] RevRepContent,          --Revocation Response
     ccr      [13] CertReqMessages,        --Cross-Cert.  Request
     ccp      [14] CertRepMessage,         --Cross-Cert.  Resp
     ckuann   [15] CAKeyUpdContent,        --CA Key Update Ann.
     cann     [16] CertAnnContent,         --Certificate Ann.
     rann     [17] RevAnnContent,          --Revocation Ann.
     crlann   [18] CRLAnnContent,          --CRL Announcement
     pkiconf  [19] PKIConfirmContent,      --Confirmation
     nested   [20] NestedMessageContent,   --Nested Message
     genm     [21] GenMsgContent,          --General Message
     genp     [22] GenRepContent,          --General Response
     error    [23] ErrorMsgContent,        --Error Message
     certConf [24] CertConfirmContent,     --Certificate Confirm
     pollReq  [25] PollReqContent,         --Polling Request
     pollRep  [26] PollRepContent          --Polling Response
  }

The specific types are described in Section 5.3 below.
PKI Message Protection
Some PKI messages will be protected for integrity.
Note: If an asymmetric algorithm is used to protect a message and the relevant public component has been certified already, then the origin of the message can also be authenticated. On the other hand, if the public component is uncertified, then the message origin cannot be automatically authenticated but may be authenticated via out-of-band means.
When protection is applied, the following structure is used:

  PKIProtection ::= BIT STRING

The input to the calculation of PKIProtection is the DER encoding of the following data structure:

  ProtectedPart ::= SEQUENCE {
     header    PKIHeader,
     body      PKIBody
  }

There MAY be cases in which the PKIProtection BIT STRING is deliberately not used to protect a message (i.e., this OPTIONAL field is omitted) because other protection, external to PKIX, will be applied instead. Such a choice is explicitly allowed in this specification. Examples of such external protection include CMS [RFC5652] and Security Multiparts [RFC1847] encapsulation of the PKIMessage (or simply the PKIBody (omitting the CHOICE tag), if the relevant PKIHeader information is securely carried in the external mechanism). It is noted, however, that many such external mechanisms require that the end entity already possesses a public-key certificate, a unique DN, and/or other such infrastructure-related information. Thus, they may not be appropriate for initial registration, key-recovery, or any other process with "bootstrapping" characteristics. For those cases, it may be necessary that the PKIProtection parameter be used. In the future, if/when external mechanisms are modified to accommodate bootstrapping scenarios, the use of PKIProtection may become rare or non-existent.
Depending on the circumstances, the PKIProtection bits may contain a MAC or signature. Only the following cases can occur:
Shared Secret Information
In this case, the sender and recipient share secret information with sufficient entropy (established via out-of-band means). PKIProtection will contain a MAC value, and the protectionAlg MAY be one of the options described in CMP Algorithms.
The algorithm identifier id-PasswordBasedMac is defined in Section 4.4 of [RFC4211] and updated by [RFC9045]. It is mentioned in Section 6.1.1 of [RFC9481] for backward compatibility. More modern alternatives are listed in Section 6.1 of [RFC9481].

  id-PasswordBasedMac OBJECT IDENTIFIER ::= {1 2 840 113533 7 66 13}
  PBMParameter ::= SEQUENCE {
     salt                OCTET STRING,
     owf                 AlgorithmIdentifier,
     iterationCount      INTEGER,
     mac                 AlgorithmIdentifier
  }

The following text gives a method of key expansion to be used when the MAC algorithm requires an input length that is larger than the size of the one-way function (OWF).
Note: Section 4.4 of [RFC4211] and [RFC9045] do not mention this key expansion method or give an example using HMAC algorithms where key expansion is not needed. It is recognized that this omission in [RFC4211] can lead to confusion and possible incompatibility if key expansion [RFC4210] is not used when needed. Therefore, when key expansion is required (when K > H), the key expansion defined in the following text MUST be used.
In the above protectionAlg, the salt value is appended to the shared secret input. The OWF is then applied iterationCount times, where the salted secret is the input to the first iteration and, for each successive iteration, the input is set to be the output of the previous iteration. The output of the final iteration (called "BASEKEY" for ease of reference, with a size of "H") is what is used to form the symmetric key. If the MAC algorithm requires a K-bit key and K <= H, then the most significant K bits of BASEKEY are used. If K > H, then all of BASEKEY is used for the most significant H bits of the key, OWF("1" || BASEKEY) is used for the next most significant H bits of the key, OWF("2" || BASEKEY) is used for the next most significant H bits of the key, and so on, until all K bits have been derived. [Here "N" is the ASCII byte encoding the number N and "||" represents concatenation.]
Note: It is RECOMMENDED that the fields of PBMParameter remain constant throughout the messages of a single transaction (e.g., ir/ip/certConf/pkiConf) to reduce the overhead associated with PasswordBasedMac computation.
DH Key Pairs
Where the sender and receiver possess finite-field or elliptic-curve-based DH certificates with compatible DH parameters in order to protect the message, the end entity must generate a symmetric key based on its private DH key value and the DH public key of the recipient of the PKI message. PKIProtection will contain a MAC value keyed with this derived symmetric key, and the protectionAlg will be the following:

  id-DHBasedMac OBJECT IDENTIFIER ::= {1 2 840 113533 7 66 30}

  DHBMParameter ::= SEQUENCE {
     owf                 AlgorithmIdentifier,
     -- AlgId for an OWF
     mac                 AlgorithmIdentifier
     -- the MAC AlgId
  }

In the above protectionAlg, OWF is applied to the result of the DH computation. The OWF output (called "BASEKEY" for ease of reference, with a size of "H") is what is used to form the symmetric key. If the MAC algorithm requires a K-bit key and K <= H, then the most significant K bits of BASEKEY are used. If K > H, then all of BASEKEY is used for the most significant H bits of the key, OWF("1" || BASEKEY) is used for the next most significant H bits of the key, OWF("2" || BASEKEY) is used for the next most significant H bits of the key, and so on, until all K bits have been derived. [Here "N" is the ASCII byte encoding the number N and "||" represents concatenation.]
Note: Hash algorithms that can be used as OWFs are listed in CMP Algorithms.
Signature
In this case, the sender possesses a signature key pair and simply signs the PKI message. PKIProtection will contain the signature value and the protectionAlg will be an AlgorithmIdentifier for a digital signature, which MAY be one of the options described in CMP Algorithms.
Key Encapsulation
In case the sender of a message has a KEM key pair, it can be used to establish a shared secret key for MAC-based message protection. This can be used for message authentication.
This approach uses the definition of KEM algorithm functions in Section 1 of [RFC9629] as follows:
A KEM algorithm provides three functions:
1. KeyGen() -> (pk, sk): Generate a public key (pk) and a private (secret) key (sk).
2. Encapsulate(pk) -> (ct, ss): Given the public key (pk), produce a ciphertext (ct) and a shared secret (ss).
3. Decapsulate(sk, ct) -> (ss): Given the private key (sk) and the ciphertext (ct), produce the shared secret (ss).
To support a particular KEM algorithm, the PKI entity that possesses a KEM key pair and wishes to use it for MAC-based message protection MUST support the KEM Decapsulate() function. The PKI entity that wishes to verify the MAC-based message protection MUST support the KEM Encapsulate() function. The respective public KEM key is usually carried in a certificate [I-D.ietf-lamps-kyber-certificates].
Note: Both PKI entities send and receive messages in a PKI management operation. Both PKI entities may independently wish to protect messages using their KEM key pairs. For ease of explanation, we use the terms "Alice" to denote the PKI entity possessing the KEM key pair and who wishes to provide MAC-based message protection and "Bob" to denote the PKI entity having Alice's authentic public KEM key and who needs to verify the MAC-based protection provided by Alice.
Assuming Bob has Alice's KEM public key, he generates the ciphertext using KEM encapsulation and transfers it to Alice in an InfoTypeAndValue structure. Alice then retrieves the KEM shared secret from the ciphertext using KEM decapsulation and the associated KEM private key. Using a key derivation function (KDF), Alice derives a shared secret key from the KEM shared secret and other data sent by Bob. PKIProtection will contain a MAC value calculated using that shared secret key, and the protectionAlg will be the following:

  id-KemBasedMac OBJECT IDENTIFIER ::= {1 2 840 113533 7 66 16}

  KemBMParameter ::= SEQUENCE {
    kdf              AlgorithmIdentifier{KEY-DERIVATION, {...}},
    kemContext   [0] OCTET STRING OPTIONAL,
    len              INTEGER (1..MAX),
    mac              AlgorithmIdentifier{MAC-ALGORITHM, {...}}
  }

Note: The OID for id-KemBasedMac was assigned on the private-use arc { iso(1) member-body(2) us(840) nortelnetworks(113533) entrust(7) } and not assigned on an IANA-owned arc because the authors wished to place it on the same branch as the existing OIDs for id-PasswordBasedMac and id-DHBasedMac.
kdf is the algorithm identifier of the chosen KDF, and any associated parameters, used to derive the shared secret key.
kemContext MAY be used to transfer additional algorithm-specific context information (see also the definition of ukm in Section 3 of [RFC9629]).
len is the output length of the KDF and MUST be the desired size of the key to be used for MAC-based message protection.
mac is the algorithm identifier of the chosen MAC algorithm, and any associated parameters, used to calculate the MAC value.
The KDF and MAC algorithms MAY be chosen from the options in CMP Algorithms [RFC9481].
The InfoTypeAndValue transferring the KEM ciphertext uses OID id-it-KemCiphertextInfo. It contains a KemCiphertextInfo structure, as defined in Section 5.3.19.18.
Note: This InfoTypeAndValue can be carried in a genm/genp message body, as specified in Section 5.3.19.18, or in the generalInfo field of PKIHeader in messages of other types (see Section 5.1.1.5).
In the following, a generic message flow for MAC-based protection using KEM is specified in more detail. It is assumed that Bob possesses Alice's public KEM key. Alice can be the initiator of a PKI management operation or the responder. For more detailed figures, see Appendix E.
Generic Message Flow:
Generic Message Flow When Alice Has a KEM Key Pair

Step#

Alice

Bob

1

perform

KEM

Encapsulate

KEM

Ciphertext

2

perform

KEM

Decapsulate,

perform

key

derivation,

format

message

with

MAC-based

protection

message

3

perform

key

derivation,

verify

MAC-based

protection

Alice

authenticated

by

Bob

Step# Alice                                Bob
---------------------------------------------------------------------
  1                                        perform KEM Encapsulate
                      <-- KEM Ciphertext <--
  2   perform KEM Decapsulate,
        perform key derivation,
        format message with
        MAC-based protection
                      -->    message     -->
  3                                        perform key derivation,
                                             verify MAC-based
                                             protection
-------------------  Alice authenticated by Bob  --------------------

1. Bob needs to possess Alice's authentic public KEM key (pk), for instance, contained in a KEM certificate that was received and successfully validated by Bob beforehand.
Bob generates a shared secret (ss) and the associated ciphertext (ct) using the KEM Encapsulate function with Alice's public KEM key (pk). Bob MUST NOT reuse the ss and ct for other PKI management operations. From this data, Bob produces a KemCiphertextInfo structure, including the KEM algorithm identifier and the ciphertext (ct) and sends it to Alice in an InfoTypeAndValue structure, as defined in Section 5.3.19.18.
Encapsulate(pk) -> (ct, ss)
2. Alice decapsulates the shared secret (ss) from the ciphertext (ct) using the KEM Decapsulate function and its private KEM key (sk).
Decapsulate(ct, sk) -> (ss)
If the decapsulation operation outputs an error, any failInfo field in an error response message SHALL contain the value badMessageCheck and the PKI management operation SHALL be terminated.
Alice derives the shared secret key (ssk) using a KDF. The shared secret (ss) is used as input key material for the KDF, and the value len is the desired output length of the KDF as required by the MAC algorithm to be used for message protection. KDF, len, and MAC will be transferred to Bob in the protectionAlg KemBMParameter. The DER-encoded KemOtherInfo structure, as defined below, is used as context for the KDF.
KDF(ss, len, context)->(ssk)
The shared secret key (ssk) is used for MAC-based protection by Alice.
3. Bob derives the same shared secret key (ssk) using the KDF. Also here, the shared secret (ss) is used as input key material for the KDF, the value len is the desired output length for the KDF, and the DER-encoded KemOtherInfo structure constructed in the same way as on Alice's side is used as context for the KDF.
KDF(ss, len, context)->(ssk)
Bob uses the shared secret key (ssk) for verifying the MAC-based protection of the message received and in this way authenticates Alice.
This shared secret key (ssk) can be reused by Alice for MAC-based protection of further messages sent to Bob within the current PKI management operation.
This approach employs the notation of KDF(IKM, L, info) as described in Section 5 of [RFC9629] with the following changes:
- IKM is the input key material. It is the symmetric secret called "ss" resulting from the KEM.
- L is dependent of the MAC algorithm that is used with the shared secret key for CMP message protection and is called "len" in this document.
- info is an additional input to the KDF, is called "context" in this document, and contains the DER-encoded KemOtherInfo structure defined as:

  KemOtherInfo ::= SEQUENCE {
    staticString      PKIFreeText,
    transactionID     OCTET STRING,
    kemContext    [0] OCTET STRING OPTIONAL
  }

staticString MUST be "CMP-KEM".
transactionID MUST be the value from the message containing the ciphertext (ct) in KemCiphertextInfo.
Note: The transactionID is used to ensure domain separation of the derived shared secret key between different PKI management operations. For all PKI management operations with more than one exchange, the transactionID MUST be set anyway (see Section 5.1.1). In case Bob provided an infoValue of type KemCiphertextInfo to Alice in the initial request message (see Figure 4 of Appendix E), the transactionID MUST be set by Bob.
kemContext MAY contain additional algorithm-specific context information.
- OKM is the output keying material of the KDF used for MAC-based message protection of length len and is called "ssk" in this document.
There are various ways that Alice can request and Bob can provide the KEM ciphertext (see Appendix E for details). The KemCiphertextInfo can be requested using PKI general messages, as described in Section 5.3.19.18. Alternatively, the generalInfo field of the PKIHeader can be used to convey the same request and response InfoTypeAndValue structures, as described in Section 5.1.1.5. The procedure also works without Alice explicitly requesting the KEM ciphertext in case Bob knows one of Alice's KEM keys beforehand and can expect that she is ready to use it.
If both the initiator and responder in a PKI management operation have KEM key pairs, this procedure can be applied by both entities independently, establishing and using different shared secret keys for either direction.
Multiple Protection
When receiving a protected PKI message, a PKI management entity, such as an RA, MAY forward that message adding its own protection. Additionally, multiple PKI messages MAY be aggregated. There are several use cases for such messages.
- The RA confirms having validated and authorized a message and forwards the original message unchanged.
- A PKI management entity collects several messages that are to be forwarded in the same direction and forwards them in a batch. Request messages can be transferred as a batch upstream (towards the CA); response or announce messages can be transferred as a batch downstream (towards an RA but not to the end entity). For instance, this can be used when bridging an offline connection between two PKI management entities.
These use cases are accomplished by nesting the messages within a new PKI message. The structure used is as follows:

  NestedMessageContent ::= PKIMessages

In case an RA needs to modify a request message, it MAY include the original PKIMessage in the generalInfo field of the modified message, as described in Section 5.1.1.3.
Common Data Structures
Before specifying the specific types that may be placed in a PKIBody, we define some data structures that are used in more than one case.
Requested Certificate Contents
Various PKI management messages require that the originator of the message indicate some of the fields that are required to be present in a certificate. The CertTemplate structure allows entities requesting a certificate to specify the data fields that they want to be included. Typically, they are required to provide at least the publicKey field. A CertTemplate structure is identical to a TBSCertificate structure (see [RFC5280]) but with all fields optional/situational.
Note: Even if the originator completely specifies the contents of a certificate it requires, a CA is free to modify fields within the certificate actually issued. If the modified certificate is unacceptable to the requester, the requester MUST send back a certConf message that either does not include this certificate (via a CertHash) or does include this certificate (via a CertHash) along with a status of "rejected". See Section 5.3.18 for the definition and use of CertHash and the certConf message.
Note: Before requesting a new certificate, an end entity can request a certTemplate structure as a kind of certificate request blueprint in order to learn which data the CA expects to be present in the certificate request (see Section 5.3.19.16).
See CRMF [RFC4211] for CertTemplate syntax.
If certTemplate is an empty SEQUENCE (i.e., all fields omitted), then the controls field in the CertRequest structure MAY contain the id-regCtrl-altCertTemplate control, specifying a template for a certificate other than an X.509v3 public-key certificate. Conversely, if certTemplate is not empty (i.e., at least one field is present), then controls MUST NOT contain id-regCtrl-altCertTemplate. The new control is defined as follows:

  id-regCtrl-altCertTemplate OBJECT IDENTIFIER ::= { iso(1)
     identified-organization(3) dod(6) internet(1) security(5)
     mechanisms(5) pkix(7) pkip(5) regCtrl(1) 7}

  AltCertTemplate ::= AttributeTypeAndValue

Also see [RFC4212] for more details on how to manage certificates in alternative formats using CRMF [RFC4211] syntax.
Encrypted Values
When encrypted data like a private key, certificate, POP challenge, or revocation passphrase is sent in PKI messages, it is RECOMMENDED to use the EnvelopedData structure. In some cases, this is accomplished by using the EncryptedKey data structure instead of EncryptedValue.

  EncryptedKey ::= CHOICE {
     encryptedValue       EncryptedValue, -- deprecated
     envelopedData    [0] EnvelopedData }

See Certificate Request Message Format (CRMF) [RFC4211] for EncryptedKey and EncryptedValue syntax and Cryptographic Message Syntax (CMS) [RFC5652] for EnvelopedData syntax. Using the EncryptedKey data structure offers the choice to either use EncryptedValue (for backward compatibility only) or EnvelopedData. The use of the EncryptedValue structure has been deprecated in favor of the EnvelopedData structure. Therefore, it is RECOMMENDED to use EnvelopedData.
Note: The EncryptedKey structure defined in CRMF [RFC4211] is used here, which makes the update backward compatible. Using the new syntax with the untagged default choice EncryptedValue is bits-on-the-wire compatible with the old syntax.
To indicate support for EnvelopedData, the pvno cmp2021 has been introduced. Details on the usage of the protocol version number are described in Section 7.
The EnvelopedData structure is RECOMMENDED to be used in CMP to transport a private key, certificate, POP challenge, or revocation passphrase in encrypted form as follows:
- It contains only one RecipientInfo structure because the content is encrypted only for one recipient.
- It may contain a private key in the AsymmetricKeyPackage structure (which is placed in the encryptedContentInfo field), as defined in [RFC5958], that is wrapped in a SignedData structure, as specified in Section 5 of [RFC5652] and [RFC8933], signed by the KGA or CA.
- It may contain a certificate, POP challenge, or revocation passphrase directly in the encryptedContent field.
The content of the EnvelopedData structure, as specified in Section 6 of [RFC5652], MUST be encrypted using a newly generated symmetric content-encryption key. This content-encryption key MUST be securely provided to the recipient using one of four key management techniques.
The choice of the key management technique to be used by the sender depends on the credential available at the recipient:
- recipient's certificate with an algorithm identifier and a public key that supports key transport and where any given key usage extension allows keyEncipherment: The content-encryption key will be protected using the key transport key management technique, as specified in Section 6.2.1 of [RFC5652].
- recipient's certificate with an algorithm identifier and a public key that supports key agreement and where any given key usage extension allows keyAgreement: The content-encryption key will be protected using the key agreement key management technique, as specified in Section 6.2.2 of [RFC5652].
- a password or shared secret: The content-encryption key will be protected using the password-based key management technique, as specified in Section 6.2.4 of [RFC5652].
- recipient's certificate with an algorithm identifier and a public key that supports KEM and where any given key usage extension allows keyEncipherment: The content-encryption key will be protected using the key management technique for KEM keys, as specified in [RFC9629].
Note: There are cases where the algorithm identifier, the type of the public key, and the key usage extension will not be sufficient to decide on the key management technique to use, e.g., when rsaEncryption is the algorithm identifier. In such cases, it is a matter of local policy to decide.
Status Codes and Failure Information for PKI Messages
All response messages will include some status information. The following values are defined.

  PKIStatus ::= INTEGER {
     accepted               (0),
     grantedWithMods        (1),
     rejection              (2),
     waiting                (3),
     revocationWarning      (4),
     revocationNotification (5),
     keyUpdateWarning       (6)
  }

Responders may use the following syntax to provide more information about failure cases.

  PKIFailureInfo ::= BIT STRING {
     badAlg                 (0),
     badMessageCheck        (1),
     badRequest             (2),
     badTime                (3),
     badCertId              (4),
     badDataFormat          (5),
     wrongAuthority         (6),
     incorrectData          (7),
     missingTimeStamp       (8),
     badPOP                 (9),
     certRevoked            (10),
     certConfirmed          (11),
     wrongIntegrity         (12),
     badRecipientNonce      (13),
     timeNotAvailable       (14),
     unacceptedPolicy       (15),
     unacceptedExtension    (16),
     addInfoNotAvailable    (17),
     badSenderNonce         (18),
     badCertTemplate        (19),
     signerNotTrusted       (20),
     transactionIdInUse     (21),
     unsupportedVersion     (22),
     notAuthorized          (23),
     systemUnavail          (24),
     systemFailure          (25),
     duplicateCertReq       (26)
  }

  PKIStatusInfo ::= SEQUENCE {
     status        PKIStatus,
     statusString  PKIFreeText     OPTIONAL,
     failInfo      PKIFailureInfo  OPTIONAL
  }

Certificate Identification
In order to identify particular certificates, the CertId data structure is used.
See [RFC4211] for CertId syntax.
Out-of-Band Root CA Public Key
Each root CA that provides a self-signed certificate must be able to publish its current public key via some "out-of-band" means or together with the respective link certificate using an online mechanism. While such mechanisms are beyond the scope of this document, we define data structures that can support such mechanisms.
There are generally two methods available: Either the CA directly publishes its self-signed certificate, or this information is available via the directory (or equivalent) and the CA publishes a hash of this value to allow verification of its integrity before use.
Note: As an alternative to out-of-band distribution of root CA public keys, the CA can provide the self-signed certificate together with link certificates, e.g., using RootCaKeyUpdateContent (Section 5.3.19.15).

  OOBCert ::= Certificate

The fields within this certificate are restricted as follows:
- The certificate MUST be self-signed (i.e., the signature must be verifiable using the SubjectPublicKeyInfo field);
- The subject and issuer fields MUST be identical;
- If the subject field contains a "NULL-DN", then both subjectAltNames and issuerAltNames extensions MUST be present and have exactly the same value; and
- The values of all other extensions must be suitable for a self-signed certificate (e.g., key identifiers for the subject and issuer must be the same).

  OOBCertHash ::= SEQUENCE {
     hashAlg     [0] AlgorithmIdentifier     OPTIONAL,
     certId      [1] CertId                  OPTIONAL,
     hashVal         BIT STRING
  }

The intention of the hash value is that anyone who has securely received the hash value (via the out-of-band means) can verify a self-signed certificate for that CA.
Archive Options
Requesters may indicate that they wish the PKI to archive a private key value using the PKIArchiveOptions structure.
See [RFC4211] for PKIArchiveOptions syntax.
Publication Information
Requesters may indicate that they wish the PKI to publish a certificate using the PKIPublicationInfo structure.
See [RFC4211] for PKIPublicationInfo syntax.
POP Structures
The POP structure used is indicated in the popo field of type ProofOfPossession in the CertReqMsg sequence (see Section 4 of [RFC4211]).

   ProofOfPossession ::= CHOICE {
      raVerified      [0] NULL,
      signature       [1] POPOSigningKey,
      keyEncipherment [2] POPOPrivKey,
      keyAgreement    [3] POPOPrivKey
   }

raVerified
An end entity MUST NOT use raVerified. If an RA performs changes to a certification request breaking the provided POP, or if the RA requests a certificate on behalf of an end entity and cannot provide the POP itself, the RA MUST use raVerified. Otherwise, it SHOULD NOT use raVerified.
When introducing raVerified, the RA MUST check the existing POP, or it MUST ensure by other means that the end entity is the holder of the private key. The RA MAY provide the original message containing the POP in the generalInfo field using the id-it-origPKIMessage (see Section 5.1.1.3) enabling the CA to verify it.
POPOSigningKey Structure
If the certification request is for a key pair that supports signing (i.e., a request for a verification certificate), then the POP of the private key is demonstrated through use of the POPOSigningKey structure; for details, see Section 4.1 of [RFC4211].

   POPOSigningKey ::= SEQUENCE {
      poposkInput [0] POPOSigningKeyInput OPTIONAL,
      algorithmIdentifier AlgorithmIdentifier,
      signature BIT STRING
   }

   POPOSigningKeyInput ::= SEQUENCE {
      authInfo CHOICE {
         sender [0] GeneralName,
         publicKeyMAC PKMACValue
      },
      publicKey SubjectPublicKeyInfo
   }

   PKMACValue ::= SEQUENCE {
      algId AlgorithmIdentifier,
      value BIT STRING
   }

Note: For the purposes of this specification, the ASN.1 comment given in Appendix C of [RFC4211] pertains not only to certTemplate but also to the altCertTemplate control, as defined in Section 5.2.1.
If certTemplate (or the altCertTemplate control) contains the subject and publicKey values, then poposkInput MUST be omitted and the signature MUST be computed on the DER-encoded value of the certReq field of the CertReqMsg (or the DER-encoded value of AltCertTemplate). If certTemplate/altCertTemplate does not contain both the subject and public key values (i.e., if it contains only one of these or neither), then poposkInput MUST be present and the signature MUST be computed on the DER-encoded value of poposkInput (i.e., the "value" OCTETs of the POPOSigningKeyInput DER).
In the special case that the CA/RA has a DH certificate that is known to the end entity and the certification request is for a key agreement key pair, the end entity can also use the POPOSigningKey structure (where the algorithmIdentifier field is DHBasedMAC and the signature field is the MAC) for demonstrating POP.
POPOPrivKey Structure
If the certification request is for a key pair that does not support signing (i.e., a request for an encryption or key agreement certificate), then the POP of the private key is demonstrated through use of the POPOPrivKey structure in one of the following three ways; for details see Sections 4.2 and 4.3 in [RFC4211].

   POPOPrivKey ::= CHOICE {
      thisMessage [0] BIT STRING, -- deprecated
      subsequentMessage [1] SubsequentMessage,
      dhMAC [2] BIT STRING, -- deprecated
      agreeMAC [3] PKMACValue,
      encryptedKey [4] EnvelopedData
   }

   SubsequentMessage ::= INTEGER {
      encrCert (0),
      challengeResp (1)
   }

When using agreeMAC or encryptedKey choices, the pvno cmp2021(3) MUST be used. Details on the usage of the protocol version number are described in Section 7.
Inclusion of the Private Key
This method mentioned previously in Section 4.3 demonstrates POP of the private key by including the encrypted private key in the CertRequest in the POPOPrivKey structure or in the PKIArchiveOptions control structure. This method SHALL only be used if archival of the private key is desired.
For a certification request message indicating cmp2021(3) in the pvno field of the PKIHeader, the encrypted private key MUST be transferred in the encryptedKey choice of POPOPrivKey (or within the PKIArchiveOptions control) in a CMS EnvelopedData structure, as defined in Section 5.2.2.
Note: The thisMessage choice has been deprecated in favor of encryptedKey. When using cmp2000(2) in the certification request message header for backward compatibility, the thisMessage choice of POPOPrivKey is used containing the encrypted private key in an EncryptedValue structure wrapped in a BIT STRING. This allows the necessary conveyance and protection of the private key while maintaining bits-on-the-wire compatibility with [RFC4211].
Indirect Method - Encrypted Certificate
The indirect method mentioned previously in Section 4.3 demonstrates POP of the private key by having the CA return the requested certificate in encrypted form (see Section 5.2.2). This method is indicated in the CertRequest by requesting the encrCert option in the subsequentMessage choice of POPOPrivKey.

end

entity

RA/CA

req

rep

(enc

cert)

conf

(cert

hash)

ack

        end entity                         RA/CA
                 ----       req        ---->
                 <---  rep (enc cert)  -----
                 ---- conf (cert hash) ---->
                 <---       ack        -----

The end entity proves knowledge of the private key to the CA by providing the correct CertHash for this certificate in the certConf message. This demonstrates POP because the end entity can only compute the correct CertHash if it is able to recover the encrypted certificate, and it can only recover the certificate if it is able to obtain the symmetric key using the required private key. Clearly, for this to work, the CA MUST NOT publish the certificate until the certConf message arrives (when certHash is to be used to demonstrate POP). See Section 5.3.18 for further details, and see Section 8.11 for security considerations regarding use of CT logs.
The recipient SHOULD maintain a context of the PKI management operation, e.g., using transactionID and certReqId, to identify the private key to use when decrypting the EnvelopedData containing the newly issued certificate. The recipient may be unable to use the RecipientInfo structure as it refers to the certificate that is still encrypted. The sender MUST populate the rid field as specified by CMS, and the client MAY ignore it.
Direct Method - Challenge-Response Protocol
The direct method mentioned previously in Section 4.3 demonstrates POP of the private key by having the end entity engage in a challenge-response protocol (using the messages popdecc of type POPODecKeyChall and popdecr of type POPODecKeyResp; see below) between CertReqMessages and CertRepMessage. This method is indicated in the CertRequest by requesting the challengeResp option in the subsequentMessage choice of POPOPrivKey.
Note: This method would typically be used in an environment in which an RA verifies POP and then makes a certification request to the CA on behalf of the end entity. In such a scenario, the CA trusts the RA to have done POP correctly before the RA requests a certificate for the end entity.
The complete protocol then looks as follows (note that req' does not necessarily encapsulate req as a nested message):

end

entity

RA

CA

req

chall

resp

req'

rep

conf

ack

rep

conf

ack

        end entity            RA            CA
                 ---- req ---->
                 <--- chall ---
                 ---- resp --->
                               ---- req' --->
                               <--- rep -----
                               ---- conf --->
                               <--- ack -----
                 <--- rep -----
                 ---- conf --->
                 <--- ack -----

This protocol is obviously much longer than the exchange given in Section 5.2.8.3.2 above but allows a Local Registration Authority (LRA) to be involved and has the property that the certificate itself is not actually created until the POP is complete. In some environments, a different order of the above messages may be required, such as the following (this may be determined by policy):

end

entity

RA

CA

req

chall

resp

req'

rep

rep

conf

conf

ack

ack

        end entity            RA            CA
                 ---- req ---->
                 <--- chall ---
                 ---- resp --->
                               ---- req' --->
                               <--- rep -----
                 <--- rep -----
                 ---- conf --->
                               ---- conf --->
                               <--- ack -----
                 <--- ack -----

The challenge-response messages for POP of a private key are specified as follows (for decryption keys, see [MvOV97], p.404 for details). This challenge-response exchange is associated with the preceding certification request message (and subsequent certification response and confirmation messages) by the transactionID used in the PKIHeader and by the protection applied to the PKIMessage.

   POPODecKeyChallContent ::= SEQUENCE OF Challenge

   Challenge ::= SEQUENCE {
      owf AlgorithmIdentifier OPTIONAL,
      witness OCTET STRING,
      challenge OCTET STRING, -- deprecated
      encryptedRand [0] EnvelopedData OPTIONAL
   }

   Rand ::= SEQUENCE {
      int INTEGER,
      sender GeneralName
   }

More details on the fields in this syntax are available in Appendix F.
For a popdecc message indicating cmp2021(3) in the pvno field of the PKIHeader, the encryption of Rand MUST be transferred in the encryptedRand field in a CMS EnvelopedData structure as defined in Section 5.2.2. The challenge field MUST contain an empty OCTET STRING.
The recipient SHOULD maintain a context of the PKI management operation, e.g., using transactionID and certReqId, to identify the private key to use when decrypting encryptedRand. The sender MUST populate the rid field in the EnvelopedData sequence using the issuerAndSerialNumber choice containing a NULL-DN as issuer and the certReqId as serialNumber. The client MAY ignore the rid field.
Note: The challenge field has been deprecated in favor of encryptedRand. When using cmp2000(2) in the popdecc message header for backward compatibility, the challenge field MUST contain the encryption (involving the public key for which the certification request is being made) of Rand and encryptedRand MUST be omitted. Using challenge (omitting the optional encryptedRand field) is bit-compatible with [RFC4210]. Note that the size of Rand, when used with challenge, needs to be appropriate for encryption, involving the public key of the requester. If, in some environment, names are so long that they cannot fit (e.g., very long DNs), then whatever portion will fit should be used (as long as it includes at least the common name, and as long as the receiver is able to deal meaningfully with the abbreviation).

   POPODecKeyRespContent ::= SEQUENCE OF INTEGER

On receiving the popdecc message, the end entity decrypts all included challenges and responds with a popdecr message containing the decrypted integer values in the same order.
Summary of POP Options
The text in this section provides several options with respect to POP techniques. Using "SK" for "signing key", "EK" for "encryption key", "KAK" for "key agreement key", and "KEMK" for "key encapsulation mechanism key", the techniques may be summarized as follows:
- RAVerified;
- SKPOP;
- EKPOPThisMessage; -- deprecated
- KAKPOPThisMessage; -- deprecated
- EKPOPEncryptedKey;
- KAKPOPEncryptedKey;
- KEMKPOPEncryptedKey;
- KAKPOPThisMessageDHMAC;
- EKPOPEncryptedCert;
- KAKPOPEncryptedCert;
- KEMKPOPEncryptedCert;
- EKPOPChallengeResp;
- KAKPOPChallengeResp; and
- KEMKPOPChallengeResp.
Given this array of options, it is natural to ask how an end entity can know what is supported by the CA/RA (i.e., which options it may use when requesting certificates). The following guidelines should clarify this situation for end entity implementers.
- RAVerified: This is not an end entity decision; the RA uses this if and only if it has verified POP before forwarding the request on to the CA, so it is not possible for the end entity to choose this technique.
- SKPOP: If the end entity has a signing key pair, this is the only POP method specified for use in the request for a corresponding certificate.
- EKPOPThisMessage (deprecated), KAKPOPThisMessage (deprecated), EKPOPEncryptedKey, KAKPOPEncryptedKey, KEMKPOPEncryptedKey: Whether or not to give up its private key to the CA/RA is an end entity decision. If the end entity decides to reveal its key, then these are the only POP methods available in this specification to achieve this (and the key pair type and protocol version used will determine which of these methods to use). The reason for deprecating EKPOPThisMessage and KAKPOPThisMessage options has been given in Section 5.2.8.3.1.
- KAKPOPThisMessageDHMAC: The end entity can only use this method if (1) the CA/RA has a DH certificate available for this purpose and (2) the end entity already has a copy of this certificate. If both these conditions hold, then this technique is clearly supported and may be used by the end entity, if desired.
- EKPOPEncryptedCert, KAKPOPEncryptedCert, KEMKPOPEncryptedCert, EKPOPChallengeResp, KAKPOPChallengeResp, and KEMKPOPChallengeResp: The end entity picks one of these (in the subsequentMessage field) in the request message, depending upon preference and key pair type. The end entity is not doing POP at this point; it is simply indicating which method it wants to use. Therefore, if the CA/RA replies with a "badPOP" error, the end entity can re-request using the other POP method chosen in subsequentMessage. Note, however, that this specification encourages the use of the EncryptedCert choice and, furthermore, says that the challenge-response would typically be used when an RA is involved and doing POP verification. Thus, the end entity should be able to make an intelligent decision regarding which of these POP methods to choose in the request message.
GeneralizedTime
GeneralizedTime is a standard ASN.1 type and SHALL be used as specified in Section 4.1.2.5.2 of [RFC5280].
Operation-Specific Data Structures
Initialization Request
An Initialization request message contains as the PKIBody a CertReqMessages data structure, which specifies the requested certificate(s). Typically, SubjectPublicKeyInfo, KeyId, and Validity are the template fields that may be supplied for each certificate requested (see the profiles defined in Section 4.1.1 of [RFC9483] and Appendices C.4 and D.7 for further information). This message is intended to be used for entities when first initializing into the PKI.
See Section 5.2.1 and [RFC4211] for CertReqMessages syntax.
Initialization Response
An Initialization response message contains as the PKIBody a CertRepMessage data structure, which has for each certificate requested a PKIStatusInfo field, a subject certificate, and possibly a private key (normally encrypted using EnvelopedData; see Section 4.1.6 of [RFC9483] for further information).
See Section 5.3.4 for CertRepMessage syntax. Note that if the PKI message protection is "shared secret information" (see Section 5.1.3.1), then any certificate transported in the caPubs field may be directly trusted as a root CA certificate by the initiator.
Certification Request
A Certification request message contains as the PKIBody a CertReqMessages data structure, which specifies the requested certificates (see the profiles defined in Section 4.1.2 of [RFC9483] and Appendix C.2 for further information). This message is intended to be used for existing PKI entities who wish to obtain additional certificates.
See Section 5.2.1 and [RFC4211] for CertReqMessages syntax.
Alternatively, the PKIBody MAY be a CertificationRequest (this structure is fully specified by the ASN.1 structure CertificationRequest given in [RFC2986]; see the profiles defined in Section 4.1.4 of [RFC9483] for further information). This structure may be required for certificate requests for signing key pairs when interoperation with legacy systems is desired, but its use is strongly discouraged whenever not absolutely necessary.
Certification Response
A Certification response message contains as the PKIBody a CertRepMessage data structure, which has a status value for each certificate requested and optionally has a CA public key, failure information, a subject certificate, and an encrypted private key.

  CertRepMessage ::= SEQUENCE {
     caPubs          [1] SEQUENCE SIZE (1..MAX) OF CMPCertificate
                         OPTIONAL,
     response            SEQUENCE OF CertResponse
  }

  CertResponse ::= SEQUENCE {
     certReqId           INTEGER,
     status              PKIStatusInfo,
     certifiedKeyPair    CertifiedKeyPair     OPTIONAL,
     rspInfo             OCTET STRING         OPTIONAL
     -- analogous to the id-regInfo-utf8Pairs string defined
     -- for regInfo in CertReqMsg [RFC4211]
  }

  CertifiedKeyPair ::= SEQUENCE {
     certOrEncCert       CertOrEncCert,
     privateKey      [0] EncryptedKey         OPTIONAL,
     -- See [RFC4211] for comments on encoding.
     publicationInfo [1] PKIPublicationInfo   OPTIONAL
  }

  CertOrEncCert ::= CHOICE {
     certificate     [0] CMPCertificate,
     encryptedCert   [1] EncryptedKey
  }

A p10cr message contains exactly one CertificationRequestInfo data structure, as specified in PKCS #10 [RFC2986], but no certReqId. Therefore, the certReqId in the corresponding Certification Response (cp) message MUST be set to -1.
Only one of the failInfo (in PKIStatusInfo) and certificate (in CertifiedKeyPair) fields can be present in each CertResponse (depending on the status). For some status values (e.g., waiting), neither of the optional fields will be present.
Given an EncryptedCert and the relevant decryption key, the certificate may be obtained. The purpose of this is to allow a CA to return the value of a certificate but with the constraint that only the intended recipient can obtain the actual certificate. The benefit of this approach is that a CA may reply with a certificate even in the absence of proof that the requester is the end entity that can use the relevant private key (note that the proof is not obtained until the certConf message is received by the CA). Thus, the CA will not have to revoke that certificate in the event that something goes wrong with the POP (but MAY do so anyway, depending upon policy).
The use of EncryptedKey is described in Section 5.2.2.
Note: To indicate support for EnvelopedData, the pvno cmp2021 has been introduced. Details on the usage of different protocol version numbers are described in Section 7.
Key Update Request Content
For key update requests, the CertReqMessages syntax is used. Typically, SubjectPublicKeyInfo, KeyId, and Validity are the template fields that may be supplied for each key to be updated (see the profiles defined in Section 4.1.3 of [RFC9483] and Appendix C.6 for further information). This message is intended to be used to request updates to existing (non-revoked and non-expired) certificates (therefore, it is sometimes referred to as a "Certificate Update" operation). An update is a replacement certificate containing either a new subject public key or the current subject public key (although the latter practice may not be appropriate for some environments).
See Section 5.2.1 and [RFC4211] for CertReqMessages syntax.
Key Update Response Content
For key update responses, the CertRepMessage syntax is used. The response is identical to the initialization response.
See Section 5.3.4 for CertRepMessage syntax.
Key Recovery Request Content
For key recovery requests, the syntax used is identical to the initialization request CertReqMessages. Typically, SubjectPublicKeyInfo and KeyId are the template fields that may be used to supply a signature public key for which a certificate is required.
See Section 5.2.1 and [RFC4211] for CertReqMessages syntax. Note that if a key history is required, the requester must supply a protocol encryption key control in the request message.
Key Recovery Response Content
For key recovery responses, the following syntax is used. For some status values (e.g., waiting), none of the optional fields will be present.

  KeyRecRepContent ::= SEQUENCE {
     status            PKIStatusInfo,
     newSigCert    [0] Certificate                 OPTIONAL,
     caCerts       [1] SEQUENCE SIZE (1..MAX) OF
                                  Certificate      OPTIONAL,
     keyPairHist   [2] SEQUENCE SIZE (1..MAX) OF
                                  CertifiedKeyPair OPTIONAL
  }

Revocation Request Content
When requesting revocation of a certificate (or several certificates), the following data structure is used (see the profiles defined in Section 4.2 of [RFC9483] for further information). The name of the requester is present in the PKIHeader structure.

  RevReqContent ::= SEQUENCE OF RevDetails

  RevDetails ::= SEQUENCE {
     certDetails         CertTemplate,
     crlEntryDetails     Extensions       OPTIONAL
  }

Revocation Response Content
The revocation response is the response to the above message. If produced, this is sent to the requester of the revocation. (A separate revocation announcement message MAY be sent to the subject of the certificate for which revocation was requested.)

  RevRepContent ::= SEQUENCE {
     status        SEQUENCE SIZE (1..MAX) OF PKIStatusInfo,
     revCerts  [0] SEQUENCE SIZE (1..MAX) OF CertId OPTIONAL,
     crls      [1] SEQUENCE SIZE (1..MAX) OF CertificateList
                   OPTIONAL
  }

Cross-Certification Request Content
Cross-certification requests use the same syntax (CertReqMessages) as normal certification requests, with the restriction that the key pair MUST have been generated by the requesting CA and the private key MUST NOT be sent to the responding CA (see the profiles defined in Appendix D.6 for further information). This request MAY also be used by subordinate CAs to get their certificates signed by the parent CA.
See Section 5.2.1 and [RFC4211] for CertReqMessages syntax.
Cross-Certification Response Content
Cross-certification responses use the same syntax (CertRepMessage) as normal certification responses, with the restriction that no encrypted private key can be sent.
See Section 5.3.4 for CertRepMessage syntax.
CA Key Update Announcement Content
When a CA updates its own key pair, the following data structure MAY be used to announce this event.

  RootCaKeyUpdateContent ::= SEQUENCE {
     newWithNew              CMPCertificate,
     newWithOld          [0] CMPCertificate OPTIONAL,
     oldWithNew          [1] CMPCertificate OPTIONAL
  }

CAKeyUpdContent ::= CHOICE {
    cAKeyUpdAnnV2      CAKeyUpdAnnContent, -- deprecated
    cAKeyUpdAnnV3  [0] RootCaKeyUpdateContent
}

When using RootCaKeyUpdateContent in the ckuann message, the pvno cmp2021 MUST be used. Details on the usage of the protocol version number are described in Section 7.
In contrast to CAKeyUpdAnnContent as supported with cmp2000, RootCaKeyUpdateContent offers omitting newWithOld and oldWithNew, depending on the needs of the end entity.
Certificate Announcement
This structure MAY be used to announce the existence of certificates.
Note that this message is intended to be used for those cases (if any) where there is no pre-existing method for publication of certificates; it is not intended to be used where, for example, X.500 is the method for publication of certificates.

  CertAnnContent ::= Certificate

Revocation Announcement
When a CA has revoked, or is about to revoke, a particular certificate, it MAY issue an announcement of this (possibly upcoming) event.

  RevAnnContent ::= SEQUENCE {
     status              PKIStatus,
     certId              CertId,
     willBeRevokedAt     GeneralizedTime,
     badSinceDate        GeneralizedTime,
     crlDetails          Extensions  OPTIONAL
  }

A CA MAY use such an announcement to warn (or notify) a subject that its certificate is about to be (or has been) revoked. This would typically be used where the request for revocation did not come from the subject concerned.
The willBeRevokedAt field contains the time at which a new entry will be added to the relevant CRLs.
CRL Announcement
When a CA issues a new CRL (or set of CRLs), the following data structure MAY be used to announce this event.

  CRLAnnContent ::= SEQUENCE OF CertificateList

PKI Confirmation Content
This data structure is used in the protocol exchange as the final PKIMessage. Its content is the same in all cases -- actually, there is no content since the PKIHeader carries all the required information.

  PKIConfirmContent ::= NULL

Use of this message for certificate confirmation is NOT RECOMMENDED; certConf SHOULD be used instead. Upon receiving a pkiconf for a certificate response, the recipient MAY treat it as a certConf with all certificates being accepted.
Certificate Confirmation Content
This data structure is used by the client to send a confirmation to the CA/RA to accept or reject certificates.

  CertConfirmContent ::= SEQUENCE OF CertStatus

  CertStatus ::= SEQUENCE {
     certHash    OCTET STRING,
     certReqId   INTEGER,
     statusInfo  PKIStatusInfo OPTIONAL,
     hashAlg [0] AlgorithmIdentifier{DIGEST-ALGORITHM, {...}}
                 OPTIONAL
  }

The hashAlg field SHOULD be used only in exceptional cases where the signatureAlgorithm of the certificate to be confirmed does not specify a hash algorithm in the OID or in the parameters or no hash algorithm is specified for hashing certificates signed using the signatureAlgorithm. Note that for EdDSA, a hash algorithm is specified in Section 3.3 of [RFC9481], such that the hashAlg field is not needed for EdDSA. Otherwise, the certHash value SHALL be computed using the same hash algorithm as used to create and verify the certificate signature or as specified for hashing certificates signed using the signatureAlgorithm. If hashAlg is used, the CMP version indicated by the certConf message header must be cmp2021(3).
For any particular CertStatus, omission of the statusInfo field indicates acceptance of the specified certificate. Alternatively, explicit status details (with respect to acceptance or rejection) MAY be provided in the statusInfo field, perhaps for auditing purposes at the CA/RA.
Within CertConfirmContent, omission of a CertStatus structure corresponding to a certificate supplied in the previous response message indicates rejection of the certificate. Thus, an empty CertConfirmContent (a zero-length SEQUENCE) MAY be used to indicate rejection of all supplied certificates. See Section 5.2.8.3.2 for a discussion of the certHash field with respect to POP.
PKI General Message Content

  InfoTypeAndValue ::= SEQUENCE {
     infoType               OBJECT IDENTIFIER,
     infoValue              ANY DEFINED BY infoType  OPTIONAL
  }

  -- where {id-it} = {id-pkix 4} = {1 3 6 1 5 5 7 4}
  GenMsgContent ::= SEQUENCE OF InfoTypeAndValue

CA Protocol Encryption Certificate
This MAY be used by the end entity to get a certificate from the CA to use to protect sensitive information during the protocol.

  GenMsg:    {id-it 1}, < absent >
  GenRep:    {id-it 1}, Certificate | < absent >

End entities MUST ensure that the correct certificate is used for this purpose.
Signing Key Pair Types
This MAY be used by the end entity to get the list of signature algorithms whose subject public key values the CA is willing to certify.

  GenMsg:    {id-it 2}, < absent >
  GenRep:    {id-it 2}, SEQUENCE SIZE (1..MAX) OF
                          AlgorithmIdentifier

Note: For the purposes of this exchange, rsaEncryption and sha256WithRSAEncryption, for example, are considered to be equivalent; the question being asked is, "Is the CA willing to certify an RSA public key?"
Note: In case several elliptic curves are supported, several id-ecPublicKey elements as defined in [RFC5480] need to be given, one per named curve.
Encryption / Key Agreement Key Pair Types
This MAY be used by the client to get the list of encryption / key agreement algorithms whose subject public key values the CA is willing to certify.

  GenMsg:    {id-it 3}, < absent >
  GenRep:    {id-it 3}, SEQUENCE SIZE (1..MAX) OF
                          AlgorithmIdentifier

Note: In case several elliptic curves are supported, several id-ecPublicKey elements as defined in [RFC5480] need to be given, one per named curve.
Preferred Symmetric Algorithm
This MAY be used by the client to get the CA-preferred symmetric encryption algorithm for any confidential information that needs to be exchanged between the end entity and the CA (for example, if the end entity wants to send its private decryption key to the CA for archival purposes).

  GenMsg:    {id-it 4}, < absent >
  GenRep:    {id-it 4}, AlgorithmIdentifier

Updated CA Key Pair
This MAY be used by the CA to announce a CA key update event.

  GenMsg:    {id-it 18}, RootCaKeyUpdateValue

See Section 5.3.13 for details of CA key update announcements.
CRL
This MAY be used by the client to get a copy of the latest CRL.

  GenMsg:    {id-it 6}, < absent >
  GenRep:    {id-it 6}, CertificateList

Unsupported Object Identifiers
This is used by the server to return a list of object identifiers that it does not recognize or support from the list submitted by the client.

  GenRep:    {id-it 7}, SEQUENCE SIZE (1..MAX) OF OBJECT IDENTIFIER

Key Pair Parameters
This MAY be used by the end entity to request the domain parameters to use for generating the key pair for certain public-key algorithms. It can be used, for example, to request the appropriate P, Q, and G to generate the DH/DSA key or to request a set of well-known elliptic curves.

  GenMsg:    {id-it 10}, OBJECT IDENTIFIER -- (Algorithm object-id)
  GenRep:    {id-it 11}, AlgorithmIdentifier | < absent >

An absent infoValue in the GenRep indicates that the algorithm specified in GenMsg is not supported.
End entities MUST ensure that the parameters are acceptable to it and that the GenRep message is authenticated (to avoid substitution attacks).
Revocation Passphrase
This MAY be used by the end entity to send a passphrase to a CA/RA for the purpose of authenticating a later revocation request (in the case that the appropriate signing private key is no longer available to authenticate the request). See Appendix B for further details on the use of this mechanism.

  GenMsg:    {id-it 12}, EncryptedKey
  GenRep:    {id-it 12}, < absent >

The use of EncryptedKey is described in Section 5.2.2.
ImplicitConfirm
See Section 5.1.1.1 for the definition and use of {id-it 13}.
ConfirmWaitTime
See Section 5.1.1.2 for the definition and use of {id-it 14}.
Original PKIMessage
See Section 5.1.1.3 for the definition and use of {id-it 15}.
Supported Language Tags
This MAY be used to determine the appropriate language tag [RFC5646] to use in subsequent messages. The sender sends its list of supported languages (in order of most to least preferred); the receiver returns the one it wishes to use. (Note: Each UTF8String MUST include a language tag.) If none of the offered tags are supported, an error MUST be returned.

  GenMsg:    {id-it 16}, SEQUENCE SIZE (1..MAX) OF UTF8String
  GenRep:    {id-it 16}, SEQUENCE SIZE (1) OF UTF8String

CA Certificates
This MAY be used by the client to get CA certificates.

  GenMsg:    {id-it 17}, < absent >
  GenRep:    {id-it 17}, SEQUENCE SIZE (1..MAX) OF
                           CMPCertificate | < absent >

Root CA Update
This MAY be used by the client to get an update of a root CA certificate, which is provided in the body of the request message. In contrast to the ckuann message, this approach follows the request/response model.
The end entity SHOULD reference its current trust anchor in RootCaCertValue in the request body, giving the root CA certificate if available.

  GenMsg:    {id-it 20}, RootCaCertValue | < absent >
  GenRep:    {id-it 18}, RootCaKeyUpdateValue | < absent >

  RootCaCertValue ::= CMPCertificate

  RootCaKeyUpdateValue ::= RootCaKeyUpdateContent

  RootCaKeyUpdateContent ::= SEQUENCE {
     newWithNew              CMPCertificate,
     newWithOld          [0] CMPCertificate OPTIONAL,
     oldWithNew          [1] CMPCertificate OPTIONAL
  }

Note: In contrast to CAKeyUpdAnnContent (which was deprecated with pvno cmp2021), RootCaKeyUpdateContent offers omitting newWithOld and oldWithNew, depending on the needs of the end entity.
Certificate Request Template
This MAY be used by the client to get a template containing requirements for certificate request attributes and extensions. The controls id-regCtrl-algId and id-regCtrl-rsaKeyLen MAY contain details on the types of subject public keys the CA is willing to certify.
The id-regCtrl-algId control MAY be used to identify a cryptographic algorithm (see Section 4.1.2.7 of [RFC5280]) other than rsaEncryption. The algorithm field SHALL identify a cryptographic algorithm. The contents of the optional parameters field will vary according to the algorithm identified. For example, when the algorithm is set to id-ecPublicKey, the parameters identify the elliptic curve to be used; see [RFC5480].
Note: The client may specify a profile name in the certProfile field (see Section 5.1.1.4).
The id-regCtrl-rsaKeyLen control SHALL be used for algorithm rsaEncryption and SHALL contain the intended modulus bit length of the RSA key.

  GenMsg:    {id-it 19}, < absent >
  GenRep:    {id-it 19}, CertReqTemplateContent | < absent >

  CertReqTemplateValue  ::= CertReqTemplateContent

  CertReqTemplateContent ::= SEQUENCE {
     certTemplate           CertTemplate,
     keySpec                Controls OPTIONAL }

  Controls  ::= SEQUENCE SIZE (1..MAX) OF AttributeTypeAndValue

  id-regCtrl-algId OBJECT IDENTIFIER ::= { iso(1)
     identified-organization(3) dod(6) internet(1) security(5)
     mechanisms(5) pkix(7) pkip(5) regCtrl(1) 11 }

  AlgIdCtrl ::= AlgorithmIdentifier{ALGORITHM, {...}}

  id-regCtrl-rsaKeyLen OBJECT IDENTIFIER ::= { iso(1)
     identified-organization(3) dod(6) internet(1) security(5)
     mechanisms(5) pkix(7) pkip(5) regCtrl(1) 12 }

  RsaKeyLenCtrl ::= INTEGER (1..MAX)

The CertReqTemplateValue contains the prefilled certTemplate to be used for a future certificate request. The publicKey field in the certTemplate MUST NOT be used. In case the PKI management entity wishes to specify supported public-key algorithms, the keySpec field MUST be used. One AttributeTypeAndValue per supported algorithm or RSA key length MUST be used.
Note: The controls for an ASN.1 type are defined in CRMF.
CRL Update Retrieval
This MAY be used by the client to get new CRLs, specifying the source of the CRLs and the thisUpdate value of the latest CRL it already has, if available. A CRL source is given either by a DistributionPointName or the GeneralNames of the issuing CA. The DistributionPointName should be treated as an internal pointer to identify a CRL that the server already has and not as a way to ask the server to fetch CRLs from external locations. The server SHALL only provide those CRLs that are more recent than the ones indicated by the client.

  GenMsg:    {id-it 22}, SEQUENCE SIZE (1..MAX) OF CRLStatus
  GenRep:    {id-it 23}, SEQUENCE SIZE (1..MAX) OF
                           CertificateList  |  < absent >

  CRLSource ::= CHOICE {
     dpn          [0] DistributionPointName,
     issuer       [1] GeneralNames }

  CRLStatus ::= SEQUENCE {
     source       CRLSource,
     thisUpdate   Time OPTIONAL }

KEM Ciphertext
This MAY be used by a PKI entity to get the KEM ciphertext for MAC-based message protection using KEM (see Section 5.1.3.4).
The PKI entity that possesses a KEM key pair can request the ciphertext by sending an InfoTypeAndValue structure of type KemCiphertextInfo where the infoValue is absent. The ciphertext can be provided in the following genp message with an InfoTypeAndValue structure of the same type.

  GenMsg:    {id-it 24}, < absent >
  GenRep:    {id-it 24}, KemCiphertextInfo

  KemCiphertextInfo ::= SEQUENCE {
    kem              AlgorithmIdentifier{KEM-ALGORITHM, {...}},
    ct               OCTET STRING
  }

kem is the algorithm identifier of the KEM algorithm, and any associated parameters, used to generate the ciphertext (ct).
ct is the ciphertext output from the KEM Encapsulate function.
Note: These InfoTypeAndValue structures can also be transferred in the generalInfo field of the PKIHeader in messages of other types (see Section 5.1.1.5).
PKI General Response Content

  GenRepContent ::= SEQUENCE OF InfoTypeAndValue

Examples of GenReps that MAY be supported include those listed in the subsections of Section 5.3.19.
Error Message Content
This data structure MAY be used by an end entity, CA, or RA to convey error information and by a PKI management entity to initiate delayed delivery of responses.

  ErrorMsgContent ::= SEQUENCE {
     pKIStatusInfo          PKIStatusInfo,
     errorCode              INTEGER           OPTIONAL,
     errorDetails           PKIFreeText       OPTIONAL
  }

This message MAY be generated at any time during a PKI transaction. If the client sends this request, the server MUST respond with a pkiconf response or another error message if any part of the header is not valid.
In case a PKI management entity sends an error message to the end entity with the pKIStatusInfo field containing the status "waiting", the end entity SHOULD initiate polling as described in Section 5.3.22. If the end entity does not initiate polling, both sides MUST treat this message as the end of the transaction (if a transaction is in progress).
If protection is desired on the message, the client MUST protect it using the same technique (i.e., signature or MAC) as the starting message of the transaction. The CA MUST always sign it with a signature key.
Polling Request and Response
This pair of messages is intended to handle scenarios in which the client needs to poll the server to determine the status of an outstanding response (i.e., when the "waiting" PKIStatus has been received).

  PollReqContent ::= SEQUENCE OF SEQUENCE {
     certReqId    INTEGER }

  PollRepContent ::= SEQUENCE OF SEQUENCE {
     certReqId    INTEGER,
     checkAfter   INTEGER,  -- time in seconds
     reason       PKIFreeText OPTIONAL }

Unless implicit confirmation has been requested and granted, in response to an ir, cr, p10cr, kur, krr, or ccr request message, polling is initiated with an ip, cp, kup, krp, or ccp response message containing status "waiting". For any type of request message, polling can be initiated with an error response message with status "waiting". The following clauses describe how polling messages are used. It is assumed that multiple certConf messages can be sent during transactions. There will be one sent in response to each ip, cp, kup, krp, or ccp that contains a CertStatus for an issued certificate.
1. In response to an ip, cp, kup, krp, or ccp message, an end entity will send a certConf for all issued certificates and expect a pkiconf for each certConf. An end entity will send a pollReq message in response to each CertResponse element of an ip, cp, or kup message with status "waiting" and in response to an error message with status "waiting". Its certReqId MUST be either the index of a CertResponse data structure with status "waiting" or -1 referring to the complete response.
2. In response to a pollReq, a CA/RA will return an ip, cp, kup, krp, or ccp if one or more of the still pending requested certificates are ready or the final response to some other type of request is available; otherwise, it will return a pollRep.
3. If the end entity receives a pollRep, it will wait for at least the number of seconds given in the checkAfter field before sending another pollReq.
Note that the checkAfter value heavily depends on the certificate management environment. There are different possible reasons for a delayed delivery of response messages, e.g., high load on the server's backend, offline transfer of messages between two PKI management entities, or required RA operator approval. Therefore, the checkAfter time can vary greatly. This should also be considered by the transfer protocol.
4. If the end entity receives an ip, cp, kup, krp, or ccp, then it will be treated in the same way as the initial response; if it receives any other response, then this will be treated as the final response to the original request.
The following client-side state machine describes polling for individual CertResponse elements at the example of an ir request message.

START

Send

ir

ip

Check

status

of

returned

certs

(issued)

(waiting)

Add

to

Check

CertResponse

Add

to

conf

list

for

each

certificate

pending

list

(empty

conf

list)

(conf

list)

ip

(empty

pending

list)

pollRep

END

Send

certConf

Send

pollReq

Wait

(pending

list)

                            START
                              |
                              v
                           Send ir
                              | ip
                              v
                         Check status
                         of returned <------------------------+
                            certs                             |
                              |                               |
    +------------------------>|<------------------+           |
    |                         |                   |           |
    |        (issued)         v       (waiting)   |           |
  Add to <----------- Check CertResponse ------> Add to       |
 conf list           for each certificate      pending list   |
                             / \                              |
                            /   \  (empty conf list)          |
               (conf list) /     \                            |
                          /       \              ip           |
                         /         \        +-----------------+
   (empty pending list) V           V       |    pollRep
     END <---- Send certConf        Send pollReq---------->Wait
                      |                 ^   ^               |
                      |                 |   |               |
                      +-----------------+   +---------------+
                         (pending list)

In the following exchange, the end entity is enrolling for two certificates in one request.

Step#

End

entity

PKI

1

format

ir

2

ir

3

handle

ir

4

manual

intervention

is

required

for

both

certs

5

ip

6

process

ip

7

format

pollReq

8

pollReq

9

check

status

of

cert

requests,

certificates

not

ready

10

format

pollRep

11

pollRep

12

wait

13

format

pollReq

14

pollReq

15

check

status

of

cert

requests,

one

certificate

is

ready

16

format

ip

17

ip

18

handle

ip

19

format

certConf

20

certConf

21

handle

certConf

22

format

ack

23

pkiconf

24

format

pollReq

25

pollReq

26

check

status

of

certificate,

certificate

is

ready

27

format

ip

28

ip

29

handle

ip

30

format

certConf

31

certConf

32

handle

certConf

33

format

ack

34

pkiconf

Step# End entity                       PKI
---------------------------------------------------------------------
  1   format ir
  2                   --> ir       -->
  3                                    handle ir
  4                                    manual intervention is
                                         required for both certs
  5                   <-- ip       <--
  6   process ip
  7   format pollReq
  8                   --> pollReq  -->
  9                                    check status of cert requests,
                                         certificates not ready
 10                                    format pollRep
 11                   <-- pollRep  <--
 12   wait
 13   format pollReq
 14                   --> pollReq  -->
 15                                    check status of cert requests,
                                         one certificate is ready
 16                                    format ip
 17                   <-- ip       <--
 18   handle ip
 19   format certConf
 20                   --> certConf -->
 21                                    handle certConf
 22                                    format ack
 23                   <-- pkiconf  <--
 24   format pollReq
 25                   --> pollReq  -->
 26                                    check status of certificate,
                                         certificate is ready
 27                                    format ip
 28                   <-- ip       <--
 29   handle ip
 30   format certConf
 31                   --> certConf -->
 32                                    handle certConf
 33                                    format ack
 34                   <-- pkiconf  <--

The following client-side state machine describes polling for a complete response message.

Start

Send

request

Receive

response

ip/cp/kup/krp/ccp/error

with

other

status

"waiting"

response

Polling

Send

pollReq

Receive

response

pollRep

other

response

Handle

response

End

                                Start
                                  |
                                  | Send request
                                  v
             +----------- Receive response ------------+
             |                                         |
             | ip/cp/kup/krp/ccp/error with            | other
             | status "waiting"                        | response
             |                                         |
             v                                         |
 +------> Polling                                      |
 |           |                                         |
 |           | Send pollReq                            |
 |           | Receive response                        |
 |           |                                         |
 |           v                                         |
 +-----------+------------------->+<-------------------+
     pollRep   other response     |
                                  v
                            Handle response
                                  |
                                  v
                                 End

In the following exchange, the end entity is sending a general message request, and the response is delayed by the server.

Step#

End

entity

PKI

1

format

genm

2

genm

3

handle

genm

4

delay

in

response

is

necessary

5

format

error

message

"waiting"

with

certReqId

set

to

-1

6

error

7

process

error

8

format

pollReq

9

pollReq

10

check

status

of

original

request,

general

message

response

not

ready

11

format

pollRep

12

pollRep

13

wait

14

format

pollReq

15

pollReq

16

check

status

of

original

request,

general

message

response

is

ready

17

format

genp

18

genp

19

handle

genp

Step# End entity                       PKI
---------------------------------------------------------------------
  1   format genm
  2                  --> genm    -->
  3                                 handle genm
  4                                 delay in response is necessary
  5                                 format error message "waiting"
                                      with certReqId set to -1
  6                  <-- error   <--
  7   process error
  8   format pollReq
  9                  --> pollReq -->
 10                                 check status of original request,
                                      general message response not
                                      ready
 11                                 format pollRep
 12                  <-- pollRep <--
 13   wait
 14   format pollReq
 15                  --> pollReq -->
 16                                 check status of original request,
                                      general message response is
                                      ready
 17                                 format genp
 18                  <-- genp    <--
 19   handle genp

Mandatory PKI Management Functions
Some of the PKI management functions outlined in Section 3.1 are described in this section.
This section deals with functions that are "mandatory" in the sense that all end entity and CA/RA implementations MUST be able to provide the functionality described. This part is effectively the profile of the PKI management functionality that MUST be supported. Note, however, that the management functions described in this section do not need to be accomplished using the PKI messages defined in Section 5 if alternate means are suitable for a given environment. See Section 7 of [RFC9483] and Appendix C for profiles of the PKIMessage structures that MUST be supported for specific use cases.
Root CA Initialization
[See Section 3.1.1.2 for this document's definition of "root CA".]
If a newly created root CA is at the top of a PKI hierarchy, it usually produces a "self-certificate", which is a certificate structure with the profile defined for the "newWithNew" certificate issued following a root CA key update.
In order to make the CA's self-certificate useful to end entities that do not acquire the self-certificate via "out-of-band" means, the CA must also produce a fingerprint for its certificate. End entities that acquire this fingerprint securely via some "out-of-band" means can then verify the CA's self-certificate and, hence, the other attributes contained therein.
The data structure used to carry the fingerprint may be the OOBCertHash (see Section 5.2.5).
Root CA Key Update
CA keys (as all other keys) have a finite lifetime and will have to be updated on a periodic basis. The certificates NewWithNew, NewWithOld, and OldWithNew (see Section 4.4.1) MAY be issued by the CA to aid existing end entities who hold the current root CA certificate (OldWithOld) to transition securely to the new root CA certificate (NewWithNew) and to aid new end entities who will hold NewWithNew to acquire OldWithOld securely for verification of existing data.
Subordinate CA Initialization
[See Section 3.1.1.2 for this document's definition of "subordinate CA".]
From the perspective of PKI management protocols, the initialization of a subordinate CA is the same as the initialization of an end entity. The only difference is that the subordinate CA must also produce an initial revocation list.
CRL Production
Before issuing any certificates, a newly established CA (which issues CRLs) must produce "empty" versions of each CRL, which are to be periodically produced.
PKI Information Request
When a PKI entity (CA, RA, or end entity) wishes to acquire information about the current status of a CA, it MAY send that CA a request for such information.
The CA MUST respond to the request by providing (at least) all of the information requested by the requester. If some of the information cannot be provided, then an error must be conveyed to the requester.
If PKIMessages are used to request and supply this PKI information, then the request MUST be the GenMsg message, the response MUST be the GenRep message, and the error MUST be the Error message. These messages are protected using a MAC based on shared secret information (e.g., password-based MAC; see "CMP Algorithms") or using any asymmetric authentication means such as a signature (if the end entity has an existing certificate).
Cross-Certification
The requester CA is the CA that will become the subject of the cross-certificate; the responder CA will become the issuer of the cross-certificate.
The requester CA must be "up and running" before initiating the cross-certification operation.
One-Way Request-Response Scheme
The cross-certification scheme is essentially a one-way operation; that is, when successful, this operation results in the creation of one new cross-certificate. If the requirement is that cross-certificates be created in "both directions", then each CA, in turn, must initiate a cross-certification operation (or use another scheme).
This scheme is suitable where the two CAs in question can already verify each other's signatures (they have some common points of trust) or where there is an out-of-band verification of the origin of the certification request.
Detailed Description:
Cross-certification is initiated at one CA known as the responder. The CA administrator for the responder identifies the CA it wants to cross-certify and the responder CA equipment generates an authorization code. The responder CA administrator passes this authorization code by out-of-band means to the requester CA administrator. The requester CA administrator enters the authorization code at the requester CA in order to initiate the online exchange.
The authorization code is used for authentication and integrity purposes. This is done by generating a symmetric key based on the authorization code and using the symmetric key for generating MACs on all messages exchanged. (Authentication may alternatively be done using signatures instead of MACs, if the CAs are able to retrieve and validate the required public keys by some means, such as an out-of-band hash comparison.)
The requester CA initiates the exchange by generating a cross-certification request (ccr) with a fresh random number (requester random number). The requester CA then sends the ccr message to the responder CA. The fields in this message are protected from modification with a MAC based on the authorization code.
Upon receipt of the ccr message, the responder CA validates the message and the MAC, saves the requester random number, and generates its own random number (responder random number). It then generates (and archives, if desired) a new requester certificate that contains the requester CA public key and is signed with the responder CA signature private key. The responder CA responds with the cross-certification response (ccp) message. The fields in this message are protected from modification with a MAC based on the authorization code.
Upon receipt of the ccp message, the requester CA validates the message (including the received random numbers) and the MAC. The requester CA responds with the certConf message. The fields in this message are protected from modification with a MAC based on the authorization code. The requester CA MAY write the requester certificate to the Repository as an aid to later certificate path construction.
Upon receipt of the certConf message, the responder CA validates the message and the MAC and sends back an acknowledgement using the pkiconf message. It MAY also publish the requester certificate as an aid to later path construction.
Notes:
1. The ccr message must contain a "complete" certification request; that is, all fields except the serial number (including, e.g., a BasicConstraints extension) must be specified by the requester CA.
2. The ccp message SHOULD contain the verification certificate of the responder CA; if present, the requester CA must then verify this certificate (for example, via the "out-of-band" mechanism).
(A simpler, non-interactive model of cross-certification may also be envisioned, in which the issuing CA acquires the subject CA's public key from some repository, verifies it via some out-of-band mechanism, and creates and publishes the cross-certificate without the subject CA's explicit involvement. This model may be perfectly legitimate for many environments, but since it does not require any protocol message exchanges, its detailed description is outside the scope of this specification.)
End Entity Initialization
As with CAs, end entities must be initialized. Initialization of end entities requires at least two steps:
- acquisition of PKI information
- out-of-band verification of one root-CA public key
(Other possible steps include the retrieval of trust condition information and/or out-of-band verification of other CA public keys.)
Acquisition of PKI Information
The information REQUIRED is:
- the current root-CA public key
- (if the certifying CA is not a root-CA) the certification path from the root CA to the certifying CA together with appropriate revocation lists
- the algorithms and algorithm parameters that the certifying CA supports for each relevant usage
Additional information could be required (e.g., supported extensions or CA policy information) in order to produce a certification request that will be successful. However, for simplicity, we do not mandate that the end entity acquires this information via the PKI messages. The end result is simply that some certification requests may fail (e.g., if the end entity wants to generate its own encryption key, but the CA doesn't allow that).
The required information MAY be acquired as described in Section 6.5.
Out-of-Band Verification of the Root CA Key
An end entity must securely possess the public key of its root CA. One method to achieve this is to provide the end entity with the CA's self-certificate fingerprint via some secure "out-of-band" means. The end entity can then securely use the CA's self-certificate.
See Section 6.1 for further details.
Certificate Request
An initialized end entity MAY request an additional certificate at any time (for any purpose). This request will be made using the certification request (cr) message. If the end entity already possesses a signing key pair (with a corresponding verification certificate), then this cr message will typically be protected by the entity's digital signature. The CA returns the new certificate (if the request is successful) in a CertRepMessage.
Key Update
When a key pair is due to expire, the relevant end entity MAY request a key update; that is, it MAY request that the CA issue a new certificate for a new key pair (or, in certain circumstances, a new certificate for the same key pair). The request is made using a key update request (kur) message (referred to, in some environments, as a "Certificate Update" operation). If the end entity already possesses a signing key pair (with a corresponding verification certificate), then this message will typically be protected by the entity's digital signature. The CA returns the new certificate (if the request is successful) in a key update response (kup) message, which is syntactically identical to a CertRepMessage.
Version Negotiation
This section defines the version negotiation used to support older protocols between clients and servers.
If a client knows the protocol version(s) supported by the server (e.g., from a previous PKIMessage exchange or via some out-of-band means), then it MUST send a PKIMessage with the highest version supported by both it and the server. If a client does not know what version(s) the server supports, then it MUST send a PKIMessage using the highest version it supports with the following exception: Version cmp2021 SHOULD only be used if cmp2021 syntax is needed for the request being sent or for the expected response.
Note: Using cmp2000 as the default pvno value is done to avoid extra message exchanges for version negotiation and to foster compatibility with cmp2000 implementations. Version cmp2021 syntax is only needed if a message exchange uses EnvelopedData, hashAlg (in CertStatus), POPOPrivKey with agreeMAC, or ckuann with RootCaKeyUpdateContent.
If a server receives a message with a version that it supports, then the version of the response message MUST be the same as the received version. If a server receives a message with a version higher or lower than it supports, then it MUST send back an ErrorMsg with the unsupportedVersion bit set (in the failureInfo field of the pKIStatusInfo). If the received version is higher than the highest supported version, then the version in the error message MUST be the highest version the server supports; if the received version is lower than the lowest supported version, then the version in the error message MUST be the lowest version the server supports.
If a client gets back an ErrorMsgContent with the unsupportedVersion bit set and a version it supports, then it MAY retry the request with that version.
Supporting RFC 2510 Implementations
[RFC2510] did not specify the behavior of implementations receiving versions they did not understand since there was only one version in existence. With the introduction of the revision in [RFC4210], the following versioning behavior is recommended.
Clients Talking to RFC 2510 Servers
If, after sending a message with a pvno value higher than cmp1999, a client receives an ErrorMsgContent with a version of cmp1999, then it MUST abort the current transaction.
If a client receives a non-error PKIMessage with a version of cmp1999, then it MAY decide to continue the transaction (if the transaction hasn't finished) using the semantics described in [RFC2510]. If it does not choose to do so and the transaction is not finished, then it MUST abort the transaction and send an ErrorMsgContent with a version of cmp1999.
Servers Receiving Version cmp1999 PKIMessages
If a server receives a version cmp1999 message, it MAY revert to the behavior described in [RFC2510] and respond with version cmp1999 messages. If it does not choose to do so, then it MUST send back an ErrorMsgContent as described above in Section 7.
Security Considerations
On the Necessity of POP
It is well established that the role of a CA is to verify that the name and public key belong to the end entity prior to issuing a certificate. If an entity holding a private key obtains a certificate containing the corresponding public key issued for a different entity, it can authenticate as the entity named in the certificate. This facilitates masquerading. It is not entirely clear what security guarantees are lost if an end entity is able to obtain a certificate containing a public key that they do not possess the corresponding private key for. There are some scenarios, described as "forwarding attacks" in Appendix A of [Gueneysu], in which this can lead to protocol attacks against a naively implemented sign-then-encrypt protocol, but in general, it merely results in the end entity obtaining a certificate that they cannot use.
POP with a Decryption Key
Some cryptographic considerations are worth explicitly spelling out. In the protocols specified above, when an end entity is required to prove possession of a decryption key, it is effectively challenged to decrypt something (its own certificate). This scheme (and many others!) could be vulnerable to an attack if the possessor of the decryption key in question could be fooled into decrypting an arbitrary challenge and returning the cleartext to an attacker. Although in this specification a number of other failures in security are required in order for this attack to succeed, it is conceivable that some future services (e.g., notary, trusted time) could potentially be vulnerable to such attacks. For this reason, we reiterate the general rule that implementations should be very careful about decrypting arbitrary "ciphertext" and revealing recovered "plaintext" since such a practice can lead to serious security vulnerabilities.
The client MUST return the decrypted values only if they match the expected content type. In an indirect method, the decrypted value MUST be a valid certificate, and in a direct method, the decrypted value MUST be a Rand as defined in Section 5.2.8.3.3.
POP by Exposing the Private Key
Note also that exposing a private key to the CA/RA as a POP technique can carry some security risks (depending upon whether or not the CA/RA can be trusted to handle such material appropriately). Implementers are advised to:
- Exercise caution in selecting and using this particular POP mechanism.
- Only use this POP mechanism if archival of the private key is desired.
- When appropriate, have the user of the application explicitly state that they are willing to trust the CA/RA to have a copy of their private key before proceeding to reveal the private key.
Attack Against DH Key Exchange
A small subgroup attack during a DH key exchange may be carried out as follows. A malicious end entity may deliberately choose DH parameters that enable it to derive (a significant number of bits of) the DH private key of the CA during a key archival or key recovery operation. Armed with this knowledge, the end entity would then be able to retrieve the decryption private key of another unsuspecting end entity, EE2, during EE2's legitimate key archival or key recovery operation with that CA. In order to avoid the possibility of such an attack, two courses of action are available. (1) The CA may generate a fresh DH key pair to be used as a protocol encryption key pair for each end entity with which it interacts. (2) The CA may enter into a key validation protocol (not specified in this document) with each requesting end entity to ensure that the end entity's protocol encryption key pair will not facilitate this attack. Option (1) is clearly simpler (requiring no extra protocol exchanges from either party) and is therefore RECOMMENDED.
Perfect Forward Secrecy
Long-term security typically requires perfect forward secrecy (pfs). When transferring encrypted long-term confidential values such as centrally generated private keys or revocation passphrases, pfs is likely important. Yet, it is not needed for CMP message protection providing integrity and authenticity because transfer of PKI messages is usually completed in very limited time. For the same reason, it is not typically required for the indirect method to provide a POP (Section 5.2.8.3.2) delivering the newly issued certificate in encrypted form.
Encrypted values (Section 5.2.2) are transferred using CMS EnvelopedData [RFC5652], which does not offer pfs. In cases where long-term security is needed, CMP messages SHOULD be transferred over a mechanism that provides pfs, such as TLS with appropriate cipher suites selected.
Private Keys for Certificate Signing and CMP Message Protection
A CA should not reuse its certificate signing key for other purposes, such as protecting CMP responses and TLS connections. This way, exposure to other parts of the system and the number of uses of this particularly critical key are reduced to a minimum.
Entropy of Random Numbers, Key Pairs, and Shared Secret Information
Implementations must generate nonces and private keys from random input. The use of inadequate pseudorandom number generators (PRNGs) to generate cryptographic keys can result in little or no security. An attacker may find it much easier to reproduce the PRNG environment that produced the keys and to search the resulting small set of possibilities than brute-force searching the whole key space. As an example of predictable random numbers, see [CVE-2008-0166]; consequences of low-entropy random numbers are discussed in Mining Your Ps and Qs. The generation of quality random numbers is difficult. ISO/IEC 20543:2019, NIST SP 800-90A Rev.1, BSI AIS 31 V2.0, and other specifications offer valuable guidance in this area.
If shared secret information is generated by a cryptographically secure random number generator (CSRNG), it is safe to assume that the entropy of the shared secret information equals its bit length. If no CSRNG is used, the entropy of shared secret information depends on the details of the generation process and cannot be measured securely after it has been generated. If user-generated passwords are used as shared secret information, their entropy cannot be measured. Passwords generated from user-supplied entropy are typically insufficient for protected delivery of centrally generated keys or trust anchors.
If the entropy of shared secret information protecting the delivery of a centrally generated key pair is known, it should not be less than the security strength of that key pair; if the shared secret information is reused for different key pairs, the security of the shared secret information should exceed the security strength of each individual key pair.
For the case of a PKI management operation that delivers a new trust anchor (e.g., a root CA certificate), using caPubs or genp that is (a) not concluded in a timely manner or (b) where the shared secret information is reused for several key management operations, the entropy of the shared secret information, if known, should not be less than the security strength of the trust anchor being managed by the operation. The shared secret information should have an entropy that at least matches the security strength of the key material being managed by the operation. Certain use cases may require shared secret information that may be of a low security strength, e.g., a human-generated password. It is RECOMMENDED that such secret information be limited to a single PKI management operation.
Importantly for this section, further information about algorithm use profiles and their security strength is available in CMP Algorithms.
Recurring Usage of KEM Keys for Message Protection
For each PKI management operation using MAC-based message protection involving KEM (see Section 5.1.3.4), the KEM Encapsulate() function, providing a fresh KEM ciphertext (ct) and shared secret (ss), MUST be invoked.
It is assumed that the overall data size of the CMP messages in a PKI management operation protected by a single shared secret key is small enough not to introduce extra security risks.
To be appropriate for use with this specification, the KEM algorithm MUST explicitly be designed to be secure when the public key is used many times. For example, a KEM algorithm with a single-use public key is not appropriate because the public key is expected to be carried in a long-lived certificate [RFC5280] and used over and over. Thus, KEM algorithms that offer indistinguishability under adaptive chosen ciphertext attack (IND-CCA2) security are appropriate. A common design pattern for obtaining IND-CCA2 security with public key reuse is to apply the Fujisaki-Okamoto (FO) transform [Fujisaki] or a variant of the FO transform [Hofheinz].
Therefore, given a long-term public key using an IND-CCA2-secure KEM algorithm, there is no limit to the number of CMP messages that can be authenticated using KEM keys for MAC-based message protection.
Trust Anchor Provisioning Using CMP Messages
A provider of trust anchors, which may be an RA involved in configuration management of its clients, MUST NOT include to-be-trusted CA certificates in a CMP message unless the specific deployment scenario can ensure that it is adequate that the receiving end entity trusts these certificates, e.g., by loading them into its trust store.
Whenever an end entity receives in a CMP message a CA certificate to be used as a trust anchor (for example, in the caPubs field of a certificate response or in a general response), it MUST properly authenticate the message sender with existing trust anchors without requiring new trust anchor information included in the message.
Additionally, the end entity MUST verify that the sender is an authorized source of trust anchors. This authorization is governed by local policy and typically indicated using shared secret information or with a signature-based message protection using a certificate issued by a PKI that is explicitly authorized for this purpose.
Authorizing Requests for Certificates with Specific EKUs
When a CA issues a certificate containing EKU extensions as defined in Section 4.5, this expresses delegation of an authorization that originally is only with the CA certificate itself. Such delegation is a very sensitive action in a PKI, and therefore, special care must be taken when approving such certificate requests to ensure that only legitimate entities receive a certificate containing such an EKU.
Usage of CT Logs
CAs that support indirect POP MUST NOT also publish final certificates to CT logs [RFC9162] before having received the certConf message containing the certHash of that certificate to complete the POP. The risk is that a malicious actor could fetch the final certificate from the CT log and use that to spoof a response to the implicit POP challenge via a certConf response. This risk does not apply to CT precertificates, so those are OK to publish.
If a certificate or its precertificate was published in a CT log, it must be revoked if a required certConf message could not be verified, especially when the implicit POP was used.
IANA Considerations
This document updates the ASN.1 modules in CMP Updates. The OID 116 (id-mod-cmp2023-02) was registered in the "SMI Security for PKIX Module Identifier" registry to identify the updated ASN.1 module.
IANA has added the following entry in the "SMI Security for PKIX CMP Information Types" registry within the SMI Numbers registry group (see https://www.iana.org/assignments/smi-numbers) [RFC7299]:
Decimal:
24
Description:
id-it-KemCiphertextInfo
Reference:
RFC 9810
Note that the new OID 1.2.840.113533.7.66.16 was registered by Entrust, and not by IANA, for id-KemBasedMac in the arc 1.2.840.113533.7.66. This was done to match the previous registrations for id-PasswordBasedMac and id-DHBasedMac, which are also on the Entrust private arc.
All existing references to [RFC2510], [RFC4210], and [RFC9480] at https://www.iana.org/assignments/smi-numbers except those in the "SMI Security for PKIX Module Identifier" registry have been replaced with references to this document.
References
Normative References
[MvOV97]

Handbook of Applied Cryptography
A. Menezes
P. van Oorschot
S. Vanstone
1996
CRC Press ISBN 0-8493-8523-7
Informative References
[RFC9811]

Internet X.509 Public Key Infrastructure -- HTTP Transfer for the Certificate Management Protocol (CMP)
Hendrik Brockhaus
Siemens
David von Oheimb
Siemens
Mike Ounsworth
Entrust
John Gray
Entrust
July 2025
RFC 9811
[NIST.SP.800_90Ar1]

Recommendation for Random Number Generation Using Deterministic Random Bit Generators
Elaine B. Barker
Information Technology Laboratory
John M. Kelsey
Information Technology Laboratory
June 2015
NIST SP 800-90Ar1
DOI 10.6028/NIST.SP.800-90Ar1
[IEEE.802.1AR-2018]

IEEE Standard for Local and Metropolitan Area Networks - Secure Device Identity
IEEE
August 2018
IEEE Std 802.1AR-2018
DOI 10.1109/ieeestd.2018.8423794
[CVE-2008-0166]

National Vulnerability Database - CVE-2008-0166
National Institute of Science and Technology (NIST)
May 2008
[MiningPsQs]

Mining Your Ps and Qs: Detection of Widespread Weak Keys in Network Devices
Nadia Heninger
UC San Diego
Zakir Durumeric
University of Michigan
Eric Wustrow
University of Michigan
J. Alex Halderman
University of Michigan
August 2012
21st USENIX Security Symposium (USENIX Security 12)
[X509.2019]

Information technology - Open Systems Interconnection - The Directory: Public-key and attribute certificate frameworks
ITU-T
October 2019
ITU-T Recommendation X.509 (10/2019)
[ISO.20543-2019]

Information technology -- Security techniques -- Test and analysis methods for random bit generators within ISO/IEC 19790 and ISO/IEC 15408
ISO/IEC
October 2019
ISO/IEC 20543:2019
[AIS31]

A proposal for: Functionality classes for random number generators - Version 2.0
Wolfgang Killmann
T-Systems GEI GmbH
Werner Schindler
Federal Office for Information Security (BSI)
September 2011
Federal Office for Information Security (BSI)
[Gueneysu]

Proof-of-possession for KEM certificates using verifiable generation
Tim Gueneysu
Philip Hodges
Georg Land
Mike Ounsworth
Douglas Stebila
Greg Zaverucha
2022
Cryptology ePrint Archive, Paper 2022/703
[Fujisaki]

Secure Integration of Asymmetric and Symmetric Encryption Schemes
Eiichiro Fujisaki
Tatsuaki Okamoto
December 2011
Journal of Cryptology, vol. 26, no. 1, pp. 80-101
DOI 10.1007/s00145-011-9114-1
[Hofheinz]

A Modular Analysis of the Fujisaki-Okamoto Transformation
Dennis Hofheinz
Kathrin Hövelmanns
Eike Kiltz
November 2017
Theory of Cryptography (TCC 2017), Lecture Notes in Computer Science, vol. 10677, pp. 341-371
DOI 10.1007/978-3-319-70500-2_12
[ETSI-3GPP.33.310]

Network Domain Security (NDS); Authentication Framework (AF)
3GPP
December 2020
3GPP TS 33.310 16.6.0
[UNISIG.Subset-137]

ERTMS/ETCS On-line Key Management FFFIS
UNISIG
December 2015
Subset-137, V1.0.0
[RFC5280]
[RFC4210]
[RFC2510]
[RFC6712]
[RFC9480]
[RFC9481]
[RFC9483]
[RFC5652]
[RFC4211]
[RFC2119]
[RFC8174]
[RFC9162]
[RFC8995]
[RFC8572]
[RFC4511]
[RFC2585]
[RFC9482]
[RFC8446]
[RFC9147]
[RFC7296]
[RFC4303]
[RFC9733]
[RFC9629]
[RFC8649]
[RFC6402]
[RFC5646]
[RFC1847]
[RFC9045]
[I-D.ietf-lamps-kyber-certificates]
[RFC4212]
[RFC5958]
[RFC8933]
[RFC2986]
[RFC5480]
[RFC7299]
[RFC2985]
[RFC5912]
[RFC6268]
[RFC3629]
Reasons for the Presence of RAs
The reasons that justify the presence of an RA can be split into those that are due to technical factors and those that are organizational in nature. Technical reasons include the following.
- If hardware tokens are in use, then not all end entities will have the equipment needed to initialize these; the RA equipment can include the necessary functionality (this may also be a matter of policy).
- Some end entities may not have the capability to publish certificates; again, the RA may be suitably placed for this.
- The RA will be able to issue signed revocation requests on behalf of end entities associated with it, whereas the end entity may not be able to do this (if the key pair is completely lost).
Some of the organizational reasons that argue for the presence of an RA are the following.
- It may be more cost effective to concentrate functionality in the RA equipment than to supply functionality to all end entities (especially if special token initialization equipment is to be used).
- Establishing RAs within an organization can reduce the number of CAs required, which is sometimes desirable.
- RAs may be better placed to identify people with their "electronic" names, especially if the CA is physically remote from the end entity.
- For many applications, there will already be some administrative structure in place so that candidates for the role of RA are easy to find (which may not be true of the CA).
Further reasons relevant for automated machine-to-machine certificate lifecycle management are available in the Lightweight CMP Profile [RFC9483].
The Use of Revocation Passphrase
A revocation request must incorporate suitable security mechanisms, including proper authentication, in order to reduce the probability of successful denial-of-service attacks. A digital signature or DH/KEM-based message protection on the request -- REQUIRED to support within this specification depending on the key type used if revocation requests are supported -- can provide the authentication required, but there are circumstances under which an alternative mechanism may be desirable (e.g., when the private key is no longer accessible and the entity wishes to request a revocation prior to re-certification of another key pair). In order to accommodate such circumstances, a password-based MAC (see CMP Algorithms) on the request is also REQUIRED to support within this specification (subject to local security policy for a given environment) if revocation requests are supported and if shared secret information can be established between the requester and the responder prior to the need for revocation.
A mechanism that has seen use in some environments is "revocation passphrase", in which a value of sufficient entropy (i.e., a relatively long passphrase rather than a short password) is shared between (only) the entity and the CA/RA at some point prior to revocation; this value is later used to authenticate the revocation request.
In this specification, the following technique to establish shared secret information (i.e., a revocation passphrase) is OPTIONAL to support. Its precise use in CMP messages is as follows.
- The OID and value specified in Section 5.3.19.9 MAY be sent in a GenMsg message at any time or MAY be sent in the generalInfo field of the PKIHeader of any PKIMessage at any time. (In particular, the EncryptedKey structure as described in Section 5.2.2 may be sent in the header of the certConf message that confirms acceptance of certificates requested in an initialization request or certificate request message.) This conveys a revocation passphrase chosen by the entity to the relevant CA/RA. When EnvelopedData is used, this is in the decrypted bytes of the encryptedContent field. When EncryptedValue is used, this is in the decrypted bytes of the encValue field. Furthermore, the transfer is accomplished with appropriate confidentiality characteristics.
- If a CA/RA receives the revocation passphrase (OID and value specified in Section 5.3.19.9) in a GenMsg, it MUST construct and send a GenRep message that includes the OID (with absent value) specified in Section 5.3.19.9. If the CA/RA receives the revocation passphrase in the generalInfo field of a PKIHeader of any PKIMessage, it MUST include the OID (with absent value) in the generalInfo field of the PKIHeader of the corresponding response PKIMessage. If the CA/RA is unable to return the appropriate response message for any reason, it MUST send an error message with a status of "rejection" and, optionally, a failInfo reason set.
- Either the localKeyId attribute of EnvelopedData as specified in [RFC2985] or the valueHint field of EncryptedValue MAY contain a key identifier (chosen by the entity, along with the passphrase itself) to assist in later retrieval of the correct passphrase (e.g., when the revocation request is constructed by the end entity and received by the CA/RA).
- The revocation request message is protected by a password-based MAC (see "CMP Algorithms") with the revocation passphrase as the key. If appropriate, the senderKID field in the PKIHeader MAY contain the value previously transmitted in localKeyId or valueHint.
Note: For a message transferring a revocation passphrase indicating cmp2021(3) in the pvno field of the PKIHeader, the encrypted passphrase MUST be transferred in the envelopedData choice of EncryptedKey as defined in Section 5.2.2. When using cmp2000(2) in the message header for backward compatibility, the encryptedValue is used. This allows the necessary conveyance and protection of the passphrase while maintaining bits-on-the-wire compatibility with [RFC4210]. The encryptedValue choice has been deprecated in favor of encryptedData.
Using the technique specified above, the revocation passphrase may be initially established and updated at any time without requiring extra messages or out-of-band exchanges. For example, the revocation request message itself (protected and authenticated through a MAC that uses the revocation passphrase as a key) may contain, in the PKIHeader, a new revocation passphrase to be used for authenticating future revocation requests for any of the entity's other certificates. In some environments, this may be preferable to mechanisms that reveal the passphrase in the revocation request message, since this can allow a denial-of-service attack in which the revealed passphrase is used by an unauthorized third party to authenticate revocation requests on the entity's other certificates. However, because the passphrase is not revealed in the request message, there is no requirement that the passphrase must always be updated when a revocation request is made (that is, the same passphrase MAY be used by an entity to authenticate revocation requests for different certificates at different times).
Furthermore, the above technique can provide strong cryptographic protection over the entire revocation request message even when a digital signature is not used. Techniques that do authentication of the revocation request by simply revealing the revocation passphrase typically do not provide cryptographic protection over the fields of the request message (so that a request for revocation of one certificate may be modified by an unauthorized third party to a request for revocation of another certificate for that entity).
PKI Management Message Profiles (REQUIRED)
This appendix contains detailed profiles for those PKIMessages that MUST be supported by conforming implementations (see Section 6).
Note: Appendices C and D focus on PKI management operations managing certificates for human end entities. In contrast, the Lightweight CMP Profile [RFC9483] focuses on typical use cases of industrial and IoT scenarios supporting highly automated certificate lifecycle management scenarios.
Profiles for the PKIMessages used in the following PKI management operations are provided:
- initial registration/certification
- basic authenticated scheme
- certificate request
- key update
General Rules for Interpretation of These Profiles
1. Where OPTIONAL or DEFAULT fields are not mentioned in individual profiles, they SHOULD be absent from the relevant message (i.e., a receiver can validly reject a message containing such fields as being syntactically incorrect). Mandatory fields are not mentioned if they have an obvious value. The protocol version number MUST be set as specified in Section 7).
2. Where structures occur in more than one message, they are separately profiled as appropriate.
3. The algorithmIdentifiers from PKIMessage structures are profiled separately.
4. A "special" X.500 DN is called the "NULL-DN"; this means a DN containing a zero-length SEQUENCE OF RelativeDistinguishedNames (its DER encoding is then '3000'H).
5. Where a GeneralName is required for a field, but no suitable value is available (e.g., an end entity produces a request before knowing its name), then the GeneralName is to be an X.500 NULL-DN (i.e., the Name field of the CHOICE is to contain a NULL-DN).
6. Where a profile omits to specify the value for a GeneralName, then the NULL-DN value is to be present in the relevant PKIMessage field. This occurs with the sender field of the PKIHeader for some messages.
7. Where any ambiguity arises due to naming of fields, the profile names these using a "dot" notation (e.g., "certTemplate.subject" means the subject field within a field called certTemplate).
8. Where a "SEQUENCE OF types" is part of a message, a zero-based array notation is used to describe fields within the SEQUENCE OF (e.g., crm[0].certReq.certTemplate.subject refers to a subfield of the first CertReqMsg contained in a request message).
9. All PKI message exchanges in Appendices C.4 to C.6 require a certConf message to be sent by the initiating entity and a pkiconf message to be sent by the responding entity. The pkiconf is not included in some of the profiles given since its body is NULL and its header contents are clear from the context. Any authenticated means can be used for the protectionAlg (e.g., password-based MAC, if shared secret information is known, or signature).
Algorithm Use Profile
For specifications of algorithm identifiers and respective conventions for conforming implementations, please refer to CMP Algorithms.
POP Profile
The table below describes the POP fields for use (in signature field of pop field of ProofOfPossession structure) when proving possession of a private signing key that corresponds to a public verification key for which a certificate has been requested.
Field | Value | Comment
algorithmIdentifier | MSG_SIG_ALG | only signature protection is allowed for this proof
signature | present | bits calculated using MSG_SIG_ALG
Note: For examples of MSG_SIG_ALG OIDs, see CMP Algorithms.
POP of a private decryption key that corresponds to a public encryption key for which a certificate has been requested does not use this profile; the CertHash field of the certConf message is used instead.
Not every CA/RA will do POP (of signing key, decryption key, or key agreement key) in the PKIX-CMP in-band certification request protocol (how POP is done MAY ultimately be a policy issue that is made explicit for any given CA in its publicized Policy OID and Certification Practice Statement). However, this specification mandates that CA/RA entities MUST do POP (by some means) as part of the certification process. All end entities MUST be prepared to provide POP (i.e., these components of the PKIX-CMP protocol MUST be supported).
Initial Registration/Certification (Basic Authenticated Scheme)
An (uninitialized) end entity requests a (first) certificate from a CA. When the CA responds with a message containing a certificate, the end entity replies with a certificate confirmation. The CA sends a pkiconf message back, closing the transaction. All messages are authenticated.
This scheme allows the end entity to request certification of a locally generated public key (typically a signature key). The end entity MAY also choose to request the centralized generation and certification of another key pair (typically an encryption key pair).
Certification may only be requested for one locally generated public key (for more, use separate PKIMessages).
The end entity MUST support POP of the private key associated with the locally generated public key.
Preconditions:
1. The end entity can authenticate the CA's signature based on out-of-band means.
2. The end entity and the CA share a symmetric MACing key.
Message Flow:

Step#

End

entity

PKI

1

format

ir

2

ir

3

handle

ir

4

format

ip

5

ip

6

handle

ip

7

format

certConf

8

certConf

9

handle

certConf

10

format

pkiconf

11

pkiconf

12

handle

pkiconf

Step# End entity                           PKI
---------------------------------------------------------------------
  1   format ir
  2                     -->   ir      -->
  3                                        handle ir
  4                                        format ip
  5                     <--   ip      <--
  6   handle ip
  7   format certConf
  8                     -->  certConf -->
  9                                        handle certConf
 10                                        format pkiconf
 11                     <--  pkiconf  <--
 12   handle pkiconf

For this profile, we mandate that the end entity MUST include all (i.e., one or two) CertReqMsg in a single PKIMessage and that the PKI (CA) MUST produce a single response PKIMessage that contains the complete response (i.e., including the OPTIONAL second key pair, if it was requested and if centralized key generation is supported). For simplicity, we also mandate that this message MUST be the final one (i.e., no use of "waiting" status value).
The end entity has an out-of-band interaction with the CA/RA. This transaction established the shared secret, the referenceNumber, and optionally the DN used for both the sender and subject name in the certificate template. See Section 8.7 for security considerations on quality of shared secret information.
Initialization Request -- ir

Field                Value

recipient            CA name
  -- the name of the CA who is being asked to produce a certificate
protectionAlg        MSG_MAC_ALG
  -- only MAC protection is allowed for this request, based
  -- on initial authentication key
senderKID            referenceNum
  -- the reference number that the CA has previously issued
  -- to the end entity (together with the MACing key)
transactionID        present
  -- implementation-specific value, meaningful to end
  -- entity.
  -- [If already in use at the CA, then a rejection message MUST
  -- be produced by the CA]

senderNonce          present
  -- 128 (pseudo-)random bits
freeText             any valid value
body                 ir (CertReqMessages)
                     only one or two CertReqMsg
                     are allowed
  -- if more certificates are required, requests MUST be
  -- packaged in separate PKIMessages

CertReqMsg           one or two present
  -- see below for details, note: crm[0] means the first
  -- (which MUST be present), crm[1] means the second (which
  -- is OPTIONAL, and used to ask for a centrally generated key)

crm[0].certReq.      fixed value of zero
   certReqId
  -- this is the index of the template within the message
crm[0].certReq       present
   certTemplate
  -- MUST include subject public key value, otherwise unconstrained
crm[0].pop...        optionally present if public key
   POPOSigningKey    from crm[0].certReq.certTemplate is
                     a signing key
  -- POP MAY be required in this exchange
  -- (see Appendix D.3 for details)
crm[0].certReq.      optionally present
   controls.archiveOptions
  -- the end entity MAY request that the locally generated
  -- private key be archived

crm[0].certReq.      optionally present
   controls.publicationInfo
  -- the end entity MAY ask for publication of resulting cert.

crm[1].certReq       fixed value of one
      certReqId
     -- the index of the template within the message
   crm[1].certReq       present
      certTemplate
      -- MUST NOT include actual public key bits, otherwise
      -- unconstrained (e.g., the names need not be the same as in
      -- crm[0]).  Note that subjectPublicKeyInfo MAY be present
      -- and contain an AlgorithmIdentifier followed by a
      -- zero-length BIT STRING for the subjectPublicKey if it is
      -- desired to inform the CA/RA of algorithm and parameter
      -- preferences regarding the to-be-generated key pair.

   crm[1].certReq.      present [object identifier MUST be
                                 PROT_ENC_ALG]

      controls.protocolEncrKey
     -- if centralized key generation is supported by this CA,
     -- this short-term asymmetric encryption key (generated by
     -- the end entity) will be used by the CA to encrypt (a
     -- symmetric key used to encrypt) a private key generated by
     -- the CA on behalf of the end entity

crm[1].certReq.      optionally present
   controls.archiveOptions
crm[1].certReq.      optionally present
   controls.publicationInfo
protection           present
  -- bits calculated using MSG_MAC_ALG

Initialization Response -- ip

Field                Value

sender               CA name
  -- the name of the CA who produced the message
messageTime          present
  -- time at which CA produced message
protectionAlg        MSG_MAC_ALG
  -- only MAC protection is allowed for this response
senderKID             referenceNum
  -- the reference number that the CA has previously issued to the
  -- end entity (together with the MACing key)
transactionID        present
  -- value from corresponding ir message
senderNonce          present
  -- 128 (pseudo-)random bits
recipNonce           present
  -- value from senderNonce in corresponding ir message
freeText             any valid value
body                 ip (CertRepMessage)
                     contains exactly one response
                     for each request
  -- The PKI (CA) responds to either one or two requests as
  -- appropriate.  crc[0] denotes the first (always present);
  -- crc[1] denotes the second (only present if the ir message
  -- contained two requests and if the CA supports centralized
  -- key generation).
crc[0].              fixed value of zero
   certReqId
  -- MUST contain the response to the first request in the
  -- corresponding ir message
crc[0].status.       present, positive values allowed:
   status               "accepted", "grantedWithMods"
                     negative values allowed:
                        "rejection"
crc[0].status.       present if and only if
   failInfo          crc[0].status.status is "rejection"
crc[0].              present if and only if
   certifiedKeyPair  crc[0].status.status is
                        "accepted" or "grantedWithMods"
certificate          present unless end entity's public
                     key is an encryption key and POP
                     is done in this in-band exchange
encryptedCert        present if and only if end entity's
                     public key is an encryption key and
                     POP done in this in-band exchange
publicationInfo      optionally present

  -- indicates where certificate has been published (present
  -- at discretion of CA)

crc[1].              fixed value of one
   certReqId
  -- MUST contain the response to the second request in the
  -- corresponding ir message
crc[1].status.       present, positive values allowed:
   status               "accepted", "grantedWithMods"
                     negative values allowed:
                        "rejection"
crc[1].status.       present if and only if
   failInfo          crc[0].status.status is "rejection"
crc[1].              present if and only if
   certifiedKeyPair  crc[0].status.status is "accepted"
                     or "grantedWithMods"
certificate          present
privateKey           present
  -- Use EnvelopedData; if backward compatibility is required,
  -- use EncryptedValue, see Section 5.2.2
publicationInfo      optionally present
  -- indicates where certificate has been published (present
  -- at discretion of CA)

protection           present
  -- bits calculated using MSG_MAC_ALG
extraCerts           optionally present
  -- the CA MAY provide additional certificates to the end
  -- entity

Certificate confirm -- certConf

Field                Value

sender               present
  -- same as in ir
recipient            CA name
  -- the name of the CA who was asked to produce a certificate
transactionID        present
  -- value from corresponding ir and ip messages
senderNonce          present
  -- 128 (pseudo-)random bits
recipNonce           present
  -- value from senderNonce in corresponding ip message
protectionAlg        MSG_MAC_ALG
  -- only MAC protection is allowed for this message.  The
  -- MAC is based on the initial authentication key shared
  -- between the end entity and the CA.

senderKID            referenceNum
  -- the reference number that the CA has previously issued
  -- to the end entity (together with the MACing key)

body                 certConf
  -- see Section 5.3.18, "PKI Confirmation Content", for the
  -- contents of the certConf fields.
  -- Note: two CertStatus structures are required if both an
  -- encryption and a signing certificate were sent.

protection           present
  -- bits calculated using MSG_MAC_ALG

Confirmation -- pkiconf

Field                Value

sender               present
  -- same as in ip
recipient            present
  -- sender name from certConf
transactionID        present
  -- value from certConf message
senderNonce          present
  -- 128 (pseudo-)random bits
recipNonce           present
  -- value from senderNonce from certConf message
protectionAlg        MSG_MAC_ALG
  -- only MAC protection is allowed for this message.
senderKID            referenceNum
body                 pkiconf
protection           present
  -- bits calculated using MSG_MAC_ALG

Certificate Request
An (initialized) end entity requests a certificate from a CA (for any reason). When the CA responds with a message containing a certificate, the end entity replies with a certificate confirmation. The CA replies with a pkiconf message to close the transaction. All messages are authenticated.
The profile for this exchange is identical to that given in Appendix C.4, with the following exceptions:
- sender name SHOULD be present;
- protectionAlg of MSG_SIG_ALG MUST be supported (MSG_MAC_ALG MAY also be supported) in request, response, certConf, and pkiconf messages;
- senderKID and recipKID are only present if required for message verification;
- body is cr or cp;
- body may contain one or two CertReqMsg structures, but either CertReqMsg may be used to request certification of a locally generated public key or a centrally generated public key (i.e., the position-dependence requirement of Appendix C.4 is removed); and
- protection bits are calculated according to the protectionAlg field.
Key Update Request
An (initialized) end entity requests a certificate from a CA (to update the key pair and/or corresponding certificate that it already possesses). When the CA responds with a message containing a certificate, the end entity replies with a certificate confirmation. The CA replies with a PKIConfirm to close the transaction. All messages are authenticated.
The profile for this exchange is identical to that given in Appendix C.4, with the following exceptions:
- sender name SHOULD be present;
- protectionAlg of MSG_SIG_ALG MUST be supported (MSG_MAC_ALG MAY also be supported) in request, response, certConfirm, and PKIConfirm messages;
- senderKID and recipKID are only present if required for message verification;
- body is kur or kup;
- body may contain one or two CertReqMsg structures, but either CertReqMsg may be used to request certification of a locally generated public key or a centrally generated public key (i.e.,the position-dependence requirement of Appendix C.4 is removed);
- protection bits are calculated according to the protectionAlg field; and
- regCtrl OldCertId SHOULD be used (unless it is clear to both the sender and receiver -- by means not specified in this document -- that it is not needed).
PKI Management Message Profiles (OPTIONAL)
This appendix contains detailed profiles for those PKIMessages that MAY be supported by implementations.
Profiles for the PKIMessages used in the following PKI management operations are provided:
- root CA key update
- information request/response
- cross-certification request/response (1-way)
- in-band initialization using external identity certificate
Future versions of this document may extend the above to include profiles for the operations listed below (along with other operations, if desired).
- revocation request
- certificate publication
- CRL publication
General Rules for Interpretation of These Profiles
Identical to Appendix C.1.
Algorithm Use Profile
Identical to Appendix C.2.
Self-Signed Certificates
The table below is a profile of how a certificate structure may be "self-signed". These structures are used for distribution of new root CA public keys. This can occur in one of three ways (see Section 4.4 above for a description of the use of these structures):
Type | Function
newWithNew | a "self-signed" certificate; the contained public key MUST be usable to verify the signature (though this provides only integrity and no authentication whatsoever)
oldWithNew | previous root CA public key signed with new private key
newWithOld | new root CA public key signed with previous private key
A newWithNew certificate (including relevant extensions) must contain "sensible" values for all fields. For example, when present, subjectAltName MUST be identical to issuerAltName, and, when present, keyIdentifiers must contain appropriate values, et cetera.
Root CA Key Update
A root CA updates its key pair. It then produces a CA key update announcement message that can be made available (via some transport mechanism) to the relevant entities. A confirmation message is not required from the end entities.
ckuann message:
Field | Value | Comment
sender | CA name CA name |
body | ckuann(RootCaKeyUpdateContent) |
newWithNew | optionally present | see Appendix D.3 above
newWithOld | optionally present | see Appendix D.3 above
oldWithNew | optionally present | see Appendix D.3 above
extraCerts | optionally present | can be used to "publish" certificates (e.g., certificates signed using the new private key)
PKI Information Request/Response
The end entity sends a general message to the PKI requesting details that will be required for later PKI management operations. The RA/CA responds with a general response. If an RA generates the response, then it will simply forward the equivalent message that it previously received from the CA, with the possible addition of certificates to the extraCerts fields of the PKIMessage. A confirmation message is not required from the end entity.
Message Flows:

Step#

End

entity

PKI

1

format

genm

2

genm

3

handle

genm

4

produce

genp

5

genp

6

handle

genp

Step# End entity                        PKI
---------------------------------------------------------------------
  1   format genm
  2                -->   genm   -->
  3                                     handle genm
  4                                     produce genp
  5                <--   genp   <--
  6   handle genp

genM:

Field               Value

recipient           CA name
  -- the name of the CA as contained in issuerAltName
  -- extensions or issuer fields within certificates
protectionAlg       MSG_MAC_ALG or MSG_SIG_ALG
  -- any authenticated protection alg.
SenderKID           present if required
  -- must be present if required for verification of message
  -- protection
freeText            any valid value
body                genr (GenReqContent)
GenMsgContent       empty SEQUENCE
  -- all relevant information requested
protection          present
  -- bits calculated using MSG_MAC_ALG or MSG_SIG_ALG

genP:

Field                Value

sender               CA name
  -- name of the CA that produced the message
protectionAlg        MSG_MAC_ALG or MSG_SIG_ALG
  -- any authenticated protection alg.
senderKID            present if required
  -- must be present if required for verification of message
  -- protection
body                 genp (GenRepContent)
CAProtEncCert        present (object identifier one
                     of PROT_ENC_ALG), with relevant
                     value
  -- to be used if end entity needs to encrypt information for
  -- the CA (e.g., private key for recovery purposes)

SignKeyPairTypes     present, with relevant value
  -- the set of signature algorithm identifiers that this CA will
  -- certify for subject public keys
EncKeyPairTypes      present, with relevant value
  -- the set of encryption / key agreement algorithm identifiers that
  -- this CA will certify for subject public keys
PreferredSymmAlg     present (object identifier one
                     of PROT_SYM_ALG) , with relevant
                     value
  -- the symmetric algorithm that this CA expects to be used
  -- in later PKI messages (for encryption)
RootCaKeyUpdate      optionally present, with
                     relevant value
  -- Use RootCaKeyUpdate; if backward compatibility with cmp2000 is
  -- required, use CAKeyUpdateInfo.
  -- The CA MAY provide information about a relevant root CA
  -- key pair using this field (note that this does not imply
  -- that the responding CA is the root CA in question)
CurrentCRL           optionally present, with relevant value
  -- the CA MAY provide a copy of a complete CRL (i.e.,
  -- fullest possible one)
protection           present
  -- bits calculated using MSG_MAC_ALG or MSG_SIG_ALG
extraCerts           optionally present
  -- can be used to send some certificates to the end
  -- entity. An RA MAY add its certificate here.

Cross-Certification Request/Response (1-way)
This section describes the creation of a single cross-certificate (i.e., not two at once). The requesting CA MAY choose who is responsible for publication of the cross-certificate created by the responding CA through use of the PKIPublicationInfo control.
Preconditions:
1. Responding CA can verify the origin of the request (possibly requiring out-of-band means) before processing the request.
2. Requesting CA can authenticate the authenticity of the origin of the response (possibly requiring out-of-band means) before processing the response.
The use of certificate confirmation and the corresponding server confirmation is determined by the generalInfo field in the PKIHeader (see Section 5.1.1). The following profile does not mandate support for either confirmation.
Message Flows:

Step#

Requesting

CA

Responding

CA

1

format

ccr

2

ccr

3

handle

ccr

4

produce

ccp

5

ccp

6

handle

ccp

Step# Requesting CA                       Responding CA
---------------------------------------------------------------------
  1   format ccr
  2                  -->    ccr    -->
  3                                       handle ccr
  4                                       produce ccp
  5                  <--    ccp    <--
  6   handle ccp

ccr:

Field                 Value

sender                Requesting CA name
  -- the name of the CA who produced the message
recipient             Responding CA name
  -- the name of the CA who is being asked to produce a certificate
messageTime           time of production of message
  -- current time at requesting CA
protectionAlg         MSG_SIG_ALG
  -- only signature protection is allowed for this request
senderKID             present if required
  -- must be present if required for verification of message
  -- protection
recipKID             present if required
  -- must be present if required for verification of message
  -- protection
transactionID         present
  -- implementation-specific value, meaningful to requesting CA.
  -- [If already in use at responding CA, then a rejection message
  -- MUST be produced by responding CA]
senderNonce           present
  -- 128 (pseudo-)random bits
freeText              any valid value
body                  ccr (CertReqMessages)
                      only one CertReqMsg
                      allowed
  -- if multiple cross-certificates are required, they MUST be
  -- packaged in separate PKIMessages
certTemplate          present
  -- details follow
version               v1 or v3
  -- v3 STRONGLY RECOMMENDED
signingAlg            present
  -- the requesting CA must know in advance with which algorithm it
  -- wishes the certificate to be signed

subject               present
  -- may be NULL-DN only if subjectAltNames extension value proposed
validity              present
  -- MUST be completely specified (i.e., both fields present)
issuer                present
  -- may be NULL-DN only if issuerAltNames extension value proposed
publicKey             present
  -- the key to be certified (which must be for a signing algorithm)
extensions            optionally present
  -- a requesting CA must propose values for all extensions
  -- that it requires to be in the cross-certificate
POPOSigningKey        present
  -- see Appendix C.3: POP Profile
protection            present
  -- bits calculated using MSG_SIG_ALG
extraCerts            optionally present
  -- MAY contain any additional certificates that requester wishes
  -- to include

ccp:

Field                 Value

sender                Responding CA name
  -- the name of the CA who produced the message
recipient             Requesting CA name
  -- the name of the CA who asked for production of a certificate
messageTime           time of production of message
  -- current time at responding CA
protectionAlg         MSG_SIG_ALG
  -- only signature protection is allowed for this message
senderKID             present if required
  -- must be present if required for verification of message
  -- protection
recipKID              present if required
transactionID         present
  -- value from corresponding ccr message
senderNonce           present
  -- 128 (pseudo-)random bits
recipNonce            present
-- senderNonce from corresponding ccr message
freeText              any valid value
body                  ccp (CertRepMessage)
                      only one CertResponse allowed
  -- if multiple cross-certificates are required, they MUST be
  -- packaged in separate PKIMessages
response              present
status                present

PKIStatusInfo.status  present
  -- if PKIStatusInfo.status is one of:
  --   accepted, or
  --   grantedWithMods,
  -- then certifiedKeyPair MUST be present and failInfo MUST
  -- be absent

failInfo              present depending on
                      PKIStatusInfo.status
  -- if PKIStatusInfo.status is:
  --   rejection,
  -- then certifiedKeyPair MUST be absent and failInfo MUST be
  -- present and contain appropriate bit settings

certifiedKeyPair      present depending on
                      PKIStatusInfo.status
certificate           present depending on
                      certifiedKeyPair
  -- content of actual certificate must be examined by requesting CA
  -- before publication
protection            present
  -- bits calculated using MSG_SIG_ALG
extraCerts            optionally present
  -- MAY contain any additional certificates that responder wishes
  -- to include

In-Band Initialization Using External Identity Certificate
An (uninitialized) end entity wishes to initialize into the PKI with a CA, CA-1. It uses, for authentication purposes, a pre-existing identity certificate issued by another (external) CA, CA-X. A trust relationship must already have been established between CA-1 and CA-X so that CA-1 can validate the end entity identity certificate signed by CA-X. Furthermore, some mechanism must already have been established within the TEE, also known as PSE, of the end entity that would allow it to authenticate and verify PKIMessages signed by CA-1 (as one example, the TEE may contain a certificate issued for the public key of CA-1, signed by another CA that the end entity trusts on the basis of out-of-band authentication techniques).
The end entity sends an initialization request to start the transaction. When CA-1 responds with a message containing the new certificate, the end entity replies with a certificate confirmation. CA-1 replies with a pkiconf message to close the transaction. All messages are signed (the end entity messages are signed using the private key that corresponds to the public key in its external identity certificate; the CA-1 messages are signed using the private key that corresponds to the public key in a certificate that can be chained to a trust anchor in the end entity's TEE).
The profile for this exchange is identical to that given in Appendix C.4, with the following exceptions:
- the end entity and CA-1 do not share a symmetric MACing key (i.e., there is no out-of-band shared secret information between these entities);
- sender name in ir MUST be present (and identical to the subject name present in the external identity certificate);
- protectionAlg of MSG_SIG_ALG MUST be used in all messages;
- external identity certificate MUST be carried in ir extraCerts field
- senderKID and recipKID are not used;
- body is ir or ip; and
- protection bits are calculated according to the protectionAlg field.
Variants of Using KEM Keys for PKI Message Protection
As described in Section 5.1.3.4, any party in a PKI management operation may wish to use a KEM key pair for message protection. Possible cases are described below.
For any PKI management operation started by a PKI entity with any type of request message, the following message flows describe the use of a KEM key. There are two cases to distinguish, namely whether the PKI entity or the PKI management entity owns a KEM key pair. If both sides own KEM key pairs, the flows need to be combined such that for each direction a shared secret key is established.
In the following message flows, Alice indicates the PKI entity that uses a KEM key pair for message authentication and Bob provides the KEM ciphertext using Alice's public KEM key, as described in Section 5.1.3.4.
Message Flow When the PKI Entity Has a KEM Key Pair and Certificate

Step#

PKI

entity

PKI

management

entity

(Alice)

(Bob)

1

format

unprotected

genm

of

type

KemCiphertextInfo

without

value,

and

KEM

certificate

in

extraCerts

2

genm

3

validate

KEM

certificate

4

perform

KEM

Encapsulate

5

format

unprotected

genp

of

type

KemCiphertextInfo

providing

KEM

ciphertext

6

genp

7

perform

KEM

Decapsulate

8

perform

key

derivation

to

get

ssk

9

format

request

with

MAC-based

protection

10

request

11

perform

key

derivation

to

get

ssk

12

verify

MAC-based

protection

PKI

entity

authenticated

by

PKI

management

entity

13

format

response

with

protection

depending

on

available

key

material

14

response

15

verify

protection

provided

by

the

PKI

management

entity

16

Further

messages

of

this

PKI

management

operation

can

be

exchanged

with

MAC-based

protection

by

the

PKI

entity

using

the

established

shared

secret

key

(ssk)

Step# PKI entity                           PKI management entity
      (Alice)                              (Bob)
---------------------------------------------------------------------
  1   format unprotected genm
        of type
        KemCiphertextInfo
        without value, and
        KEM certificate in
        extraCerts
  2                     -->   genm    -->
  3                                        validate KEM certificate
  4                                        perform KEM Encapsulate
  5                                        format unprotected genp
                                             of type
                                             KemCiphertextInfo
                                             providing KEM ciphertext
  6                     <--   genp    <--
  7   perform KEM Decapsulate
  8   perform key derivation
        to get ssk
  9   format request with
        MAC-based protection
 10                     -->  request  -->
 11                                        perform key derivation
                                             to get ssk
 12                                        verify MAC-based
                                             protection

--------  PKI entity authenticated by PKI management entity  --------

 13                                        format response with
                                             protection depending on
                                             available key material
 14                     <-- response  <--
 15   verify protection
        provided by the
        PKI management entity

 16       Further messages of this PKI management operation
        can be exchanged with MAC-based protection by the PKI
         entity using the established shared secret key (ssk)

Message Flow When the PKI Entity Knows That the PKI Management Entity Uses a KEM Key Pair and Has the Authentic Public Key

Step#

PKI

entity

PKI

management

entity

(Bob)

(Alice)

1

perform

KEM

Encapsulate

2

format

request

providing

KEM

ciphertext

in

generalInfo

of

type

KemCiphertextInfo,

and

with

protection

depending

on

available

key

material

3

request

4

perform

KEM

Decapsulate

5

perform

key

derivation

to

get

ssk

6

format

response

with

MAC-based

protection

7

response

8

perform

key

derivation

to

get

ssk

9

verify

MAC-based

protection

PKI

management

entity

authenticated

by

PKI

entity

10

Further

messages

of

this

PKI

management

operation

can

be

exchanged

with

MAC-based

protection

by

the

PKI

management

entity

using

the

established

shared

secret

key

(ssk)

Step# PKI entity                           PKI management entity
      (Bob)                                (Alice)
---------------------------------------------------------------------
  1   perform KEM Encapsulate
  2   format request providing
        KEM ciphertext in
        generalInfo of type
        KemCiphertextInfo,
        and with protection
        depending on available
        key material
  3                     -->  request  -->
  4                                        perform KEM Decapsulate
  5                                        perform key derivation
                                             to get ssk
  6                                        format response with
                                             MAC-based protection
  7                     <-- response  <--
  8   perform key derivation
        to get ssk
  9   verify MAC-based
        protection

--------  PKI management entity authenticated by PKI entity  --------

 10       Further messages of this PKI management operation
          can be exchanged with MAC-based protection by the
             PKI management entity using the established
                        shared secret key (ssk)

Note: Figure 4 describes the situation where KEM-based message protection may not require more than one message exchange. In this case, the transactionID MUST also be used by the PKI entity (Bob) to ensure domain separation between different PKI management operations.
Message Flow When the PKI Entity Does Not Know That the PKI Management Entity Uses a KEM Key Pair

Step#

PKI

entity

PKI

management

entity

(Bob)

(Alice)

1

format

request

with

protection

depending

on

available

key

material

2

request

3

format

unprotected

error

with

status

"rejection"

and

failInfo

"wrongIntegrity"

and

KEM

certificate

in

extraCerts

4

error

5

validate

KEM

certificate

6

proceed

as

shown

in

the

figure

before

Step# PKI entity                           PKI management entity
      (Bob)                                (Alice)
---------------------------------------------------------------------
  1   format request with
        protection depending
        on available key
        material
  2                     -->  request  -->
  3                                        format unprotected error
                                             with status "rejection"
                                             and failInfo
                                             "wrongIntegrity" and KEM
                                             certificate in
                                             extraCerts
  4                     <--   error   <--
  5   validate KEM certificate

  6              proceed as shown in the figure before

Compilable ASN.1 Definitions
This section contains the updated 2002 ASN.1 module from [RFC5912], which was updated in [RFC9480]. This module replaces the module in Section 9 of [RFC5912]. The module contains those changes to the normative ASN.1 module from Appendix F of [RFC4210] that were specified in [RFC9480], as well as changes made in this document. This module makes reference to ASN.1 structures defined in [RFC6268], as well as the UTF-8 encoding defined in [RFC3629].

PKIXCMP-2023
    { iso(1) identified-organization(3) dod(6) internet(1)
    security(5) mechanisms(5) pkix(7) id-mod(0)
    id-mod-cmp2023-02(116) }
DEFINITIONS EXPLICIT TAGS ::=
BEGIN
IMPORTS

AttributeSet{}, SingleAttribute{}, Extensions{}, EXTENSION, ATTRIBUTE
FROM PKIX-CommonTypes-2009
    {iso(1) identified-organization(3) dod(6) internet(1) security(5)
    mechanisms(5) pkix(7) id-mod(0) id-mod-pkixCommon-02(57)}

AlgorithmIdentifier{}, SIGNATURE-ALGORITHM, ALGORITHM,
    DIGEST-ALGORITHM, MAC-ALGORITHM, KEY-DERIVATION
FROM AlgorithmInformation-2009
    {iso(1) identified-organization(3) dod(6) internet(1) security(5)
    mechanisms(5) pkix(7) id-mod(0)
    id-mod-algorithmInformation-02(58)}

Certificate, CertificateList, Time, id-kp
FROM PKIX1Explicit-2009
    {iso(1) identified-organization(3) dod(6) internet(1) security(5)
    mechanisms(5) pkix(7) id-mod(0) id-mod-pkix1-explicit-02(51)}

DistributionPointName, GeneralNames, GeneralName, KeyIdentifier
FROM PKIX1Implicit-2009
    {iso(1) identified-organization(3) dod(6) internet(1) security(5)
    mechanisms(5) pkix(7) id-mod(0) id-mod-pkix1-implicit-02(59)}

CertTemplate, PKIPublicationInfo, EncryptedKey, CertId,
    CertReqMessages, Controls, RegControlSet, id-regCtrl
FROM PKIXCRMF-2009
    { iso(1) identified-organization(3) dod(6) internet(1)
    security(5) mechanisms(5) pkix(7) id-mod(0)
    id-mod-crmf2005-02(55) }
    -- The import of EncryptedKey is added due to the updates made
    -- in [RFC9480]. EncryptedValue does not need to be imported
    -- anymore and is therefore removed here.

CertificationRequest
FROM PKCS-10
    {iso(1) identified-organization(3) dod(6) internet(1) security(5)
    mechanisms(5) pkix(7) id-mod(0) id-mod-pkcs10-2009(69)}
-- (specified in [RFC2986] with 1993 ASN.1 syntax and IMPLICIT
-- tags).  Alternatively, implementers may directly include
-- the syntax of [RFC2986] in this module.

localKeyId
FROM PKCS-9
    {iso(1) member-body(2) us(840) rsadsi(113549) pkcs(1) pkcs-9(9)
    modules(0) pkcs-9(1)}
    -- The import of localKeyId is added due to the updates made in
    -- [RFC9480]

EnvelopedData, SignedData
FROM CryptographicMessageSyntax-2010
    {iso(1) member-body(2) us(840) rsadsi(113549) pkcs(1) pkcs-9(9)
    smime(16) modules(0) id-mod-cms-2009(58)}
    -- The import of EnvelopedData and SignedData from [RFC6268] is
    -- added due to the updates made in CMP Updates [RFC9480]

KEM-ALGORITHM
FROM KEMAlgorithmInformation-2023  -- [RFC9629]
    { iso(1) identified-organization(3) dod(6) internet(1)
    security(5) mechanisms(5) pkix(7) id-mod(0)
    id-mod-kemAlgorithmInformation-2023(109) }
    -- The import of KEM-ALGORITHM was added due to the updates made
    -- in [RFC9810]
;

-- History of the PKIXCMP ASN.1 modules
-- [RFC2510]
--    1988 Syntax, PKIXCMP, 1.3.6.1.5.5.7.0.9 (id-mod-cmp)
--    Obsoleted by RFC 4210 PKIXCMP, 1.3.6.1.5.5.7.0.16
--                                   (id-mod-cmp2000)
-- [RFC4210]
--    1988 Syntax, PKIXCMP, 1.3.6.1.5.5.7.0.16 (id-mod-cmp2000)
--    Replaced by RFC 9480 PKIXCMP, 1.3.6.1.5.5.7.0.99
--                                  (id-mod-cmp2021-88)
-- [RFC5912]
--    2002 Syntax, PKIXCMP-2009, 1.3.6.1.5.5.7.0.50
--                               (id-mod-cmp2000-02)
--    Replaced by RFC 9480 PKIXCMP-2021, 1.3.6.1.5.5.7.0.100
--                                       (id-mod-cmp2021-02)
-- [RFC9480]
--    1988 Syntax, PKIXCMP, 1.3.6.1.5.5.7.0.99 (id-mod-cmp2021-88)
--    2002 Syntax, PKIXCMP-2021, 1.3.6.1.5.5.7.0.100
--                               (id-mod-cmp2021-02)
--    Obsoleted by [RFC9810] PKIXCMP-2023, 1.3.6.1.5.5.7.0.116
--                                         (id-mod-cmp2023-02)
-- [RFC9810]
--    2002 Syntax, PKIXCMP-2023, 1.3.6.1.5.5.7.0.116
--                               (id-mod-cmp2023-02)

-- The rest of the module contains locally defined OIDs and
-- constructs:

CMPCertificate ::= CHOICE { x509v3PKCert Certificate, ... }
-- This syntax, while bits-on-the-wire compatible with the
-- standard X.509 definition of "Certificate", allows the
-- possibility of future certificate types (such as X.509
-- attribute certificates, card-verifiable certificates, or other
-- kinds of certificates) within this Certificate Management
-- Protocol, should a need ever arise to support such generality.
-- Those implementations that do not foresee a need to ever support
-- other certificate types MAY, if they wish, comment out the
-- above structure and "uncomment" the following one prior to
-- compiling this ASN.1 module.  (Note that interoperability
-- with implementations that don't do this will be unaffected by
-- this change.)

-- CMPCertificate ::= Certificate

PKIMessage ::= SEQUENCE {
    header           PKIHeader,
    body             PKIBody,
    protection   [0] PKIProtection OPTIONAL,
    extraCerts   [1] SEQUENCE SIZE (1..MAX) OF CMPCertificate
                  OPTIONAL }

PKIMessages ::= SEQUENCE SIZE (1..MAX) OF PKIMessage

PKIHeader ::= SEQUENCE {
    pvno                INTEGER     { cmp1999(1), cmp2000(2),
                                      cmp2021(3) },
    sender              GeneralName,
    -- identifies the sender
    recipient           GeneralName,
    -- identifies the intended recipient
    messageTime     [0] GeneralizedTime         OPTIONAL,
    -- time of production of this message (used when sender
    -- believes that the transport will be "suitable", i.e.,
    -- that the time will still be meaningful upon receipt)
    protectionAlg   [1] AlgorithmIdentifier{ALGORITHM, {...}}
                            OPTIONAL,
    -- algorithm used for calculation of protection bits
    senderKID       [2] KeyIdentifier           OPTIONAL,
    recipKID        [3] KeyIdentifier           OPTIONAL,
    -- to identify specific keys used for protection
    transactionID   [4] OCTET STRING            OPTIONAL,
    -- identifies the transaction, i.e., this will be the same in
    -- corresponding request, response, certConf, and pkiconf
    -- messages
    senderNonce     [5] OCTET STRING            OPTIONAL,
    recipNonce      [6] OCTET STRING            OPTIONAL,
    -- nonces used to provide replay protection, senderNonce
    -- is inserted by the creator of this message; recipNonce
    -- is a nonce previously inserted in a related message by
    -- the intended recipient of this message.
    freeText        [7] PKIFreeText             OPTIONAL,
    -- this may be used to indicate context-specific instructions
    -- (this field is intended for human consumption)
    generalInfo     [8] SEQUENCE SIZE (1..MAX) OF
                        InfoTypeAndValue     OPTIONAL
    -- this may be used to convey context-specific information
    -- (this field is not primarily intended for human consumption)
}

PKIFreeText ::= SEQUENCE SIZE (1..MAX) OF UTF8String
    -- text encoded as UTF-8 string [RFC3629]

PKIBody ::= CHOICE {       -- message-specific body elements
    ir       [0]  CertReqMessages,        --Initialization Request
    ip       [1]  CertRepMessage,         --Initialization Response
    cr       [2]  CertReqMessages,        --Certification Request
    cp       [3]  CertRepMessage,         --Certification Response
    p10cr    [4]  CertificationRequest,   --imported from [RFC2986]
    popdecc  [5]  POPODecKeyChallContent, --pop Challenge
    popdecr  [6]  POPODecKeyRespContent,  --pop Response
    kur      [7]  CertReqMessages,        --Key Update Request
    kup      [8]  CertRepMessage,         --Key Update Response
    krr      [9]  CertReqMessages,        --Key Recovery Request
    krp      [10] KeyRecRepContent,       --Key Recovery Response
    rr       [11] RevReqContent,          --Revocation Request
    rp       [12] RevRepContent,          --Revocation Response
    ccr      [13] CertReqMessages,        --Cross-Cert. Request
    ccp      [14] CertRepMessage,         --Cross-Cert. Response
    ckuann   [15] CAKeyUpdContent,        --CA Key Update Ann.
    cann     [16] CertAnnContent,         --Certificate Ann.
    rann     [17] RevAnnContent,          --Revocation Ann.
    crlann   [18] CRLAnnContent,          --CRL Announcement
    pkiconf  [19] PKIConfirmContent,      --Confirmation
    nested   [20] NestedMessageContent,   --Nested Message
    genm     [21] GenMsgContent,          --General Message
    genp     [22] GenRepContent,          --General Response
    error    [23] ErrorMsgContent,        --Error Message
    certConf [24] CertConfirmContent,     --Certificate Confirm
    pollReq  [25] PollReqContent,         --Polling Request
    pollRep  [26] PollRepContent          --Polling Response
}

PKIProtection ::= BIT STRING

ProtectedPart ::= SEQUENCE {
    header    PKIHeader,
    body      PKIBody }

id-PasswordBasedMac OBJECT IDENTIFIER ::= { iso(1) member-body(2)
    usa(840) nt(113533) nsn(7) algorithms(66) 13 }
PBMParameter ::= SEQUENCE {
    salt                OCTET STRING,
    -- Note:  Implementations MAY wish to limit acceptable sizes
    -- of this string to values appropriate for their environment
    -- in order to reduce the risk of denial-of-service attacks.
    owf                 AlgorithmIdentifier{DIGEST-ALGORITHM, {...}},
    -- AlgId for the OWF
    iterationCount      INTEGER,
    -- number of times the OWF is applied
    -- Note:  Implementations MAY wish to limit acceptable sizes
    -- of this integer to values appropriate for their environment
    -- in order to reduce the risk of denial-of-service attacks.
    mac                 AlgorithmIdentifier{MAC-ALGORITHM, {...}}
    -- AlgId of the MAC algorithm
}

id-DHBasedMac OBJECT IDENTIFIER ::= { iso(1) member-body(2)
    usa(840) nt(113533) nsn(7) algorithms(66) 30 }
DHBMParameter ::= SEQUENCE {
    owf                 AlgorithmIdentifier{DIGEST-ALGORITHM, {...}},
    -- AlgId for an OWF
    mac                 AlgorithmIdentifier{MAC-ALGORITHM, {...}}
    -- AlgId of the MAC algorithm
}

-- id-KemBasedMac and KemBMParameter were added in [RFC9810]

id-KemBasedMac OBJECT IDENTIFIER ::= { iso(1) member-body(2)
    usa(840) nt(113533) nsn(7) algorithms(66) 16 }
KemBMParameter ::= SEQUENCE {
    kdf              AlgorithmIdentifier{KEY-DERIVATION, {...}},
    -- AlgId of the Key Derivation Function algorithm
    kemContext   [0] OCTET STRING OPTIONAL,
    -- MAY contain additional algorithm-specific context information
    len              INTEGER (1..MAX),
    -- Defines the length of the keying material output of the KDF
    -- SHOULD be the maximum key length of the MAC function
    mac              AlgorithmIdentifier{MAC-ALGORITHM, {...}}
    -- AlgId of the MAC algorithm
}

PKIStatus ::= INTEGER {
    accepted               (0),
    -- you got exactly what you asked for
    grantedWithMods        (1),
    -- you got something like what you asked for; the
    -- requester is responsible for ascertaining the differences
    rejection              (2),
    -- you don't get it, more information elsewhere in the message
    waiting                (3),
    -- the request body part has not yet been processed; expect to
    -- hear more later (note: proper handling of this status
    -- response MAY use the polling req/rep PKIMessages specified
    -- in Section 5.3.22; alternatively, polling in the underlying
    -- transport layer MAY have some utility in this regard)
    revocationWarning      (4),
    -- this message contains a warning that a revocation is
    -- imminent
    revocationNotification (5),
    -- notification that a revocation has occurred
    keyUpdateWarning       (6)
    -- update already done for the oldCertId specified in
    -- CertReqMsg
}

PKIFailureInfo ::= BIT STRING {
-- since we can fail in more than one way!
-- More codes may be added in the future if/when required.
    badAlg              (0),
    -- unrecognized or unsupported algorithm identifier
    badMessageCheck     (1),
    -- integrity check failed (e.g., signature did not verify)
    badRequest          (2),
    -- transaction not permitted or supported
    badTime             (3),
    -- messageTime was not sufficiently close to the system time,
    -- as defined by local policy
    badCertId           (4),
    -- no certificate could be found matching the provided criteria
    badDataFormat       (5),
    -- the data submitted has the wrong format
    wrongAuthority      (6),
    -- the authority indicated in the request is different from the
    -- one creating the response token
    incorrectData       (7),
    -- the requester's data is incorrect (for notary services)
    missingTimeStamp    (8),
    -- when the timestamp is missing but should be there
    -- (by policy)
    badPOP              (9),
    -- the POP failed
    certRevoked         (10),
    -- the certificate has already been revoked
    certConfirmed       (11),
    -- the certificate has already been confirmed
    wrongIntegrity      (12),
    -- KEM ciphertext missing for MAC-based protection of response,
    -- or not valid integrity of message received (password based
    -- instead of signature or vice versa)
    badRecipientNonce   (13),
    -- not valid recipient nonce, either missing or wrong value
    timeNotAvailable    (14),
    -- the TSA's time source is not available
    unacceptedPolicy    (15),
    -- the requested TSA policy is not supported by the TSA
    unacceptedExtension (16),
    -- the requested extension is not supported by the TSA
    addInfoNotAvailable (17),
    -- the additional information requested could not be
    -- understood or is not available
    badSenderNonce      (18),
    -- not valid sender nonce, either missing or wrong size
    badCertTemplate     (19),
    -- not valid cert. template or missing mandatory information
    signerNotTrusted    (20),
    -- signer of the message unknown or not trusted
    transactionIdInUse  (21),
    -- the transaction identifier is already in use
    unsupportedVersion  (22),
    -- the version of the message is not supported
    notAuthorized       (23),
    -- the sender was not authorized to make the preceding
    -- request or perform the preceding action
    systemUnavail       (24),
    -- the request cannot be handled due to system unavailability
    systemFailure       (25),
    -- the request cannot be handled due to system failure
    duplicateCertReq    (26)
    -- certificate cannot be issued because a duplicate
    -- certificate already exists
}

PKIStatusInfo ::= SEQUENCE {
    status        PKIStatus,
    statusString  PKIFreeText     OPTIONAL,
    failInfo      PKIFailureInfo  OPTIONAL }

OOBCert ::= CMPCertificate

OOBCertHash ::= SEQUENCE {
    hashAlg     [0] AlgorithmIdentifier{DIGEST-ALGORITHM, {...}}
                        OPTIONAL,
    certId      [1] CertId                  OPTIONAL,
    hashVal         BIT STRING
    -- hashVal is calculated over the DER encoding of the
    -- self-signed certificate with the identifier certID.
}

POPODecKeyChallContent ::= SEQUENCE OF Challenge
-- One Challenge per encryption or key agreement key certification
-- request (in the same order as these requests appear in
-- CertReqMessages).

-- encryptedRand was added in [RFC9810]

Challenge ::= SEQUENCE {
   owf                 AlgorithmIdentifier{DIGEST-ALGORITHM, {...}}
                            OPTIONAL,
   -- MUST be present in the first Challenge; MAY be omitted in
   -- any subsequent Challenge in POPODecKeyChallContent (if
   -- omitted, then the owf used in the immediately preceding
   -- Challenge is to be used).
   witness             OCTET STRING,
   -- the result of applying the OWF to a
   -- randomly generated INTEGER, A. (Note that a different
   -- INTEGER MUST be used for each Challenge.)
   challenge           OCTET STRING,
   -- MUST be used for cmp2000(2) popdecc messages and MUST be
   -- the encryption of Rand (using a mechanism depending on the
   -- private key type).
   -- MUST be an empty OCTET STRING for cmp2021(3) popdecc messages.
   -- Note: Using challenge omitting the optional encryptedRand is
   -- bit-compatible to the syntax without adding this optional
   -- field.
   encryptedRand   [0] EnvelopedData OPTIONAL
   -- MUST be omitted for cmp2000(2) popdecc messages.
   -- MUST be used for cmp2021(3) popdecc messages and MUST contain
   -- the encrypted value of Rand using CMS EnvelopedData using the
   -- key management technique depending on the private key type as
   -- defined in Section 5.2.2.
}

-- Rand was added in [RFC9480]

Rand ::= SEQUENCE {
-- Rand is encrypted involving the public key to form the content of
-- challenge or encryptedRand in POPODecKeyChallContent
   int                  INTEGER,
   -- the randomly generated INTEGER A (above)
   sender               GeneralName
   -- the sender's name (as included in PKIHeader)
}

POPODecKeyRespContent ::= SEQUENCE OF INTEGER
-- One INTEGER per encryption or key agreement key certification
-- request (in the same order as these requests appear in
-- CertReqMessages). The retrieved INTEGER A (above) is returned to
-- the sender of the corresponding Challenge.

CertRepMessage ::= SEQUENCE {
    caPubs       [1] SEQUENCE SIZE (1..MAX) OF CMPCertificate
                  OPTIONAL,
    response         SEQUENCE OF CertResponse }

CertResponse ::= SEQUENCE {
    certReqId           INTEGER,
    -- to match this response with the corresponding request (a value
    -- of -1 is to be used if certReqId is not specified in the
    -- corresponding request, which can only be a p10cr)
    status              PKIStatusInfo,
    certifiedKeyPair    CertifiedKeyPair    OPTIONAL,
    rspInfo             OCTET STRING        OPTIONAL
    -- analogous to the id-regInfo-utf8Pairs string defined
    -- for regInfo in CertReqMsg [RFC4211]
}

CertifiedKeyPair ::= SEQUENCE {
    certOrEncCert       CertOrEncCert,
    privateKey      [0] EncryptedKey      OPTIONAL,
    -- See [RFC4211] for comments on encoding.
    -- Changed from EncryptedValue to EncryptedKey as a CHOICE of
    -- EncryptedValue and EnvelopedData due to the changes made in
    -- [RFC9480].
    -- Using the choice EncryptedValue is bit-compatible to the
    -- syntax without this change.
    publicationInfo [1] PKIPublicationInfo  OPTIONAL }

CertOrEncCert ::= CHOICE {
    certificate     [0] CMPCertificate,
    encryptedCert   [1] EncryptedKey
    -- Changed from Encrypted Value to EncryptedKey as a CHOICE of
    -- EncryptedValue and EnvelopedData due to the changes made in
    -- [RFC9480].
    -- Using the choice EncryptedValue is bit-compatible to the
    -- syntax without this change.
}

KeyRecRepContent ::= SEQUENCE {
    status                  PKIStatusInfo,
    newSigCert          [0] CMPCertificate OPTIONAL,
    caCerts             [1] SEQUENCE SIZE (1..MAX) OF
                                     CMPCertificate OPTIONAL,
    keyPairHist         [2] SEQUENCE SIZE (1..MAX) OF
                                     CertifiedKeyPair OPTIONAL }

RevReqContent ::= SEQUENCE OF RevDetails

RevDetails ::= SEQUENCE {
    certDetails         CertTemplate,
    -- allows requester to specify as much as they can about
    -- the cert. for which revocation is requested
    -- (e.g., for cases in which serialNumber is not available)
    crlEntryDetails     Extensions{{...}}    OPTIONAL
    -- requested crlEntryExtensions
}

RevRepContent ::= SEQUENCE {
    status       SEQUENCE SIZE (1..MAX) OF PKIStatusInfo,
    -- in same order as was sent in RevReqContent
    revCerts [0] SEQUENCE SIZE (1..MAX) OF CertId OPTIONAL,
    -- IDs for which revocation was requested
    -- (same order as status)
    crls     [1] SEQUENCE SIZE (1..MAX) OF CertificateList OPTIONAL
    -- the resulting CRLs (there may be more than one)
}

CAKeyUpdAnnContent ::= SEQUENCE {
    oldWithNew   CMPCertificate, -- old pub signed with new priv
    newWithOld   CMPCertificate, -- new pub signed with old priv
    newWithNew   CMPCertificate  -- new pub signed with new priv
}

-- CAKeyUpdContent was added in [RFC9810]
CAKeyUpdContent ::= CHOICE {
    cAKeyUpdAnnV2      CAKeyUpdAnnContent, -- deprecated
    cAKeyUpdAnnV3  [0] RootCaKeyUpdateContent
}
-- With cmp2021, the use of CAKeyUpdAnnContent is deprecated, use
-- RootCaKeyUpdateContent instead.

CertAnnContent ::= CMPCertificate

RevAnnContent ::= SEQUENCE {
    status              PKIStatus,
    certId              CertId,
    willBeRevokedAt     GeneralizedTime,
    badSinceDate        GeneralizedTime,
    crlDetails          Extensions{{...}}  OPTIONAL
    -- extra CRL details (e.g., crl number, reason, location, etc.)
}

CRLAnnContent ::= SEQUENCE OF CertificateList

PKIConfirmContent ::= NULL

NestedMessageContent ::= PKIMessages

-- CertReqTemplateContent, AttributeTypeAndValue,
-- ExpandedRegControlSet, id-regCtrl-altCertTemplate,
-- AltCertTemplate, regCtrl-algId, id-regCtrl-algId, AlgIdCtrl,
-- regCtrl-rsaKeyLen, id-regCtrl-rsaKeyLen, and RsaKeyLenCtrl
-- were added in [RFC9480]

CertReqTemplateContent ::= SEQUENCE {
   certTemplate           CertTemplate,
   -- prefilled certTemplate structure elements
   -- The SubjectPublicKeyInfo field in the certTemplate MUST NOT
   -- be used.
   keySpec                Controls OPTIONAL
   -- MAY be used to specify supported algorithms
   -- Controls  ::= SEQUENCE SIZE (1..MAX) OF AttributeTypeAndValue
   -- as specified in CRMF [RFC4211]
   }

AttributeTypeAndValue ::= SingleAttribute{{ ... }}

ExpandedRegControlSet ATTRIBUTE ::= { RegControlSet |
   regCtrl-altCertTemplate | regCtrl-algId | regCtrl-rsaKeyLen, ... }

regCtrl-altCertTemplate ATTRIBUTE ::=
   { TYPE AltCertTemplate IDENTIFIED BY id-regCtrl-altCertTemplate }

id-regCtrl-altCertTemplate OBJECT IDENTIFIER ::= { id-regCtrl 7 }

AltCertTemplate ::= AttributeTypeAndValue
   -- specifies a template for a certificate other than an X.509v3
   -- public key certificate

regCtrl-algId ATTRIBUTE ::=
   { TYPE AlgIdCtrl IDENTIFIED BY id-regCtrl-algId }

id-regCtrl-algId OBJECT IDENTIFIER ::= { id-regCtrl 11 }

AlgIdCtrl ::= AlgorithmIdentifier{ALGORITHM, {...}}
   -- SHALL be used to specify supported algorithms other than RSA

regCtrl-rsaKeyLen ATTRIBUTE ::=
   { TYPE RsaKeyLenCtrl IDENTIFIED BY id-regCtrl-rsaKeyLen }

id-regCtrl-rsaKeyLen OBJECT IDENTIFIER ::= { id-regCtrl 12 }

RsaKeyLenCtrl ::= INTEGER (1..MAX)
   -- SHALL be used to specify supported RSA key lengths

-- RootCaKeyUpdateContent, CRLSource, and CRLStatus were added in
-- [RFC9480]

RootCaKeyUpdateContent ::= SEQUENCE {
   newWithNew       CMPCertificate,
   -- new root CA certificate
   newWithOld   [0] CMPCertificate OPTIONAL,
   -- X.509 certificate containing the new public root CA key
   -- signed with the old private root CA key
   oldWithNew   [1] CMPCertificate OPTIONAL
   -- X.509 certificate containing the old public root CA key
   -- signed with the new private root CA key
   }

CRLSource ::= CHOICE {
   dpn          [0] DistributionPointName,
   issuer       [1] GeneralNames }

CRLStatus ::= SEQUENCE {
   source       CRLSource,
   thisUpdate   Time OPTIONAL }

-- KemCiphertextInfo and KemOtherInfo were added in [RFC9810]

KemCiphertextInfo ::= SEQUENCE {
   kem              AlgorithmIdentifier{KEM-ALGORITHM, {...}},
   -- AlgId of the KEM algorithm
   ct               OCTET STRING
   -- Ciphertext output from the Encapsulate function
   }

KemOtherInfo ::= SEQUENCE {
   staticString     PKIFreeText,
   -- MUST be "CMP-KEM"
   transactionID    OCTET STRING,
   -- MUST contain the values from the message previously received
   -- containing the ciphertext (ct) in KemCiphertextInfo
   kemContext   [0] OCTET STRING OPTIONAL
   -- MAY contain additional algorithm-specific context information
  }

INFO-TYPE-AND-VALUE ::= TYPE-IDENTIFIER

InfoTypeAndValue ::= SEQUENCE {
    infoType    INFO-TYPE-AND-VALUE.
                    &id({SupportedInfoSet}),
    infoValue   INFO-TYPE-AND-VALUE.
                    &Type({SupportedInfoSet}{@infoType}) }

SupportedInfoSet INFO-TYPE-AND-VALUE ::= { ... }

-- Example InfoTypeAndValue contents include, but are not limited
-- to, the following (uncomment in this ASN.1 module and use as
-- appropriate for a given environment):
--
--   id-it-caProtEncCert    OBJECT IDENTIFIER ::= {id-it 1}
--      CAProtEncCertValue      ::= CMPCertificate
--   id-it-signKeyPairTypes OBJECT IDENTIFIER ::= {id-it 2}
--      SignKeyPairTypesValue   ::= SEQUENCE SIZE (1..MAX) OF
--                                      AlgorithmIdentifier{{...}}
--   id-it-encKeyPairTypes  OBJECT IDENTIFIER ::= {id-it 3}
--      EncKeyPairTypesValue    ::= SEQUENCE SIZE (1..MAX) OF
--                                      AlgorithmIdentifier{{...}}
--   id-it-preferredSymmAlg OBJECT IDENTIFIER ::= {id-it 4}
--      PreferredSymmAlgValue   ::= AlgorithmIdentifier{{...}}
--   id-it-caKeyUpdateInfo  OBJECT IDENTIFIER ::= {id-it 5}
--      CAKeyUpdateInfoValue    ::= CAKeyUpdAnnContent
--      - id-it-caKeyUpdateInfo was deprecated with cmp2021
--   id-it-currentCRL       OBJECT IDENTIFIER ::= {id-it 6}
--      CurrentCRLValue         ::= CertificateList
--   id-it-unsupportedOIDs  OBJECT IDENTIFIER ::= {id-it 7}
--      UnsupportedOIDsValue    ::= SEQUENCE SIZE (1..MAX) OF
--                                          OBJECT IDENTIFIER
--   id-it-keyPairParamReq  OBJECT IDENTIFIER ::= {id-it 10}
--      KeyPairParamReqValue    ::= OBJECT IDENTIFIER
--   id-it-keyPairParamRep  OBJECT IDENTIFIER ::= {id-it 11}
--      KeyPairParamRepValue    ::= AlgorithmIdentifier{{...}}
--   id-it-revPassphrase    OBJECT IDENTIFIER ::= {id-it 12}
--      RevPassphraseValue      ::= EncryptedKey
--      - Changed from Encrypted Value to EncryptedKey as a CHOICE
--      - of EncryptedValue and EnvelopedData due to the changes
--      - made in [RFC9480]
--      - Using the choice EncryptedValue is bit-compatible to
--      - the syntax without this change
--   id-it-implicitConfirm  OBJECT IDENTIFIER ::= {id-it 13}
--      ImplicitConfirmValue    ::= NULL
--   id-it-confirmWaitTime  OBJECT IDENTIFIER ::= {id-it 14}
--      ConfirmWaitTimeValue    ::= GeneralizedTime
--   id-it-origPKIMessage   OBJECT IDENTIFIER ::= {id-it 15}
--      OrigPKIMessageValue     ::= PKIMessages
--   id-it-suppLangTags     OBJECT IDENTIFIER ::= {id-it 16}
--      SuppLangTagsValue       ::= SEQUENCE OF UTF8String
--   id-it-caCerts          OBJECT IDENTIFIER ::= {id-it 17}
--      CaCertsValue            ::= SEQUENCE SIZE (1..MAX) OF
--                                             CMPCertificate
--      - id-it-caCerts added in [RFC9480]
--   id-it-rootCaKeyUpdate  OBJECT IDENTIFIER ::= {id-it 18}
--      RootCaKeyUpdateValue    ::= RootCaKeyUpdateContent
--      - id-it-rootCaKeyUpdate added in [RFC9480]
--   id-it-certReqTemplate  OBJECT IDENTIFIER ::= {id-it 19}
--      CertReqTemplateValue    ::= CertReqTemplateContent
--      - id-it-certReqTemplate added in [RFC9480]
--   id-it-rootCaCert       OBJECT IDENTIFIER ::= {id-it 20}
--      RootCaCertValue         ::= CMPCertificate
--      - id-it-rootCaCert added in [RFC9480]
--   id-it-certProfile      OBJECT IDENTIFIER ::= {id-it 21}
--      CertProfileValue        ::= SEQUENCE SIZE (1..MAX) OF
--                                                 UTF8String
--      - id-it-certProfile added in [RFC9480]
--   id-it-crlStatusList    OBJECT IDENTIFIER ::= {id-it 22}
--      CRLStatusListValue      ::= SEQUENCE SIZE (1..MAX) OF
--                                                  CRLStatus
--      - id-it-crlStatusList added in [RFC9480]
--   id-it-crls             OBJECT IDENTIFIER ::= {id-it 23}
--      CRLsValue               ::= SEQUENCE SIZE (1..MAX) OF
--                                            CertificateList
--      - id-it-crls added in [RFC9480]
--   id-it-KemCiphertextInfo    OBJECT IDENTIFIER ::= {id-it 24}
--      KemCiphertextInfoValue  ::= KemCiphertextInfo
--      - id-it-KemCiphertextInfo was added in [RFC9810]
--
-- where
--
--   id-pkix OBJECT IDENTIFIER ::= {
--      iso(1) identified-organization(3)
--      dod(6) internet(1) security(5) mechanisms(5) pkix(7)}
-- and
--   id-it   OBJECT IDENTIFIER ::= {id-pkix 4}
--
--
-- This construct MAY also be used to define new PKIX Certificate
-- Management Protocol request and response messages or
-- general-purpose (e.g., announcement) messages for future needs
-- or for specific environments.

GenMsgContent ::= SEQUENCE OF InfoTypeAndValue

-- May be sent by end entity, RA, or CA (depending on message
-- content).  The OPTIONAL infoValue parameter of InfoTypeAndValue
-- will typically be omitted for some of the examples given above.
-- The receiver is free to ignore any contained OIDs that it
-- does not recognize.  If sent from end entity to CA, the empty set
-- indicates that the CA may send
-- any/all information that it wishes.

GenRepContent ::= SEQUENCE OF InfoTypeAndValue
-- The receiver MAY ignore any contained OIDs that it does not
-- recognize.

ErrorMsgContent ::= SEQUENCE {
    pKIStatusInfo          PKIStatusInfo,
    errorCode              INTEGER           OPTIONAL,
    -- implementation-specific error codes
    errorDetails           PKIFreeText       OPTIONAL
    -- implementation-specific error details
}

CertConfirmContent ::= SEQUENCE OF CertStatus

CertStatus ::= SEQUENCE {
    certHash    OCTET STRING,
    -- the hash of the certificate, using the same hash algorithm
    -- as is used to create and verify the certificate signature
    certReqId   INTEGER,
    -- to match this confirmation with the corresponding req/rep
    statusInfo  PKIStatusInfo OPTIONAL,
    hashAlg [0] AlgorithmIdentifier{DIGEST-ALGORITHM, {...}} OPTIONAL
    -- the hash algorithm to use for calculating certHash
    -- SHOULD NOT be used in all cases where the AlgorithmIdentifier
    -- of the certificate signature specifies a hash algorithm
   }

PollReqContent ::= SEQUENCE OF SEQUENCE {
    certReqId              INTEGER }

PollRepContent ::= SEQUENCE OF SEQUENCE {
    certReqId              INTEGER,
    checkAfter             INTEGER,  -- time in seconds
    reason                 PKIFreeText OPTIONAL }

--
-- EKU extension for PKI entities used in CMP
-- operations, added due to the changes made in [RFC9480]
-- The EKUs for the CA and RA are reused from CMC, as defined in
-- [RFC6402]
--

-- id-kp-cmcCA OBJECT IDENTIFIER ::= { id-kp 27 }
-- id-kp-cmcRA OBJECT IDENTIFIER ::= { id-kp 28 }
id-kp-cmKGA OBJECT IDENTIFIER ::= { id-kp 32 }

END

Acknowledgements
The authors of this document wish to thank Carlisle Adams, Stephen Farrell, Tomi Kause, and Tero Mononen, the original authors of [RFC4210], for their work.
We also thank all reviewers of this document for their valuable feedback.
Adding KEM support to this document was partly funded by the German Federal Ministry of Education and Research in the project Quoryptan through grant number 16KIS2033.